Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CINT2000 Result

Copyright ©1999-2005, Standard Performance Evaluation Corporation

Sun Microsystems Ultra Enterprise 2

SPECint2000 = SPECint_base2000 = -- 116 SPEC license #: 6 Tested by: Sun Microsystems Test date: Jun-2006 Hardware Avail: Apr-1997 Software Avail: Mar-2005

Benchmark

Reference

Time

Base Runtime

Base Ratio Runtime Ratio 30 60 90 120 150

164.gzip 1400 1325 106

175.vpr 1400 1248 112

176.gcc 1100 954 115

181.mcf 1800 1492 121

186.crafty 1000 994 101

197.parser 1800 1604 112

252.eon 1300 1105 118

253.perlbmk 1800 1444 125

254.gap 1100 1041 106

255.vortex 1900 1410 135

256.bzip2 1500 1346 111

300.twolf 3000 2096 143

Hardware

CPU: UltraSPARC II CPU MHz: 296 FPU: Integrated CPU(s) enabled: 2 cores, 2 chips, 1 core/chip CPU(s) orderable: 1,2 Parallel: No Primary Cache: 16KBI+16KBD on chip Secondary Cache: 2MB(I+D) off chip L3 Cache: none Other Cache: None Memory: 2GB Disk Subsystem: 2x36GB 10K RPM SCSI (1 sys disk, 1 for SPEC) Other Hardware: none

Software

Operating System: Solaris 10 3/05 Compiler: Sun Forte Developer 6 File System: ufs System State: Default

Notes/Tuning Information

 This is a "historical" submission: the system tested
 here is not currently sold, but is reported for
 historical reference.

 Although two CPUs were enabled during testing,
 the SPEC CPU2000 benchmarks used only 1 CPU.

 Tuning:  C    flags: -fast
          C++  flags: -fast

Portability:
     176.gcc: -Dalloca=__builtin_alloca -DHOST_WORDS_BIG_ENDIAN
     186.crafty: -DSUN
     253.perlbmk: -DSPEC_CPU2000_SOLARIS
     254.gap:  -DSYS_IS_USG -DSYS_HAS_TIME_PROTO -DSYS_HAS_SIGNAL_PROTO -DSYS_HAS_CALLOC_PROTO