Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2005, Standard Performance Evaluation Corporation

Sun Microsystems Ultra Enterprise 2

SPECfp2000 = SPECfp_base2000 = -- 147 SPEC license #: 6 Tested by: Sun Microsystems Test date: Jun-2006 Hardware Avail: Apr-1997 Software Avail: Mar-2005

Benchmark

Reference

Time

Base Runtime

Base Ratio Runtime Ratio 100 200 300 400 500

168.wupwise 1600 1361 118

171.swim 3100 1563 198

172.mgrid 1800 1238 145

173.applu 2100 1773 118

177.mesa 1400 1200 117

178.galgel 2900 958 303

179.art 2600 1292 201

183.equake 1300 1298 100

187.facerec 1900 983 193

188.ammp 2200 1704 129

189.lucas 2000 1346 149

191.fma3d 2100 1614 130

200.sixtrack 1100 967 114

301.apsi 2600 1851 140

Hardware

CPU: UltraSPARC II CPU MHz: 296 FPU: Integrated CPU(s) enabled: 2 cores, 2 chips, 1 core/chip CPU(s) orderable: 1,2 Parallel: No Primary Cache: 16KBI+16KBD on chip Secondary Cache: 2MB(I+D) off chip L3 Cache: none Other Cache: None Memory: 2GB Disk Subsystem: 2x36GB 10K RPM SCSI (1 sys disk, 1 for SPEC) Other Hardware: none

Software

Operating System: Solaris 10 3/05 Compiler: Sun Forte Developer 6 File System: ufs System State: Default

Notes/Tuning Information

 This is a "historical" submission: the system tested
 here is not currently sold, but is reported for
 historical reference.

 Although two CPUs were enabled during testing,
 the SPEC CPU2000 benchmarks used only 1 CPU.

 Tuning:  C    flags: -fast
          F90  flags: -fast

  Portability:
    178.galgel: -fixed