Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2005, Standard Performance Evaluation Corporation

SGI_{SGI Altix 4700 Bandwidth System (Itanium2 Processor 9050 1.6GHz/24M)} SPECfp_rate2000 =

SPECfp_rate_base2000 = -- 486 SPEC license #: 4 Tested by: SGI Test date: Jul-2006 Hardware Avail: Jul-2006 Software Avail: Jun-2006

Benchmark

Base Copies

Base Runtime

Base Ratio Copies Runtime Ratio

1000

2000

3000

4000

168.wupwise 16 68.8 432

171.swim 16 104 551

172.mgrid 16 87.8 381

173.applu 16 52.0 749

177.mesa 16 98.1 265

178.galgel 16 38.7 1390

179.art 16 13.3 3625

183.equake 16 40.8 591

187.facerec 16 77.5 455

188.ammp 16 126 325

189.lucas 16 114 325

191.fma3d 16 136 286

200.sixtrack 16 74.5 274

301.apsi 16 238 203

Hardware

CPU: Intel Itanium 2 CPU MHz: 1600 FPU: Integrated CPU(s) enabled: 16 cores, 8 chips, 2 cores/chip (Hyper-Threading Technology disabled) CPU(s) orderable: 1-512 chips Parallel: No Primary Cache: 16 KB (I) + 16 KB (D) on chip, per core Secondary Cache: 1 MB (I) + 256 KB (D) on chip, per core L3 Cache: 12 MB (I+D) on chip, per core Other Cache: N/A Memory: 64 GB (8*1GB DDR2-400 DIMMS per 2 core module) Disk Subsystem: 1 x 137 GB SCSI Other Hardware: None

Software

Operating System: SGI ProPack(TM) v4.0 Service Pack 3 Compiler: Intel(R) Fortran Compiler for Linux 9.1 (Build 20060523)

Intel(R) C++ Compiler for Linux 9.1 (Build 20060523)

File System: xfs System State: Multi-user

Notes/Tuning Information

 Baseline optimization flags:
   C programs:       -fast -ansi_alias -IPF_fp_relaxed +FDO
   Fortran programs: -fast -IPF_fp_relaxed +FDO

 Portability Flags:
   178.galgel:  -FI

 Processes were bound to CPUs using dplace.