Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2005, Standard Performance Evaluation Corporation

Fujitsu Siemens Computers

PRIMERGY TX300 S3, Intel Xeon 5110 processor, 1.60 GHz

SPECfp_rate2000 = SPECfp_rate_base2000 =

31.5 31.5

SPEC license #: 22 Tested by: Fujitsu Siemens Computers Test date: Jul-2006 Hardware Avail: Jul-2006 Software Avail: Jan-2006

Benchmark

Base Copies

Base Runtime

Base Ratio Copies Runtime Ratio 10 20 30 40 50 60 70 80 90 168.wupwise 2 78.7 47.2 2 78.7 47.2

171.swim 2 263 27.3 2 263 27.3

172.mgrid 2 184 22.6 2 184 22.6

173.applu 2 198 24.6 2 198 24.6

177.mesa 2 84.4 38.5 2 84.4 38.5

178.galgel 2 92.9 72.4 2 92.9 72.4

179.art 2 68.9 87.5 2 68.9 87.5

183.equake 2 109 27.8 2 109 27.8

187.facerec 2 119 37.1 2 119 37.1

188.ammp 2 198 25.7 2 198 25.7

189.lucas 2 186 24.9 2 186 24.9

191.fma3d 2 198 24.7 2 198 24.7

200.sixtrack 2 182 14.0 2 182 14.0

301.apsi 2 257 23.5 2 257 23.5

Hardware

CPU: Intel Xeon 5110 processor (1.60 GHz, 4MB SLC, 1066 MHz system bus) CPU MHz: 1600 FPU: Integrated CPU(s) enabled: 2 cores, 1 chip, 2 cores/chip CPU(s) orderable: 1,2 Parallel: No Primary Cache: 32KB(I) + 32KB(D) on chip, per core Secondary Cache: 4096KB(I+D) on chip, per chip L3 Cache: N/A Other Cache: N/A Memory: 8x1024 MB DDRII-RAM PC2-4200F (CAS 4-4-4) Disk Subsystem: Seagate ST336754SS (SAS, 15.4krpm, 36GB) Other Hardware: none

Software

Operating System: 64-Bit SUSE LINUX Enterprise Server 9 with SP3

Kernel 2.6.5-7.244-smp on an x86_64

Compiler: Intel C++ and Fortran Compiler 9.0 for EM64T

Build 20060120 (for 64-bit applications)

File System: ext2 System State: Multi-user run level 3

Notes/Tuning Information

 GENERAL
 +FDO implies feedback-directed optimization
 PASS1: -prof_gen  PASS2: -prof_use

 Optimization flags
 ONESTEP=yes set for all benchmarks

 Portability flags
 -DSPEC_CPU2000_LP64 applied to all benchmarks
 178.galgel: -FI for fixed-format Fortran

 Base tuning flags
    for Fortran and C programs: -fast +FDO

 Peak tuning flags
    same as baseline (basepeak=true set globally)

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2005, Standard Performance Evaluation Corporation

Fujitsu Siemens Computers

PRIMERGY TX300 S3, Intel Xeon 5110 processor, 1.60 GHz

SPECfp_rate2000 = SPECfp_rate_base2000 =

31.5 31.5

SPEC license #: 22 Tested by: Fujitsu Siemens Computers Test date: Jul-2006 Hardware Avail: Jul-2006 Software Avail: Jan-2006

Notes/Tuning Information (Continued)

 The system bus runs at 1066 MHz

 This result was measured with 64-bit binaries using the 64-bit version of
 the operating system.

 For information about Fujitsu Siemens Computers in your country please see:
 http://www.fujitsu-siemens.com/countries