Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CINT2000 Result

Copyright ©1999-2005, Standard Performance Evaluation Corporation

Advanced Micro Devices

Tyan Thunder K9QE (S4985) AMD Opteron (TM) 2220SE

SPECint_rate2000 = SPECint_rate_base2000 =

22.4 19.7

SPEC license #: 49 Tested by: AMD Austin, TX Test date: Jul-2006 Hardware Avail: Sep-2006 Software Avail: Sep-2005

Benchmark

Base Copies

Base Runtime

Base Ratio Copies Runtime Ratio 5 10 15 20 25 30 35 164.gzip 1 103 15.8 1 90.1 18.0

175.vpr 1 116 14.0 1 92.8 17.5

176.gcc 1 76.8 16.6 1 53.3 23.9

181.mcf 1 152 13.7 1 121 17.3

186.crafty 1 52.7 22.0 1 50.3 23.1

197.parser 1 104 20.1 1 104 20.0

252.eon 1 50.2 30.0 1 44.9 33.6

253.perlbmk 1 87.2 23.9 1 85.4 24.5

254.gap 1 58.6 21.8 1 58.6 21.8

255.vortex 1 73.6 29.9 1 68.9 32.0

256.bzip2 1 102 17.0 1 99.8 17.4

300.twolf 1 176 19.7 1 134 26.0

Hardware

CPU: AMD Opteron (TM) 2220SE CPU MHz: 2800 FPU: Integrated CPU(s) enabled: 2 cores, 1 chip, 2 cores/chip CPU(s) orderable: 1,2,4 Parallel: no Primary Cache: 64KBI + 64KBD on chip per core Secondary Cache: 1024KB (I+D) on chip per core L3 Cache: N/A Other Cache: N/A Memory: 4x512MB, DDR2-667 CL4 ECC Reg Disk Subsystem: SATA, 74Gb Other Hardware: None

Software

Operating System: Windows Server 2003 SP1 (32-bit) Compiler: Intel C++ 9.0 build 20050912Z for IA32

Microsoft Visual Studio .NET 7.0.9466 (libraries) MicroQuill Smartheap Library 7.0

File System: NTFS System State: default

Notes/Tuning Information

  shlW32M.lib is the SmartHeap library V7.0 from MicroQuill (www.microquill.com)
  +FDO: PASS1=-Qprof_gen  PASS2=-Qprof_use
  Portability:
    176.gcc:      -Dalloca=_alloca /F10000000
    186.crafty:   -DNT_i386
    253.perlbmk:  -DSPEC_CPU2000_NTOS -DPERLDLL /MT
    254.gap:      -DSYS_HAS_CALLOC_PROTO -DSYS_HAS_MALLOC_PROTO
  Baseline C:   -O3 -Qipo -Op +FDO
  Baseline C++: -O3 -Qipo -Qcxx-features +FDO
 Peak Tuning:
  164.gzip:     -O3 -Qipo -QxW +FDO
  175.vpr:      -O3 -Qipo -QxW +FDO
                -Qoption,c,-ip_ninl_max_stats=2000,-ip_ninl_max_total_stats=4500
  176.gcc:      -O3 -Qipo -QxW -Oi- -Qunroll3 +FDO
  181.mcf:      -O3 -Qipo -QaxN      +FDO
  186.crafty:   -O3 -Qipo -QxW +FDO
  197.parser:   -QxW +FDO -Oi- -Qipo
  252.eon:      -O3 -Qipo -QxW +FDO -Qansi_alias
                -Qoption,c,-ip_ninl_max_stats=2000,-ip_ninl_max_total_stats=4500
  253.perlbmk:  -O3 -Qipo -QxW +FDO

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CINT2000 Result

Copyright ©1999-2005, Standard Performance Evaluation Corporation

Advanced Micro Devices

Tyan Thunder K9QE (S4985) AMD Opteron (TM) 2220SE

SPECint_rate2000 = SPECint_rate_base2000 =

22.4 19.7

SPEC license #: 49 Tested by: AMD Austin, TX Test date: Jul-2006 Hardware Avail: Sep-2006 Software Avail: Sep-2005

Notes/Tuning Information (Continued)

  254.gap:       basepeak = yes
  255.vortex:   -O3 -Qipo -arch:SSE  +FDO -Oi- shlW32M.lib
                -Qoption,c,-ip_ninl_max_stats=2000,-ip_ninl_max_total_stats=4500
  256.bzip2:    -O3 -Qipo              -Qunroll2
  300.twolf:    -O3 -Qipo -QxW +FDO    -Qunroll3 shlW32M.lib -Qansi_alias
 All memory slots populated on all CPU(s)
 The system can be built using a Zippy 700W EPS12V power supply and any SSI-MEB case.
 BIOS Changes: Enable Basic ECC