Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2005, Standard Performance Evaluation Corporation

Intel(R) Corporation

Intel(R) DG965WH motherboard( 3.73 GHz, Intel(R) Pentium(R) Extreme processor 965)

SPECfp2000 = SPECfp_base2000 =

2283 2280

SPEC license #: 13 Tested by: Intel Corporation Test date: Jul-2006 Hardware Avail: Jul-2006 Software Avail: May-2006

Benchmark

Reference

Time

Base Runtime

Base Ratio Runtime Ratio 2000 4000 6000 8000

168.wupwise 1600 36.5 4380 36.5 4380

171.swim 3100 93.0 3332 93.1 3329

172.mgrid 1800 105 1714 105 1716

173.applu 2100 103 2035 103 2035

177.mesa 1400 86.7 1615 86.7 1615

178.galgel 2900 72.6 3992 72.7 3990

179.art 2600 46.3 5616 46.3 5616

183.equake 1300 38.2 3403 37.1 3503

187.facerec 1900 82.1 2314 82.3 2310

188.ammp 2200 163 1354 162 1360

189.lucas 2000 78.6 2544 78.7 2543

191.fma3d 2100 114 1839 114 1839

200.sixtrack 1100 150 735 151 729

301.apsi 2600 172 1515 172 1514

Hardware

CPU: Intel(R) Pentium(R) Extreme processor 965( 3.73 GHz, 1066 MHz bus) CPU MHz: 3733 FPU: Integrated CPU(s) enabled: 2 cores, 1 chip, 2 cores/chip (Hyper-Threading Technology enabled) CPU(s) orderable: 1 Parallel: No Primary Cache: 12k micro-opsI + 16KBD per core, on chip Secondary Cache: 2MB(I+D) per core, on chip L3 Cache: None Other Cache: None Memory: 2 GB (2 1GB Corsair TWIN2X2048-8500C5 DDR2 1066 CL5-5-5 DIMMs) Disk Subsystem: Maxtor DiamondMax 10 6B300S0 300GB NCQ Serial ATA (7200 RPM, 16MB cache) Other Hardware: ATI Radeon X1900 XTX PCI express graphics card

Software

Operating System: Windows XP Professional SP2 Compiler: Intel C++ and Fortran Compiler 9.1 for 32-bit applications

Build 20060323Z Package ID: W_FC_P_9.1.020 Microsoft Visual Studio 2005(for libraries) SmartHeap Library Version 8.0 from http://www.microquill.com/

File System: NTFS System State: Default

Notes/Tuning Information

 +FDO: PASS1=  -Qprof_gen  PASS2=-Qprof_use
 Base tuning for Fortran programs:  -fast -Qansi_alias +FDO
 Base tuning for C programs:  -fast    +FDO shlW32M-80.lib
 Portability:
 178.galgel:   -FI /F32000000
 Peak tuning:
 168.wupwise:  -fast -Qansi_alias +FDO
 171.swim:     -fast -Qansi_alias +FDO
 172.mgrid:    -fast -Qansi_alias +FDO
 173.applu:  basepeak=yes
 177.mesa:   basepeak=yes
 178.galgel:   -fast -Qansi_alias +FDO
 179.art:      basepeak=yes
 183.equake:   -QxP -Oa -Qrcd -Qipo  +FDO  shlW32M-80.lib
 187.facerec:  -fast -Qunroll1 -Qscalar_rep- +FDO
 188.ammp:     -fast -Oa +FDO  shlW32M-80.lib
 189.lucas:    -fast -Qprefetch- +FDO

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2005, Standard Performance Evaluation Corporation

Intel(R) Corporation

Intel(R) DG965WH motherboard( 3.73 GHz, Intel(R) Pentium(R) Extreme processor 965)

SPECfp2000 = SPECfp_base2000 =

2283 2280

SPEC license #: 13 Tested by: Intel Corporation Test date: Jul-2006 Hardware Avail: Jul-2006 Software Avail: May-2006

Notes/Tuning Information (Continued)

 191.fma3d:    basepeak=yes
 200.sixtrack: -Qipo -QxP +FDO
 301.apsi:     -fast +FDO
 Tested systems can be used with Shin-G ATX case, Antec NeoPower 480W power supply
 Product description located as of 07/2006
 http://www.intel.com/products/motherboard/dg965wh/index.htm
 The system bus runs at 1066 MHz