Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2005, Standard Performance Evaluation Corporation

ASUS Computer International

Asus M2N32-SLI Deluxe, AMD Athlon (TM) 64 5000+

SPECfp_rate2000 = SPECfp_rate_base2000 =

35.2 32.0

SPEC license #: 13 Tested by: Intel Corporation Test date: Jul-2006 Hardware Avail: Jun-2006 Software Avail: Jun-2006

Benchmark

Base Copies

Base Runtime

Base Ratio Copies Runtime Ratio 10 20 30 40 50 60 70 168.wupwise 2 60.3 61.6 2 60.7 61.1

171.swim 2 231 31.1 2 176 40.9

172.mgrid 2 149 28.0 2 149 28.1

173.applu 2 163 30.0 2 147 33.0

177.mesa 2 151 21.6 2 73.7 44.1

178.galgel 2 140 48.2 2 136 49.4

179.art 2 120 50.5 2 120 50.5

183.equake 2 93.1 32.4 2 91.3 33.0

187.facerec 2 108 40.9 2 108 40.8

188.ammp 2 244 20.9 2 212 24.1

189.lucas 2 137 34.0 2 131 35.5

191.fma3d 2 148 33.0 2 146 33.4

200.sixtrack 2 139 18.4 2 139 18.4

301.apsi 2 244 24.7 2 244 24.7

Hardware

CPU: AMD Athlon (TM) 64 5000+ CPU MHz: 2600 FPU: Integrated CPU(s) enabled: 2 cores, 1 chip, 2 cores/chip CPU(s) orderable: 1 Parallel: no Primary Cache: 64KBI + 64KBD on chip, per core Secondary Cache: 512KB (I+D) on chip, per core L3 Cache: N/A Other Cache: N/A Memory: 2x1 GB, Corsair CM2X1024-8500C5 DDR2-1066 (manually set to DDR2-800 5-5-5-15 in the bios) Disk Subsystem: SATA, Western Digital WD740GD, 10000 rpm Other Hardware: None

Software

Operating System: Microsoft Windows XP SP2 Compiler: Intel C++ 9.1 build 20060519Z for IA32,

Intel Fortran 9.1 build 20060519Z for IA32, PGI Fortran compiler 6.0-5 for Windows XP, PGI C compiler 6.0-5 for Windows XP, ACML Version 2.5.3 (bundled with PGI 6.0-5)

File System: NTFS System State: default

Notes/Tuning Information

  +FDO:
   icl, ifort  : PASS1=-Qprof_gen  PASS2=-Qprof_use
   pgf90       : PASS1=-Mpfi       PASS2=-Mpfo
  ifort is the Intel Fortran compiler, icl is the Intel C++ compiler and
  pgf90 is the PGI Fortran 90 compiler.
  pgcc is the PGI C compiler.
  ONESTEP is set to 1 for every compile with the PGI compilers.
  Portability:
  178.galgel:                 -Mfixed
  Baseline: C      :  pgcc    -fastsse -Mipa=fast,inline
  Baseline: Fortran:  pgf90   -fastsse -Mipa=fast,inline +FDO
  Peak tuning:
  168.wupwise:        pgf90   -fastsse -Mipa=fast,inline -Mnovect
  171.swim:           ifort   -Qipo  -O3  -QaxN -QxW -Qunroll0 +FDO
  172.mgrid:          pgf90   -fastsse -Mipa=fast,inline
  173.applu:          ifort   -Qipo  -O3 -QaxN -QxW -auto +FDO
  177.mesa:           icl     -Qipo -arch:SSE2 -Qunroll1 -Qansi_alias +FDO

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2005, Standard Performance Evaluation Corporation

ASUS Computer International

Asus M2N32-SLI Deluxe, AMD Athlon (TM) 64 5000+

SPECfp_rate2000 = SPECfp_rate_base2000 =

35.2 32.0

SPEC license #: 13 Tested by: Intel Corporation Test date: Jul-2006 Hardware Avail: Jun-2006 Software Avail: Jun-2006

Notes/Tuning Information (Continued)

                              -Qoption,f,-ip_ninl_max_stats=1500,-ip_ninl_max_total_stats=4500
  178.galgel:         pgf90   -fastsse -Mipa=fast,safe -Munix -lacml
                              RM_SOURCES=lapak.f90
  179.art:            pgcc     basepeak=yes
  183.equake:         icl     -fast -arch:SSE2 -QaxW +FDO
  187.facerec:        pgf90   -fastsse -Mipa=fast,inline +FDO
  188.ammp:           icl     -Oa   -arch:SSE2  -Zp4 -Qansi_alias
  189.lucas:          ifort   -Qipo -QxW -Qunroll1
  191.fma3d:          pgf90   -Mipa=fast,inline -fastsse -Mnovect +FDO
  200.sixtrack:       pgf90   -fastsse -Mipa=fast,inline
  301.apsi:           pgf90   -fastsse -Mipa=fast,inline
 The SUT was built with a discrete PCIe graphics card (ATI Radeon X850 XT)
 and an ATX 550W power supply. The 2 DIMMs were configured in dual-channel mode.