Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CINT2000 Result

Copyright ©1999-2005, Standard Performance Evaluation Corporation

Itautec

Servidor Itautec MX221 (Intel Xeon 5030 processor, 2.66GHz)

SPECint_rate2000 = SPECint_rate_base2000 =

33.0 33.0

SPEC license #: 9001 Tested by: Itautec Test date: Nov-2006 Hardware Avail: Jul-2006 Software Avail: Mar-2006

Benchmark

Base Copies

Base Runtime

Base Ratio Copies Runtime Ratio 10 20 30 40 50 60 164.gzip 4 240 27.1 4 240 27.1

175.vpr 4 300 21.7 4 300 21.7

176.gcc 4 117 43.7 4 117 43.7

181.mcf 4 309 27.0 4 309 27.0

186.crafty 4 197 23.5 4 197 23.5

197.parser 4 265 31.5 4 265 31.5

252.eon 4 134 45.0 4 134 45.0

253.perlbmk 4 253 33.0 4 253 33.0

254.gap 4 137 37.2 4 137 37.2

255.vortex 4 165 53.5 4 165 53.5

256.bzip2 4 245 28.4 4 245 28.4

300.twolf 4 359 38.8 4 359 38.8

Hardware

CPU: Intel Xeon 5030 processor (2.66 GHz, 2x2MB L2, 1066 MHz system bus) CPU MHz: 2660 FPU: Integrated CPU(s) enabled: 2 cores, 1 chip, 2 cores/chip (Hyper-Threading Technology enabled) CPU(s) orderable: 1 Parallel: No Primary Cache: 32 KB I + 32 KB D on chip per core Secondary Cache: 2MB (I+D) on chip, per core L3 Cache: N/A Other Cache: N/A Memory: 8GB (8x1GB DDR2-RAM PC2-4200 FB-DIMM CL4 ECC) Disk Subsystem: 1 x 73GB SCSI U320 10000 RPM Other Hardware: None

Software

Operating System: Windows Server 2003 Enterprise Edition + SP1 (32-bit) Compiler: Intel C++ Compiler 9.1

Build 20060323Z (for 32-bit applications), Microsoft Visual Studio .NET 7.0.9466 (for libraries), MicroQuill SmartHeap for SMP Library v.8.0

File System: NTFS System State: Default

Notes/Tuning Information

 PORTABILITY FLAGS
    176.gcc:     -Dalloca=_alloca /F10000000
    186.crafty:  -DNT_i386
    253.perlbmk: -DSPEC_CPU2000_NTOS -DPERLDLL /MT
    254.gap:     -DSYS_HAS_CALLOC_PROTO -DSYS_HAS_MALLOC_PROTO
 GENERAL

 Base tuning flags
    for C programs:   -fast -QxP +FDO shlsmpmt.lib
    for C++ programs: -fast -Qcxx_features +FDO
 EXTRA LIBRARIES
   MicroQuill SmartHeap for SMP Library v.8.0
   http://www.microquill.com

   BIOS settings default.
   The system bus runs at 1066 MHz

   This result was measured with 32-bit binaries using the 32-bit version of the operating system.