Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2005, Standard Performance Evaluation Corporation

Apple Computer, Inc.

Xserve (3000 MHz Intel Dual-Core Xeon, 1333 MHz Bus)

SPECfp_rate2000 = SPECfp_rate_base2000 = -- 76.2

SPEC license #: 77 Tested by: Apple Computer, Inc. Test date: Nov-2006 Hardware Avail: Nov-2006 Software Avail: Nov-2006

Benchmark

Base Copies

Base Runtime

Base Ratio Copies Runtime Ratio 50 100 150 200 250 168.wupwise 4 68.5 108

171.swim 4 266 54.2

172.mgrid 4 173 48.2

173.applu 4 184 52.9

177.mesa 4 47.8 136

178.galgel 4 59.0 228

179.art 4 68.5 176

183.equake 4 113 53.5

187.facerec 4 89.4 98.6

188.ammp 4 207 49.3

189.lucas 4 179 51.7

191.fma3d 4 158 61.6

200.sixtrack 4 96.9 52.7

301.apsi 4 194 62.3

Hardware

CPU: Intel Dual-Core Xeon 5160 CPU MHz: 3000 FPU: Integrated CPU(s) enabled: 4 cores, 2 chips, 2 cores/chip CPU(s) orderable: 2 Parallel: No Primary Cache: 32 KB I + 32 KB D on chip per core Secondary Cache: 4 MB I+D on chip per chip (shared) L3 Cache: N/A Other Cache: N/A Memory: 4 GB (4x1GB FB-DIMM DDR2 667 MHz) Disk Subsystem: 80 GB SATA Other Hardware:

Software

Operating System: Mac OS X 10.4.8 (8L2127) Compiler: Intel C++ Compiler for Mac OS X Version 9.1, Build 20060928 (032) Intel Fortran Compiler for Mac OS X Version 9.1, Build 20060928 (032) File System: Journaled HFS+ System State: Default

Notes/Tuning Information

 +FDO: PASS1=-prof_gen  PASS2=-prof_use

 Base tuning for Fortran programs: -fast +FDO -lstmalloc
 Base tuning for C programs:       -fast +FDO -lstmalloc
 Portability flags:
   178.galgel:  -FI

 Boot ROM Version: XS11.0076.B00
 SMC Version: 1.11f4

 Memory Details:
   BRANCH 0 CHANNEL 0/DIMM 1: 1 GB DDR2 FB-DIMM 667 MHz
   BRANCH 0 CHANNEL 1/DIMM 2: 1 GB DDR2 FB-DIMM 667 MHz
   BRANCH 1 CHANNEL 0/DIMM 3: 1 GB DDR2 FB-DIMM 667 MHz
   BRANCH 1 CHANNEL 1/DIMM 4: 1 GB DDR2 FB-DIMM 667 MHz