Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CINT2000 Result

Copyright ©1999-2005, Standard Performance Evaluation Corporation

Apple Computer, Inc.

Xserve (3000 MHz Intel Dual-Core Xeon, 1333 MHz Bus)

SPECint2000 = SPECint_base2000 = -- 2929

SPEC license #: 77 Tested by: Apple Computer, Inc. Test date: Nov-2006 Hardware Avail: Nov-2006 Software Avail: Nov-2006

Benchmark

Reference

Time

Base Runtime

Base Ratio Runtime Ratio 2000 4000 6000 8000

164.gzip 1400 77.1 1816

175.vpr 1400 63.5 2205

176.gcc 1100 35.8 3070

181.mcf 1800 41.4 4349

186.crafty 1000 35.4 2827

197.parser 1800 83.3 2161

252.eon 1300 37.6 3456

253.perlbmk 1800 51.9 3470

254.gap 1100 38.2 2878

255.vortex 1900 41.3 4597

256.bzip2 1500 66.9 2244

300.twolf 3000 87.6 3424

Hardware

CPU: Intel Dual-Core Xeon 5160 CPU MHz: 3000 FPU: Integrated CPU(s) enabled: 4 cores, 2 chips, 2 cores/chip CPU(s) orderable: 2 Parallel: No Primary Cache: 32 KB I + 32 KB D on chip per core Secondary Cache: 4 MB I+D on chip per chip (shared) L3 Cache: N/A Other Cache: N/A Memory: 4 GB (4x1GB FB-DIMM DDR2 667 MHz) Disk Subsystem: 80 GB SATA Other Hardware:

Software

Operating System: Mac OS X 10.4.8 (8L2127) Compiler: Intel C++ Compiler for Mac OS X Version 9.1, Build 20060928 (032) File System: Journaled HFS+ System State: Default

Notes/Tuning Information

 +FDO: PASS1=-prof_gen  PASS2=-prof_use

 Base tuning for C programs:   -fast +FDO -lstmalloc
 Base tuning for C++ programs: -fast +FDO -lstmalloc

 Portability flags:
   176.gcc:     -DHOST_WORDS_LITTLE_ENDIAN
   186.crafty:  -DLINUX_i386
   197.parser:  -D_POSIX_SOURCE
   252.eon:     -DHAS_ERRLIST -DFMAX_IS_DOUBLE
   253.perlbmk: -DSPEC_CPU2000_MACOSX_IA32
   254.gap:     -DSYS_IS_BSD -DSYS_HAS_IOCTL_PROTO -DSYS_HAS_TIME_PROTO
                -DSYS_HAS_SIGNAL_PROTO -DSYS_HAS_ANSI -DSYS_HAS_CALLOC_PROTO
                -DSYS_HAS_STDIO_PROTO

 Boot ROM Version: XS11.0076.B00
 SMC Version: 1.11f4

 Memory Details:
   BRANCH 0 CHANNEL 0/DIMM 1: 1 GB DDR2 FB-DIMM 667 MHz

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CINT2000 Result

Copyright ©1999-2005, Standard Performance Evaluation Corporation

Apple Computer, Inc.

Xserve (3000 MHz Intel Dual-Core Xeon, 1333 MHz Bus)

SPECint2000 = SPECint_base2000 = -- 2929

SPEC license #: 77 Tested by: Apple Computer, Inc. Test date: Nov-2006 Hardware Avail: Nov-2006 Software Avail: Nov-2006

Notes/Tuning Information (Continued)

   BRANCH 0 CHANNEL 1/DIMM 2: 1 GB DDR2 FB-DIMM 667 MHz
   BRANCH 1 CHANNEL 0/DIMM 3: 1 GB DDR2 FB-DIMM 667 MHz
   BRANCH 1 CHANNEL 1/DIMM 4: 1 GB DDR2 FB-DIMM 667 MHz