Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2007, Standard Performance Evaluation Corporation

Intel(R) Corporation

Intel(R) DG965WH motherboard( 2.4 GHz, Intel(R) Core(TM) 2 Duo processor E6600)

SPECfp_rate2000 = SPECfp_rate_base2000 =

47.2 47.2

SPEC license #: 13 Tested by: Intel Corporation Test date: Oct-2006 Hardware Avail: Jul-2006 Software Avail: May-2006

Benchmark

Base Copies

Base Runtime

Base Ratio Copies Runtime Ratio 30 60 90 120 150 168.wupwise 2 47.7 77.9 2 47.7 77.9

171.swim 2 185 38.8 2 185 38.8

172.mgrid 2 128 32.6 2 128 32.6

173.applu 2 144 33.8 2 144 33.8

177.mesa 2 62.0 52.3 2 62.0 52.3

178.galgel 2 61.3 110 2 61.2 110

179.art 2 47.2 128 2 47.2 128

183.equake 2 58.8 51.3 2 59.1 51.0

187.facerec 2 82.2 53.6 2 82.8 53.2

188.ammp 2 145 35.3 2 144 35.5

189.lucas 2 117 39.8 2 117 39.7

191.fma3d 2 137 35.6 2 137 35.6

200.sixtrack 2 116 21.9 2 118 21.6

301.apsi 2 162 37.2 2 162 37.2

Hardware

CPU: Intel(R) Core(TM) 2 Duo processor E6600( 2.4 GHz, 1066 MHz bus) CPU MHz: 2400 FPU: Integrated CPU(s) enabled: 2 cores, 1 chip, 2 cores/chip CPU(s) orderable: 1 Parallel: No Primary Cache: 32KBI + 32KBD per core, on chip Secondary Cache: 4 MB(I+D) per chip, on chip (shared) L3 Cache: None Other Cache: None Memory: 2 GB (2 1GB Micron MT16HTF12864AY-80ED4 DDR2 800, CL5) Disk Subsystem: Maxtor DiamondMax 10 6B300S0 300GB NCQ Serial ATA (7200 RPM, 16MB cache) Other Hardware: SoundBlaster Live! PCI card

Software

Operating System: Windows XP Professional SP2 Compiler: Intel C++ and Fortran Compiler 9.1 for 32-bit applications

Build 20060323Z Package IDs: W_CC_P_9.1.020 and W_FC_P_9.1.020 Microsoft Visual Studio 2005(for libraries) SmartHeap Library Version 8.0 from http://www.microquill.com/

File System: NTFS System State: Default

Notes/Tuning Information

 +FDO: PASS1=  -Qprof_gen  PASS2=-Qprof_use
 Base tuning for Fortran programs:  -fast -Qansi_alias +FDO
 Base tuning for 177.mesa:   -fast   +FDO shlW32M.lib
 Base tuning for 179.art:    -fast   +FDO shlW32M.lib
 Base tuning for 183.equake: -fast   +FDO shlW32M.lib
 Base tuning for 188.ammp:   -fast   +FDO shlW32M.lib
 Portability:
 178.galgel:   -FI /F32000000
 Peak tuning:
 168.wupwise:  -fast -Qansi_alias +FDO
 171.swim:     -fast -Qansi_alias +FDO
 172.mgrid:    -fast -Qansi_alias +FDO
 173.applu:  basepeak=yes
 177.mesa:   basepeak=yes
 178.galgel:   -fast -Qansi_alias +FDO
 179.art:      basepeak=yes
 183.equake:   -QxP -Oa -Qrcd -Qipo  +FDO  shlW32M.lib

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2007, Standard Performance Evaluation Corporation

Intel(R) Corporation

Intel(R) DG965WH motherboard( 2.4 GHz, Intel(R) Core(TM) 2 Duo processor E6600)

SPECfp_rate2000 = SPECfp_rate_base2000 =

47.2 47.2

SPEC license #: 13 Tested by: Intel Corporation Test date: Oct-2006 Hardware Avail: Jul-2006 Software Avail: May-2006

Notes/Tuning Information (Continued)

 187.facerec:  -fast -Qunroll1 -Qscalar_rep- +FDO
 188.ammp:     -fast -Oa +FDO  shlW32M.lib
 189.lucas:    -fast -Qprefetch- +FDO
 191.fma3d:    basepeak=yes
 200.sixtrack: -Qipo -QxP +FDO
 301.apsi:     -fast +FDO
 Tested systems can be used with Shin-G ATX case, Antec NeoPower 480W power supply
 Product description located as of 1/2007:
 http://www.intel.com/products/motherboard/DG965WH/index.htm
 The system bus runs at 1066 MHz