Standard Performance Evaluation Corporation info@spec.org http://www.spec.org/

Page 1 spec^® SPEC

® CFP2006 Result

Copyright 2006-2014 Standard Performance Evaluation Corporation

Fujitsu Siemens Computers

2.66 GHz

PRIMERGY RX200 S4, Intel Xeon processor E5430,

SPECfp^®_rate2006 = 65.9 SPECfp_rate_base2006 = 65.9

CPU2006 license: 22 Test date: Nov-2007 Test sponsor: Fujitsu Siemens Computers Hardware Availability: Dec-2007 Tested by: Fujitsu Siemens Computers Software Availability: Nov-2007 410.bwaves 416.gamess 433.milc 434.zeusmp 435.gromacs 436.cactusADM

437.leslie3d 444.namd 447.dealII 450.soplex 453.povray 454.calculix 459.GemsFDTD

465.tonto 470.lbm 481.wrf 482.sphinx3

Copies

SPECfp_rate2006 = 65.9

SPECfp_rate_base2006 = 65.9

0 180

10.0 20.0 30.0 40.0 50.0 60.0 70.0 80.0 90.0 100 110 120 130 140 150 160 170 8 35.3

8 156

8 33.3

8 66.9

8 129

8 70.1

8 27.6

8 112

8 122

8 37.6

8 176

8 106

8 28.7

8 108

8 26.5

8 50.4

8 67.6

Hardware

CPU Name: Intel Xeon E5430 CPU Characteristics: 1333 MHz system bus CPU MHz: 2667 FPU: Integrated CPU(s) enabled: 8 cores, 2 chips, 4 cores/chip CPU(s) orderable: 1,2 chips Primary Cache: 32 KB I + 32 KB D on chip per core Secondary Cache: 12 MB I+D on chip per chip, 6 MB shared / 2 cores

Software

Operating System: SUSE Linux Enterprise Server 10 (x86_64) SP1,

Kernel 2.6.16.46-0.12-smp

Compiler: Intel C++ and Fortran Compiler for Linux32 and Linux64 Version 10.1 - Build 20070725 Auto Parallel: No File System: ext2 System State: Multiuser, Runlevel 3 Base Pointers: 64-bit

Continued on next page Continued on next page

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org/

Page 2 spec^® SPEC CFP2006 Result

Copyright 2006-2014 Standard Performance Evaluation Corporation

Fujitsu Siemens Computers

2.66 GHz

PRIMERGY RX200 S4, Intel Xeon processor E5430,

SPECfp_rate2006 = 65.9 SPECfp_rate_base2006 = 65.9

CPU2006 license: 22 Test date: Nov-2007 Test sponsor: Fujitsu Siemens Computers Hardware Availability: Dec-2007 Tested by: Fujitsu Siemens Computers Software Availability: Nov-2007 L3 Cache: None Other Cache: None Memory: 16 GB (8x2 GB PC2-5300F, 2 rank, CAS 5-5-5,

with ECC)

Disk Subsystem: Seagate ST973451SS (SAS, 73GB, 15000rpm) Other Hardware: None

Peak Pointers: 64-bit Other Software: None

Results Table

Benchmark Copies Seconds Ratio Seconds Ratio Seconds Ratio

Base Copies Seconds Ratio Seconds Ratio Seconds Ratio

Peak

410.bwaves 8 3084 35.3 3084 35.3 3083 35.3 8 3084 35.3 3084 35.3 3083 35.3 416.gamess 8 1002 156 1000 157 1001 156 8 1002 156 1000 157 1001 156 433.milc 8 2251 32.6 2208 33.3 2208 33.3 8 2251 32.6 2208 33.3 2208 33.3 434.zeusmp 8 1084 67.1 1089 66.8 1088 66.9 8 1084 67.1 1089 66.8 1088 66.9 435.gromacs 8 441 129 449 127 441 130 8 441 129 449 127 441 130 436.cactusADM 8 1365 70.0 1365 70.1 1360 70.3 8 1365 70.0 1365 70.1 1360 70.3 437.leslie3d 8 2722 27.6 2734 27.5 2729 27.6 8 2722 27.6 2734 27.5 2729 27.6 444.namd 8 582 110 574 112 574 112 8 582 110 574 112 574 112 447.dealII 8 748 122 736 124 752 122 8 748 122 736 124 752 122 450.soplex 8 1780 37.5 1776 37.6 1773 37.6 8 1780 37.5 1776 37.6 1773 37.6 453.povray 8 242 176 242 176 242 176 8 242 176 242 176 242 176 454.calculix 8 624 106 633 104 616 107 8 624 106 633 104 616 107 459.GemsFDTD 8 2931 29.0 2962 28.7 2953 28.7 8 2931 29.0 2962 28.7 2953 28.7 465.tonto 8 724 109 727 108 728 108 8 724 109 727 108 728 108 470.lbm 8 4148 26.5 4145 26.5 4143 26.5 8 4148 26.5 4145 26.5 4143 26.5 481.wrf 8 1775 50.4 1771 50.4 1766 50.6 8 1775 50.4 1771 50.4 1766 50.6 482.sphinx3 8 2297 67.9 2305 67.6 2306 67.6 8 2297 67.9 2305 67.6 2306 67.6

Results appear in the order in which they were run. Bold underlined text indicates a median measurement.

Operating System Notes

 ’ulimit -s unlimited’ was used to set the stacksize to unlimited prior to run

General Notes

 This result has been produced with binaries provided and compiled by Intel.
 BIOS configuration:
 Hardware Prefetch = Disable, Adjacent Sector Prefetch = Disable
 For information about Fujitsu Siemens Computers please see:
 http://www.fujitsu-siemens.com

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org/

Page 3 spec^® SPEC CFP2006 Result

Copyright 2006-2014 Standard Performance Evaluation Corporation

Fujitsu Siemens Computers

2.66 GHz

PRIMERGY RX200 S4, Intel Xeon processor E5430,

SPECfp_rate2006 = 65.9

SPECfp_rate_base2006 = 65.9

CPU2006 license: 22 Test date: Nov-2007 Test sponsor: Fujitsu Siemens Computers Hardware Availability: Dec-2007 Tested by: Fujitsu Siemens Computers Software Availability: Nov-2007

Base Compiler Invocation

C benchmarks:

icc

C++ benchmarks:

icpc

Fortran benchmarks:

ifort

Benchmarks using both Fortran and C:

icc ifort

Base Portability Flags

410.bwaves: -DSPEC_CPU_LP64 416.gamess: -DSPEC_CPU_LP64

433.milc: -DSPEC_CPU_LP64 434.zeusmp: -DSPEC_CPU_LP64 435.gromacs: -DSPEC_CPU_LP64 -nofor_main 436.cactusADM: -DSPEC_CPU_LP64 -nofor_main 437.leslie3d: -DSPEC_CPU_LP64

444.namd: -DSPEC_CPU_LP64 447.dealII: -DSPEC_CPU_LP64 450.soplex: -DSPEC_CPU_LP64 453.povray: -DSPEC_CPU_LP64 454.calculix: -DSPEC_CPU_LP64 -nofor_main 459.GemsFDTD: -DSPEC_CPU_LP64

465.tonto: -DSPEC_CPU_LP64 470.lbm: -DSPEC_CPU_LP64 481.wrf: -DSPEC_CPU_LP64 -DSPEC_CPU_CASE_FLAG -DSPEC_CPU_LINUX 482.sphinx3: -DSPEC_CPU_LP64

Base Optimization Flags

C benchmarks:

-fast

C++ benchmarks:

-fast

Fortran benchmarks:

-fast

Benchmarks using both Fortran and C:

-fast

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org/

Page 4 spec^® SPEC CFP2006 Result

Copyright 2006-2014 Standard Performance Evaluation Corporation

Fujitsu Siemens Computers

2.66 GHz

PRIMERGY RX200 S4, Intel Xeon processor E5430,

SPECfp_rate2006 = 65.9 SPECfp_rate_base2006 = 65.9

CPU2006 license: 22 Test date: Nov-2007 Test sponsor: Fujitsu Siemens Computers Hardware Availability: Dec-2007 Tested by: Fujitsu Siemens Computers Software Availability: Nov-2007

Peak Optimization Flags

C benchmarks:

433.milc: basepeak = yes 470.lbm: basepeak = yes 482.sphinx3: basepeak = yes C++ benchmarks:

444.namd: basepeak = yes 447.dealII: basepeak = yes 450.soplex: basepeak = yes 453.povray: basepeak = yes Fortran benchmarks:

410.bwaves: basepeak = yes 416.gamess: basepeak = yes 434.zeusmp: basepeak = yes 437.leslie3d: basepeak = yes 459.GemsFDTD: basepeak = yes

465.tonto: basepeak = yes Benchmarks using both Fortran and C:

435.gromacs: basepeak = yes 436.cactusADM: basepeak = yes

454.calculix: basepeak = yes 481.wrf: basepeak = yes

The flags file that was used to format this result can be browsed at

http://www.spec.org/cpu2006/flags/Intel-ic10.1-FP-intel64-linux-flags.20090714.05.html

You can also download the XML flags source by saving the following link:

http://www.spec.org/cpu2006/flags/Intel-ic10.1-FP-intel64-linux-flags.20090714.05.xml

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org/

Page 5 spec^® SPEC CFP2006 Result

Copyright 2006-2014 Standard Performance Evaluation Corporation

Fujitsu Siemens Computers

2.66 GHz

PRIMERGY RX200 S4, Intel Xeon processor E5430,

SPECfp_rate2006 = 65.9 SPECfp_rate_base2006 = 65.9

CPU2006 license: 22 Test date: Nov-2007 Test sponsor: Fujitsu Siemens Computers Hardware Availability: Dec-2007 Tested by: Fujitsu Siemens Computers Software Availability: Nov-2007

Originally published on 12 December 2007.

Report generated on Tue Jul 22 13:32:11 2014 by SPEC CPU2006 PS/PDF formatter v6932.

Tested with SPEC CPU2006 v1.0.

For other inquiries, please contact webmaster@spec.org.

For questions about this result, please contact the tester.

holders.

this result are trademarks or registered trademarks of their respective

Evaluation Corporation. All other brand and product names appearing in

SPEC and SPECfp are registered trademarks of the Standard Performance