Page 1 Standard Performance Evaluation Corporation (info@spec.org) https://www.spec.org/ spec^® SPEC CPU

®2017 Floating Point Rate Result

Copyright 2017-2020 Standard Performance Evaluation Corporation

(Test Sponsor: HPE)

Hewlett Packard Enterprise

(2.40 GHz, Intel Xeon E5-2699A v4)

ProLiant DL380 Gen9 SPECrate®2017_fp_peak = 148

SPECrate^®2017_fp_base = 147

CPU2017 License: 3 Test Date: Dec-2016 Test Sponsor: HPE Hardware Availability: Oct-2016 Tested by: HPE Software Availability: Sep-2016

503.bwaves_r

507.cactuBSSN_r

508.namd_r

510.parest_r

511.povray_r

519.lbm_r

521.wrf_r

526.blender_r

527.cam4_r

538.imagick_r

544.nab_r

549.fotonik3d_r

554.roms_r

Copies

(148)

SPECrate^®2017_fp_peak

(147)

SPECrate^®2017_fp_base

0 305

15.0 30.0 45.0 60.0 75.0 90.0 105 120 135 150 165 180 195 210 225 240 255 270 285 88 298 296 88 113 111 88 154 155 88 72.9 73.0 88 242 297 88 73.5 73.4 88 134 133 88 221 217 88 182 182 88 235 215 88 299 304 88 97.1 93.6 88 60.8 60.2

Hardware

CPU Name: Intel Xeon E5-2699A v4 Max MHz: 3600 Nominal: 2400 Enabled: 44 cores, 2 chips, 2 threads/core Orderable: 1,2 chips Cache L1: 32 KB I + 32 KB D on chip per core L2: 256 KB I+D on chip per core L3: 55 MB I+D on chip per chip Other: None Memory: 512 GB (16 x 32 GB 2Rx4 PC4-2400T-R) Storage: 1 x 400 GB SAS SSD, RAID 0 Other: None

Software

OS: SUSE Linux Enterprise Server 12 (x86_64) SP1

Kernel 3.12.49-11-default

Compiler: C/C++: Version 17.0.0.098 of Intel C/C++ Compiler for Linux;

Fortran: Version 17.0.0.098 of Intel Fortran Compiler for Linux Parallel: No Firmware: P89 v2.30 9/12/16 File System: xfs System State: Run level 3 (multi-user) Base Pointers: 32/64-bit Peak Pointers: 32/64-bit Other: Microquill SmartHeap V10.2 Power Management: --

Page 2 Standard Performance Evaluation Corporation (info@spec.org) https://www.spec.org/ spec^® SPEC CPU

®2017 Floating Point Rate Result

Copyright 2017-2020 Standard Performance Evaluation Corporation

(Test Sponsor: HPE)

Hewlett Packard Enterprise

(2.40 GHz, Intel Xeon E5-2699A v4)

ProLiant DL380 Gen9 SPECrate®2017_fp_peak = 148

SPECrate^®2017_fp_base = 147

CPU2017 License: 3 Test Date: Dec-2016 Test Sponsor: HPE Hardware Availability: Oct-2016 Tested by: HPE Software Availability: Sep-2016

Results Table

Benchmark Copies Seconds Ratio Seconds Ratio Seconds Ratio

Base Copies Seconds Ratio Seconds Ratio Seconds Ratio

Peak

503.bwaves_r 88 2957 298 2955 299 2956 298 88 2979 296 2978 296 2979 296 507.cactuBSSN_r 88 989 113 989 113 991 112 88 1001 111 1004 111 1004 111 508.namd_r 88 545 153 544 154 543 154 88 540 155 535 156 540 155 510.parest_r 88 3157 72.9 3158 72.9 3166 72.7 88 3153 73.0 3158 72.9 3151 73.1 511.povray_r 88 850 242 844 243 848 242 88 691 297 689 298 692 297 519.lbm_r 88 1262 73.5 1262 73.5 1262 73.5 88 1263 73.4 1265 73.3 1263 73.4 521.wrf_r 88 1473 134 1473 134 1475 134 88 1477 133 1482 133 1482 133 526.blender_r 88 607 221 606 221 607 221 88 617 217 615 218 617 217 527.cam4_r 88 844 182 844 182 847 182 88 844 182 846 182 847 182 538.imagick_r 88 931 235 930 235 932 235 88 1019 215 1019 215 1021 214 544.nab_r 88 495 299 494 300 495 299 88 486 305 487 304 487 304 549.fotonik3d_r 88 3543 96.8 3533 97.1 3529 97.2 88 3661 93.7 3664 93.6 3663 93.6 554.roms_r 88 2301 60.8 2298 60.8 2305 60.7 88 2325 60.2 2324 60.2 2321 60.2 SPECrate^®2017_fp_base = 147 SPECrate^®2017_fp_peak = 148

Results appear in the order in which they were run. Bold underlined text indicates a median measurement.

Submit Notes

The config file option ’submit’ was used.

Operating System Notes

 Stack size set to unlimited using "ulimit -s unlimited"
 Transparent Huge Pages enabled by default
 Filesystem page cache cleared with:
  echo 1 >       /proc/sys/vm/drop_caches
 runcpu command invoked through numactl i.e.:
  numactl --interleave=all runcpu <etc>

General Notes

Environment variables set by runcpu before the start of the run:
LD_LIBRARY_PATH = "/home/cpu2017/lib/ia32:/home/cpu2017/lib/intel64:/home/cpu2017/sh10.2"

 Binaries compiled on a system with 1x Intel Core i7-4790K CPU + 32GB RAM
 memory using Redhat Enterprise Linux 7.2

Platform Notes

 BIOS Configuration:
   Power Profile set to Custom

(Continued on next page)

Page 3 Standard Performance Evaluation Corporation (info@spec.org) https://www.spec.org/ spec^® SPEC CPU

®2017 Floating Point Rate Result

Copyright 2017-2020 Standard Performance Evaluation Corporation

(Test Sponsor: HPE)

Hewlett Packard Enterprise

(2.40 GHz, Intel Xeon E5-2699A v4)

ProLiant DL380 Gen9 SPECrate®2017_fp_peak = 148

SPECrate^®2017_fp_base = 147

CPU2017 License: 3 Test Date: Dec-2016 Test Sponsor: HPE Hardware Availability: Oct-2016 Tested by: HPE Software Availability: Sep-2016

Platform Notes (Continued)

   Power Regulator set to Static High Performance Mode
   Minimum Processor Idle Power Core C-State set to C3 State
   Minimum Processor Idle Power Package C-State set to No Package State
   Collaborative Power Control set to Disabled
   QPI Snoop Configuration set to Cluster On Die
   Thermal Configuration set to Maximum Cooling
   Processor Power and Utilization Monitoring set to Disabled
   Memory Refresh Rate set to 1x Refresh
   Energy Performance Bias set to Balanced Performance
 Sysinfo program /home/cpu2017/Docs/sysinfo
 Rev: r5007 of 2016-11-15 fc8dc82f217779bedfed4d694d580ba9
 running on dl380-gen9-2699a Sat Dec 10 00:28:29 2016

 This section contains SUT (System Under Test) info as seen by some common
 utilities.
 For more information on this section, see
 http://www.spec.org/cpu2017/Docs/config.html#sysinfo

 From /proc/cpuinfo
    model name : Intel(R) Xeon(R) CPU E5-2699A v4 @ 2.40GHz
       2 "physical id"s (chips)
       88 "processors"
    cores, siblings (Caution: counting these is hw and system dependent.  The
    following excerpts from /proc/cpuinfo might not be reliable.  Use with
    caution.)
       cpu cores : 22
       siblings  : 44
       physical 0: cores 0 1 2 3 4 5 8 9 10 11 12 16 17 18 19 20 21 24 25 26 27
       28
       physical 1: cores 0 1 2 3 4 5 8 9 10 11 12 16 17 18 19 20 21 24 25 26 27
       28
    cache size : 28160 KB

 The view from numactl --hardware follows.  WARNING: a numactl ’node’ might or
 might not correspond to a physical chip.
   available: 4 nodes (0-3)
   node 0 cpus: 0 1 2 3 4 5 6 7 8 9 10 44 45 46 47 48 49 50 51 52 53 54
   node 0 size: 128869 MB
   node 0 free: 128230 MB
   node 1 cpus: 11 12 13 14 15 16 17 18 19 20 21 55 56 57 58 59 60 61 62 63 64 65
   node 1 size: 129277 MB
   node 1 free: 128701 MB
   node 2 cpus: 22 23 24 25 26 27 28 29 30 31 32 66 67 68 69 70 71 72 73 74 75 76
   node 2 size: 129277 MB
   node 2 free: 128714 MB
   node 3 cpus: 33 34 35 36 37 38 39 40 41 42 43 77 78 79 80 81 82 83 84 85 86 87
   node 3 size: 129133 MB

(Continued on next page)

Page 4 Standard Performance Evaluation Corporation (info@spec.org) https://www.spec.org/ spec^® SPEC CPU

®2017 Floating Point Rate Result

Copyright 2017-2020 Standard Performance Evaluation Corporation

(Test Sponsor: HPE)

Hewlett Packard Enterprise

(2.40 GHz, Intel Xeon E5-2699A v4)

ProLiant DL380 Gen9 SPECrate®2017_fp_peak = 148

SPECrate^®2017_fp_base = 147

CPU2017 License: 3 Test Date: Dec-2016 Test Sponsor: HPE Hardware Availability: Oct-2016 Tested by: HPE Software Availability: Sep-2016

Platform Notes (Continued)

   node 3 free: 128592 MB
   node distances:
   node   0   1   2   3
     0:  10  21  31  31
     1:  21  10  31  31
     2:  31  31  10  21
     3:  31  31  21  10

 From /proc/meminfo
    MemTotal:       528955384 kB
    HugePages_Total:       0
    Hugepagesize:       2048 kB

 /usr/bin/lsb_release -d
    SUSE Linux Enterprise Server 12 SP1

 From /etc/*release* /etc/*version*
    SuSE-release:
       SUSE Linux Enterprise Server 12 (x86_64)
       VERSION = 12
       PATCHLEVEL = 1
       # This file is deprecated and will be removed in a future service pack or
       release.
       # Please check /etc/os-release for details about this release.
    os-release:
       NAME="SLES"
       VERSION="12-SP1"
       VERSION_ID="12.1"
       PRETTY_NAME="SUSE Linux Enterprise Server 12 SP1"
       ID="sles"
       ANSI_COLOR="0;32"
       CPE_NAME="cpe:/o:suse:sles:12:sp1"

 uname -a:
    Linux dl380-gen9-2699a 3.12.49-11-default #1 SMP Wed Nov 11 20:52:43 UTC 2015
    (8d714a0) x86_64 x86_64 x86_64 GNU/Linux

 run-level 3 Dec 10 00:25

 SPEC is set to: /home/cpu2017
    Filesystem     Type  Size  Used Avail Use% Mounted on
    /dev/sda4      xfs   331G  137G  194G  42% /home

 Additional information from dmidecode follows.  WARNING: Use caution when you
 interpret this section. The ’dmidecode’ program reads system data which is
 "intended to allow hardware to be accurately determined", but the intent may not
 be met, as there are frequent changes to hardware, firmware, and the "DMTF

(Continued on next page)

Page 5 Standard Performance Evaluation Corporation (info@spec.org) https://www.spec.org/ spec^® SPEC CPU

®2017 Floating Point Rate Result

Copyright 2017-2020 Standard Performance Evaluation Corporation

(Test Sponsor: HPE)

Hewlett Packard Enterprise

(2.40 GHz, Intel Xeon E5-2699A v4)

ProLiant DL380 Gen9 SPECrate®2017_fp_peak = 148

SPECrate^®2017_fp_base = 147

CPU2017 License: 3 Test Date: Dec-2016 Test Sponsor: HPE Hardware Availability: Oct-2016 Tested by: HPE Software Availability: Sep-2016

Platform Notes (Continued)

 SMBIOS" standard.
   BIOS HP P89 09/12/2016
   Memory:
    8x UNKNOWN NOT AVAILABLE
    16x UNKNOWN NOT AVAILABLE 32 GB 2 rank 2400 MHz

 (End of data from sysinfo program)

Compiler Version Notes

==============================================================================
C               | 519.lbm_r(base, peak) 538.imagick_r(base, peak)
                | 544.nab_r(base, peak)
------------------------------------------------------------------------------
icc (ICC) 17.0.0 20160721
Copyright (C) 1985-2016 Intel Corporation.  All rights reserved.
------------------------------------------------------------------------------

==============================================================================
C++             | 508.namd_r(base, peak) 510.parest_r(base, peak)
------------------------------------------------------------------------------
icpc (ICC) 17.0.0 20160721
Copyright (C) 1985-2016 Intel Corporation.  All rights reserved.
------------------------------------------------------------------------------

==============================================================================
C++, C          | 511.povray_r(base pass 0, base pass 0, peak pass 1, peak
                | pass 1, peak pass 2, peak pass 2) 526.blender_r(base pass
                | 0, base pass 0, peak pass 1, peak pass 1, peak pass 2, peak
                | pass 2)
------------------------------------------------------------------------------
icc (ICC) 17.0.0 20160721
Copyright (C) 1985-2016 Intel Corporation.  All rights reserved.
------------------------------------------------------------------------------

==============================================================================
C++, C          | 507.cactuBSSN_r(base pass 0, peak pass 1) 511.povray_r(base
                | pass 0, base pass 0, peak pass 1, peak pass 1, peak pass 2,
                | peak pass 2) 526.blender_r(base pass 0, base pass 0, peak
                | pass 1, peak pass 1, peak pass 2, peak pass 2)
------------------------------------------------------------------------------
icpc (ICC) 17.0.0 20160721
Copyright (C) 1985-2016 Intel Corporation.  All rights reserved.
------------------------------------------------------------------------------

==============================================================================

(Continued on next page)

Page 6 Standard Performance Evaluation Corporation (info@spec.org) https://www.spec.org/ spec^® SPEC CPU

®2017 Floating Point Rate Result

Copyright 2017-2020 Standard Performance Evaluation Corporation

(Test Sponsor: HPE)

Hewlett Packard Enterprise

(2.40 GHz, Intel Xeon E5-2699A v4)

ProLiant DL380 Gen9 SPECrate®2017_fp_peak = 148

SPECrate^®2017_fp_base = 147

CPU2017 License: 3 Test Date: Dec-2016 Test Sponsor: HPE Hardware Availability: Oct-2016 Tested by: HPE Software Availability: Sep-2016

Compiler Version Notes (Continued)

C++, C          | 511.povray_r(base pass 0, base pass 0, peak pass 1, peak
                | pass 1, peak pass 2, peak pass 2) 526.blender_r(base pass
                | 0, base pass 0, peak pass 1, peak pass 1, peak pass 2, peak
                | pass 2)
------------------------------------------------------------------------------
icc (ICC) 17.0.0 20160721
Copyright (C) 1985-2016 Intel Corporation.  All rights reserved.
------------------------------------------------------------------------------

==============================================================================
C++, C          | 507.cactuBSSN_r(base pass 0, peak pass 1) 511.povray_r(base
                | pass 0, base pass 0, peak pass 1, peak pass 1, peak pass 2,
                | peak pass 2) 526.blender_r(base pass 0, base pass 0, peak
                | pass 1, peak pass 1, peak pass 2, peak pass 2)
------------------------------------------------------------------------------
icpc (ICC) 17.0.0 20160721
Copyright (C) 1985-2016 Intel Corporation.  All rights reserved.
------------------------------------------------------------------------------

==============================================================================
C++, C, Fortran | 507.cactuBSSN_r(base pass 0, peak pass 1, peak pass 2)
------------------------------------------------------------------------------
icc (ICC) 17.0.0 20160721
Copyright (C) 1985-2016 Intel Corporation.  All rights reserved.
------------------------------------------------------------------------------

==============================================================================
C++, C, Fortran | 507.cactuBSSN_r(peak pass 2)
------------------------------------------------------------------------------
icpc (ICC) 17.0.0 20160721
Copyright (C) 1985-2016 Intel Corporation.  All rights reserved.
------------------------------------------------------------------------------

==============================================================================
C++, C, Fortran | 507.cactuBSSN_r(base pass 0, peak pass 1, peak pass 2)
------------------------------------------------------------------------------
ifort (IFORT) 17.0.0 20160721
Copyright (C) 1985-2016 Intel Corporation.  All rights reserved.
------------------------------------------------------------------------------

==============================================================================
C++, C, Fortran | 507.cactuBSSN_r(base pass 0, peak pass 1, peak pass 2)
------------------------------------------------------------------------------
icc (ICC) 17.0.0 20160721
Copyright (C) 1985-2016 Intel Corporation.  All rights reserved.
------------------------------------------------------------------------------

(Continued on next page)

Page 7 Standard Performance Evaluation Corporation (info@spec.org) https://www.spec.org/ spec^® SPEC CPU

®2017 Floating Point Rate Result

Copyright 2017-2020 Standard Performance Evaluation Corporation

(Test Sponsor: HPE)

Hewlett Packard Enterprise

(2.40 GHz, Intel Xeon E5-2699A v4)

ProLiant DL380 Gen9 SPECrate®2017_fp_peak = 148

SPECrate^®2017_fp_base = 147

CPU2017 License: 3 Test Date: Dec-2016 Test Sponsor: HPE Hardware Availability: Oct-2016 Tested by: HPE Software Availability: Sep-2016

Compiler Version Notes (Continued)

==============================================================================
C++, C, Fortran | 507.cactuBSSN_r(peak pass 2)
------------------------------------------------------------------------------
icpc (ICC) 17.0.0 20160721
Copyright (C) 1985-2016 Intel Corporation.  All rights reserved.
------------------------------------------------------------------------------

==============================================================================
C++, C, Fortran | 507.cactuBSSN_r(base pass 0, peak pass 1, peak pass 2)
------------------------------------------------------------------------------
ifort (IFORT) 17.0.0 20160721
Copyright (C) 1985-2016 Intel Corporation.  All rights reserved.
------------------------------------------------------------------------------

==============================================================================
C++, C, Fortran | 507.cactuBSSN_r(base pass 0, peak pass 1, peak pass 2)
------------------------------------------------------------------------------
icc (ICC) 17.0.0 20160721
Copyright (C) 1985-2016 Intel Corporation.  All rights reserved.
------------------------------------------------------------------------------

==============================================================================
C++, C, Fortran | 507.cactuBSSN_r(peak pass 2)
------------------------------------------------------------------------------
icpc (ICC) 17.0.0 20160721
Copyright (C) 1985-2016 Intel Corporation.  All rights reserved.
------------------------------------------------------------------------------

==============================================================================
C++, C, Fortran | 507.cactuBSSN_r(base pass 0, peak pass 1, peak pass 2)
------------------------------------------------------------------------------
ifort (IFORT) 17.0.0 20160721
Copyright (C) 1985-2016 Intel Corporation.  All rights reserved.
------------------------------------------------------------------------------

==============================================================================
Fortran         | 503.bwaves_r(base, peak) 549.fotonik3d_r(base, peak)
                | 554.roms_r(base, peak)
------------------------------------------------------------------------------
ifort (IFORT) 17.0.0 20160721
Copyright (C) 1985-2016 Intel Corporation.  All rights reserved.
------------------------------------------------------------------------------

==============================================================================
Fortran, C      | 521.wrf_r(base pass 0, base pass 0, peak pass 1, peak pass
                | 1, peak pass 2, peak pass 2) 527.cam4_r(base pass 0, base
                | pass 0, peak pass 1, peak pass 1, peak pass 2, peak pass 2)

(Continued on next page)

Page 8 Standard Performance Evaluation Corporation (info@spec.org) https://www.spec.org/ spec^® SPEC CPU

®2017 Floating Point Rate Result

Copyright 2017-2020 Standard Performance Evaluation Corporation

(Test Sponsor: HPE)

Hewlett Packard Enterprise

(2.40 GHz, Intel Xeon E5-2699A v4)

ProLiant DL380 Gen9 SPECrate®2017_fp_peak = 148

SPECrate^®2017_fp_base = 147

CPU2017 License: 3 Test Date: Dec-2016 Test Sponsor: HPE Hardware Availability: Oct-2016 Tested by: HPE Software Availability: Sep-2016

Compiler Version Notes (Continued)

------------------------------------------------------------------------------
icc (ICC) 17.0.0 20160721
Copyright (C) 1985-2016 Intel Corporation.  All rights reserved.
------------------------------------------------------------------------------

==============================================================================
Fortran, C      | 521.wrf_r(base pass 0, base pass 0, peak pass 1, peak pass
                | 1, peak pass 2, peak pass 2) 527.cam4_r(base pass 0, base
                | pass 0, peak pass 1, peak pass 1, peak pass 2, peak pass 2)
------------------------------------------------------------------------------
ifort (IFORT) 17.0.0 20160721
Copyright (C) 1985-2016 Intel Corporation.  All rights reserved.
------------------------------------------------------------------------------

==============================================================================
Fortran, C      | 521.wrf_r(base pass 0, base pass 0, peak pass 1, peak pass
                | 1, peak pass 2, peak pass 2) 527.cam4_r(base pass 0, base
                | pass 0, peak pass 1, peak pass 1, peak pass 2, peak pass 2)
------------------------------------------------------------------------------
icc (ICC) 17.0.0 20160721
Copyright (C) 1985-2016 Intel Corporation.  All rights reserved.
------------------------------------------------------------------------------

==============================================================================
Fortran, C      | 521.wrf_r(base pass 0, base pass 0, peak pass 1, peak pass
                | 1, peak pass 2, peak pass 2) 527.cam4_r(base pass 0, base
                | pass 0, peak pass 1, peak pass 1, peak pass 2, peak pass 2)
------------------------------------------------------------------------------
ifort (IFORT) 17.0.0 20160721
Copyright (C) 1985-2016 Intel Corporation.  All rights reserved.
------------------------------------------------------------------------------

Base Compiler Invocation

C benchmarks:

icc -m64 -std=c11

C++ benchmarks:

icpc -m64

Fortran benchmarks:

ifort -m64

Benchmarks using both Fortran and C:

ifort -m64 icc -m64 -std=c11

(Continued on next page)

Page 9 Standard Performance Evaluation Corporation (info@spec.org) https://www.spec.org/ spec^® SPEC CPU

®2017 Floating Point Rate Result

Copyright 2017-2020 Standard Performance Evaluation Corporation

(Test Sponsor: HPE)

Hewlett Packard Enterprise

(2.40 GHz, Intel Xeon E5-2699A v4)

ProLiant DL380 Gen9 SPECrate®2017_fp_peak = 148

SPECrate^®2017_fp_base = 147

CPU2017 License: 3 Test Date: Dec-2016 Test Sponsor: HPE Hardware Availability: Oct-2016 Tested by: HPE Software Availability: Sep-2016

Base Compiler Invocation (Continued)

Benchmarks using both C and C++:

icpc -m64 icc -m64 -std=c11

Benchmarks using Fortran, C, and C++:

icpc -m64 icc -m64 -std=c11 ifort -m64

Base Portability Flags

503.bwaves_r: -DSPEC_LP64 507.cactuBSSN_r: -DSPEC_LP64 508.namd_r: -DSPEC_LP64 510.parest_r: -DSPEC_LP64 511.povray_r: -DSPEC_LP64 519.lbm_r: -DSPEC_LP64 521.wrf_r: -DSPEC_LP64 -DSPEC_CASE_FLAG -convert big_endian 526.blender_r: -DSPEC_LP64 -DSPEC_LINUX -funsigned-char 527.cam4_r: -DSPEC_LP64 -DSPEC_CASE_FLAG 538.imagick_r: -DSPEC_LP64 544.nab_r: -DSPEC_LP64 549.fotonik3d_r: -DSPEC_LP64 554.roms_r: -DSPEC_LP64

Base Optimization Flags

C benchmarks:

-xCORE-AVX2 -ipo -O3 -no-prec-div -auto-p32 -qopt-prefetch
-qopt-mem-layout-trans=3

C++ benchmarks:

-Wl,-z,muldefs -xCORE-AVX2 -ipo -O3 -no-prec-div -auto-p32
-qopt-prefetch -qopt-mem-layout-trans=3 -L/sh10.2 -lsmartheap64

Fortran benchmarks:

-xCORE-AVX2 -ipo -O3 -no-prec-div -qopt-prefetch
-qopt-mem-layout-trans=3 -nostandard-realloc-lhs

Benchmarks using both Fortran and C:

-xCORE-AVX2 -ipo -O3 -no-prec-div -auto-p32 -qopt-prefetch
-qopt-mem-layout-trans=3 -nostandard-realloc-lhs

Benchmarks using both C and C++:

-Wl,-z,muldefs -xCORE-AVX2 -ipo -O3 -no-prec-div -auto-p32

(Continued on next page)

Page 10 Standard Performance Evaluation Corporation (info@spec.org) https://www.spec.org/ spec^® SPEC CPU

®2017 Floating Point Rate Result

Copyright 2017-2020 Standard Performance Evaluation Corporation

(Test Sponsor: HPE)

Hewlett Packard Enterprise

(2.40 GHz, Intel Xeon E5-2699A v4)

ProLiant DL380 Gen9 SPECrate®2017_fp_peak = 148

SPECrate^®2017_fp_base = 147

CPU2017 License: 3 Test Date: Dec-2016 Test Sponsor: HPE Hardware Availability: Oct-2016 Tested by: HPE Software Availability: Sep-2016

Base Optimization Flags (Continued)

Benchmarks using both C and C++ (continued):

-qopt-prefetch -qopt-mem-layout-trans=3 -L/sh10.2 -lsmartheap64

Benchmarks using Fortran, C, and C++:

-Wl,-z,muldefs -xCORE-AVX2 -ipo -O3 -no-prec-div -auto-p32
-qopt-prefetch -qopt-mem-layout-trans=3 -nostandard-realloc-lhs
-L/sh10.2 -lsmartheap64

Peak Compiler Invocation

C benchmarks:

icc -m64 -std=c11

C++ benchmarks:

icpc -m64

Fortran benchmarks:

ifort -m64

Benchmarks using both Fortran and C:

ifort -m64 icc -m64 -std=c11

Benchmarks using both C and C++:

icpc -m64 icc -m64 -std=c11

Benchmarks using Fortran, C, and C++:

icpc -m64 icc -m64 -std=c11 ifort -m64

Peak Portability Flags

Same as Base Portability Flags

Peak Optimization Flags

C benchmarks:

-prof-gen(pass 1) -prof-use(pass 2) -xCORE-AVX2 -ipo -O3
-no-prec-div -auto-p32 -qopt-prefetch -qopt-mem-layout-trans=3

C++ benchmarks:

-Wl,-z,muldefs -prof-gen(pass 1) -prof-use(pass 2) -xCORE-AVX2 -ipo

(Continued on next page)

Page 11 Standard Performance Evaluation Corporation (info@spec.org) https://www.spec.org/ spec^® SPEC CPU

®2017 Floating Point Rate Result

Copyright 2017-2020 Standard Performance Evaluation Corporation

(Test Sponsor: HPE)

Hewlett Packard Enterprise

(2.40 GHz, Intel Xeon E5-2699A v4)

ProLiant DL380 Gen9 SPECrate®2017_fp_peak = 148

SPECrate^®2017_fp_base = 147

CPU2017 License: 3 Test Date: Dec-2016 Test Sponsor: HPE Hardware Availability: Oct-2016 Tested by: HPE Software Availability: Sep-2016

Peak Optimization Flags (Continued)

C++ benchmarks (continued):

-O3 -no-prec-div -auto-p32 -qopt-prefetch -qopt-mem-layout-trans=3
-L/sh10.2 -lsmartheap64

Fortran benchmarks:

-prof-gen(pass 1) -prof-use(pass 2) -xCORE-AVX2 -ipo -O3
-no-prec-div -qopt-prefetch -qopt-mem-layout-trans=3
-nostandard-realloc-lhs

Benchmarks using both Fortran and C:

-prof-gen(pass 1) -prof-use(pass 2) -xCORE-AVX2 -ipo -O3
-no-prec-div -auto-p32 -qopt-prefetch -qopt-mem-layout-trans=3
-nostandard-realloc-lhs

Benchmarks using both C and C++:

-Wl,-z,muldefs -prof-gen(pass 1) -prof-use(pass 2) -xCORE-AVX2 -ipo
-O3 -no-prec-div -auto-p32 -qopt-prefetch -qopt-mem-layout-trans=3
-L/sh10.2 -lsmartheap64

Benchmarks using Fortran, C, and C++:

-Wl,-z,muldefs -prof-gen(pass 1) -prof-use(pass 2) -xCORE-AVX2 -ipo
-O3 -no-prec-div -auto-p32 -qopt-prefetch -qopt-mem-layout-trans=3
-nostandard-realloc-lhs -L/sh10.2 -lsmartheap64

The flags files that were used to format this result can be browsed at

http://www.spec.org/cpu2017/flags/Intel-ic17.0-official-linux64-revD.html
http://www.spec.org/cpu2017/flags/HP-Platform-Flags-Intel-V1.2-HSW-revE.html

You can also download the XML flags sources by saving the following links:

http://www.spec.org/cpu2017/flags/Intel-ic17.0-official-linux64-revD.xml
http://www.spec.org/cpu2017/flags/HP-Platform-Flags-Intel-V1.2-HSW-revE.xml

Originally published on 2017-06-19.

Report generated on 2020-02-06 17:18:03 by CPU2017 PS formatter v6255.

Tested with SPEC CPU^®2017 v0.904.0 on 2016-12-09 13:58:28-0500.

For questions about this result, please contact the tester. For other inquiries, please contact info@spec.org.

names appearing in this result are trademarks or registered trademarks of their respective holders.

SPEC CPU and SPECrate are registered trademarks of the Standard Performance Evaluation Corporation. All other brand and product