### System parameters on server driver1

###

###

###

    # sysctl settings are defined through files in
    # /usr/lib/sysctl.d/, /run/sysctl.d/, and /etc/sysctl.d/.
    #
    # Vendors settings live in /usr/lib/sysctl.d/.
    # To override a whole file, create a new file with the same in
    # /etc/sysctl.d/ and put new settings there. To override
    # only specific settings, add a file with a lexically later
    # name in /etc/sysctl.d/ and put new settings there.
    #
    # For more information, see sysctl.conf(5) and sysctl.d(5).
    net.ipv4.icmp_echo_ignore_broadcasts = 1
      net.ipv4.conf.all.rp_filter = 1
      fs.inotify.max_user_watches = 65536
      net.ipv4.conf.default.promote_secondaries = 1
      net.ipv4.conf.all.promote_secondaries = 1
      fs.file-max = 1048576
      kernel.sem = 250 32000 100 128
      kernel.shmall = 4294967296
      kernel.shmmax = 68719476736
      net.core.optmem_max = 30000000
      net.core.rmem_default = 30000000
      net.core.wmem_default = 30000000
      net.ipv4.conf.all.arp_announce = 2
      net.ipv4.conf.all.arp_ignore = 1
      net.ipv4.conf.default.rp_filter = 1
      net.ipv4.conf.default.accept_source_route = 0
      net.ipv4.ip_forward = 0
      net.ipv4.ip_local_port_range = 1024 65000
      net.ipv4.tcp_max_syn_backlog = 30000
      net.ipv4.tcp_max_tw_buckets = 2000000
      net.ipv4.tcp_mem  = 30000000 30000000 30000000
      kernel.sched_compat_yield = 1
      net.core.somaxconn = 32767
      net.core.netdev_max_backlog = 250000
      net.ipv4.tcp_fin_timeout = 30
      net.ipv4.tcp_keepalive_intvl = 15
      net.ipv4.tcp_keepalive_probes = 5
      net.core.rmem_max = 32554432
      net.core.wmem_max = 32554432
      net.ipv4.tcp_rmem = 20480 174760 32554432
      net.ipv4.tcp_wmem = 20480 174760 32554432
      net.ipv4.tcp_window_scaling = 1
      net.ipv4.tcp_timestamps = 1
      net.ipv4.tcp_sack = 1
      net.ipv4.tcp_no_metrics_save = 1
      kernel.pid_max = 229376

            Processor info for server driver1

    processor	: 0
    cpu		: POWER8 (architected), altivec supported
    processor	: 1
    cpu		: POWER8 (architected), altivec supported
    processor	: 2
    cpu		: POWER8 (architected), altivec supported
    processor	: 3
    cpu		: POWER8 (architected), altivec supported
    processor	: 4
    cpu		: POWER8 (architected), altivec supported
    processor	: 5
    cpu		: POWER8 (architected), altivec supported
    processor	: 6
    cpu		: POWER8 (architected), altivec supported
    processor	: 7
    cpu		: POWER8 (architected), altivec supported
    processor	: 8
    cpu		: POWER8 (architected), altivec supported
    processor	: 9
    cpu		: POWER8 (architected), altivec supported
    processor	: 10
    cpu		: POWER8 (architected), altivec supported
    processor	: 11
    cpu		: POWER8 (architected), altivec supported
    processor	: 12
    cpu		: POWER8 (architected), altivec supported
    processor	: 13
    cpu		: POWER8 (architected), altivec supported
    processor	: 14
    cpu		: POWER8 (architected), altivec supported
    processor	: 15
    cpu		: POWER8 (architected), altivec supported
    processor	: 16
    cpu		: POWER8 (architected), altivec supported
    processor	: 17
    cpu		: POWER8 (architected), altivec supported
    processor	: 18
    cpu		: POWER8 (architected), altivec supported
    processor	: 19
    cpu		: POWER8 (architected), altivec supported
    processor	: 20
    cpu		: POWER8 (architected), altivec supported
    processor	: 21
    cpu		: POWER8 (architected), altivec supported
    processor	: 22
    cpu		: POWER8 (architected), altivec supported
    processor	: 23
    cpu		: POWER8 (architected), altivec supported
    processor	: 24
    cpu		: POWER8 (architected), altivec supported
    processor	: 25
    cpu		: POWER8 (architected), altivec supported
    processor	: 26
    cpu		: POWER8 (architected), altivec supported
    processor	: 27
    cpu		: POWER8 (architected), altivec supported
    processor	: 28
    cpu		: POWER8 (architected), altivec supported
    processor	: 29
    cpu		: POWER8 (architected), altivec supported
    processor	: 30
    cpu		: POWER8 (architected), altivec supported
    processor	: 31
    cpu		: POWER8 (architected), altivec supported
    processor	: 32
    cpu		: POWER8 (architected), altivec supported
    processor	: 33
    cpu		: POWER8 (architected), altivec supported
    processor	: 34
    cpu		: POWER8 (architected), altivec supported
    processor	: 35
    cpu		: POWER8 (architected), altivec supported
    processor	: 36
    cpu		: POWER8 (architected), altivec supported
    processor	: 37
    cpu		: POWER8 (architected), altivec supported
    processor	: 38
    cpu		: POWER8 (architected), altivec supported
    processor	: 39
    cpu		: POWER8 (architected), altivec supported
    processor	: 40
    cpu		: POWER8 (architected), altivec supported
    processor	: 41
    cpu		: POWER8 (architected), altivec supported
    processor	: 42
    cpu		: POWER8 (architected), altivec supported
    processor	: 43
    cpu		: POWER8 (architected), altivec supported
    processor	: 44
    cpu		: POWER8 (architected), altivec supported
    processor	: 45
    cpu		: POWER8 (architected), altivec supported
    processor	: 46
    cpu		: POWER8 (architected), altivec supported
    processor	: 47
    cpu		: POWER8 (architected), altivec supported
    processor	: 48
    cpu		: POWER8 (architected), altivec supported
    processor	: 49
    cpu		: POWER8 (architected), altivec supported
    processor	: 50
    cpu		: POWER8 (architected), altivec supported
    processor	: 51
    cpu		: POWER8 (architected), altivec supported
    processor	: 52
    cpu		: POWER8 (architected), altivec supported
    processor	: 53
    cpu		: POWER8 (architected), altivec supported
    processor	: 54
    cpu		: POWER8 (architected), altivec supported
    processor	: 55
    cpu		: POWER8 (architected), altivec supported
    processor	: 56
    cpu		: POWER8 (architected), altivec supported
    processor	: 57
    cpu		: POWER8 (architected), altivec supported
    processor	: 58
    cpu		: POWER8 (architected), altivec supported
    processor	: 59
    cpu		: POWER8 (architected), altivec supported
    processor	: 60
    cpu		: POWER8 (architected), altivec supported
    processor	: 61
    cpu		: POWER8 (architected), altivec supported
    processor	: 62
    cpu		: POWER8 (architected), altivec supported
    processor	: 63
    cpu		: POWER8 (architected), altivec supported
    processor	: 64
    cpu		: POWER8 (architected), altivec supported
    processor	: 65
    cpu		: POWER8 (architected), altivec supported
    processor	: 66
    cpu		: POWER8 (architected), altivec supported
    processor	: 67
    cpu		: POWER8 (architected), altivec supported
    processor	: 68
    cpu		: POWER8 (architected), altivec supported
    processor	: 69
    cpu		: POWER8 (architected), altivec supported
    processor	: 70
    cpu		: POWER8 (architected), altivec supported
    processor	: 71
    cpu		: POWER8 (architected), altivec supported
    processor	: 72
    cpu		: POWER8 (architected), altivec supported
    processor	: 73
    cpu		: POWER8 (architected), altivec supported
    processor	: 74
    cpu		: POWER8 (architected), altivec supported
    processor	: 75
    cpu		: POWER8 (architected), altivec supported
    processor	: 76
    cpu		: POWER8 (architected), altivec supported
    processor	: 77
    cpu		: POWER8 (architected), altivec supported
    processor	: 78
    cpu		: POWER8 (architected), altivec supported
    processor	: 79
    cpu		: POWER8 (architected), altivec supported
    model		: IBM,8286-42A

            Memory info for server driver1

    MemTotal:       49193856 kB
    MemFree:        46376832 kB
    MemAvailable:   46091392 kB
    SwapCached:            0 kB
    SwapTotal:       4194240 kB
    SwapFree:        4194240 kB

            Kernel on server driver1

    Linux 3.10.0-693.el7.ppc64le #1 SMP Thu Jul 6 19:59:44 EDT 2017 ppc64le