For more Information Contact

SPEC info@spec.org http://www.spec.org

SPECweb99 Result

© Copyright 1999, Standard Performance Evaluation Corporation

Compaq Computer Corp.: Alphaserver DS20 6/667

Zeus Ltd: Zeus 3.3.5

SPECweb99 = 1050

Test Date: Tester:

Feb-2000 Compaq

Hardware Avail: Apr-2000 OS Avail: Apr-1999 HTTP Software Avail: Feb-2000 Sup. Software Avail: Apr-1999 SPEC license #: 2

Hardware

Vendor: Compaq Computer Corp. Model: Alphaserver DS20 6/667 Processor: 667 MHz 21264A # Processors: 2 cores, 2 chips, 1 core/chip Primary Cache: 64KB(I)+64KB(D) on chip Secondary Cache: 8MB off chip Other Cache: none Memory: 2 GB Disk Subsystem:^{3x4GB(RZ1CF-CF), 3x9GB(RZ1DB-CS)} Disk Controllers: Integral FW SCSI Other Hardware:^{2 x ALTEON ACEswitch 180 GbE Switch}

Software

Operating System: Compaq Tru64 UNIX V4.0F File System: UFS and AdvFS Other Software: none

HTTP Software

Vendor: Zeus Ltd HTTP Software: Zeus 3.3.5 API: ISAPI Server Cache: none Log Mode: Common Log Format

Test Sponsor

Test Date: Feb-2000 Tested By: Compaq SPEC License: 2

Network

# of Controllers: 2 Network Controllers: 2 x DEGPA-SA # of Nets: 2 Type of Nets: Gigabit Ethernet Network Speed: 1000Mbit MSL (sec): 30 (Non RFC1122) Time-Wait (sec): 60 (Non RFC1122) MTU: 1500

Clients

# of Clients: 10 Model: Digital Personal WorkStation 600au Processor: 600MHz 21164 # of Processors: 1 Memory: 1GB Network Controller: DEGPA-SA Operating System: Compaq Tru64 UNIX V4.0F Compiler: DEC C V5.9-005

Notes/Tuning Information

SUT Notes

Operating System Notes

OS Tuning parameters: proc:

maxusers = 2048 max-proc-per-user = 0 max-threads-per-user = 1024 per-proc-data-size = 0x40000000000 max-per-proc-data-size = 0x40000000000 max-per-proc-address-space = 0x40000000000 per-proc-address-space = 0x40000000000 socket:

sominconn = 32765 somaxconn = 32765 umc = 1 inet:

ipqs = 10 tcbhashnum = 10 tcbhashsize = 8192 tcp_sendspace = 60000 tcp_recvspace = 60000 ipqmaxlen=2000 vm: ubc-maxpercent = 60 vm-mapentries = 50000

For more Information Contact

SPEC info@spec.org http://www.spec.org

SPECweb99 Result

© Copyright 1999, Standard Performance Evaluation Corporation

Notes/Tuning Information (Continued)

Operating System Notes (Continued)

vm-vpagemax = 131072 vm-maxvas = 0x40000000000

vfs:

name-cache-hash-size = 8192 namei-cache-valid-time = 8400 advfs:

AdvfsCacheMaxPercent = 25 AdvfsCacheHashSize = 32768

AdvfsPreallocAccess = 32768

net:

netisrthreads=2 netisrwakeupthreshold=192

HTTP Software Notes

Zeus 3.3.5 Tuning runningsites/&lt;host&gt;: bindaddr text 16.45.205.151,16.49.209.151 global.cfg:

tuning!bind_any yes tuning!cache_files 37097 tuning!cache_flush_interval 9000 tuning!cache_large_file 1048576 tuning!cache_max_bytes 0 tuning!cache_small_file 102 tuning!cache_stat_expire 86400 tuning!num_children 3 tuning!so_wbuff_size 1048576 tuning!softservers no tuning!unique_bind no tuning!use_poll no

Hardware Notes

Disk Configuration:

disk1: OS and swap (/, /usr, swap) disk2: URLroot (/www) disk3 & disk4: file_set (/www/file_set) [AdvFS Domain] disk5 & disk6: http logging (/log) [lsm stripeset]

Network Notes

Network Tuning: N/A

Client Notes

proc:

maxusers = 1024 max-proc-per-user = 0 max-threads-per-user = 1024 socket:

sominconn = 32765 somaxconn = 32765 inet:

ipport_userreserved = 65000 tcp_recvspace = 60000 ipqmaxlen=2000

For more Information Contact

SPEC info@spec.org http://www.spec.org

SPECweb99 Result

© Copyright 1999, Standard Performance Evaluation Corporation

Notes/Tuning Information (Continued)

Client Notes (Continued)

tcbhashsize=8192