For more Information Contact

SPEC info@spec.org http://www.spec.org

SPECweb99_SSL Result

© Copyright 1999-2004, Standard Performance Evaluation Corporation

Hewlett-Packard Company: hp server rx5670 Zeus Technology Ltd: Zeus 4.1r4

SPECweb99_SSL =1498

Test Date: Tester:

Aug-2002 Hewlett-Packard Company

Hardware Avail: Aug-2002 OS Avail: Oct-2002 HTTPS Software Avail: Aug-2002 Sup. Software Avail: Aug-2002 SPEC license #: 3

Hardware

Vendor: Hewlett-Packard Company Model: hp server rx5670 Processor: 1 GHz Intel Itanium 2 # Processors: 4 cores, 4 chips, 1 core/chip Primary Cache: 16KBI+16KBD on chip Secondary Cache: 256KB unified on chip Other Cache: 3072KB unified on chip Memory: 12 GB Disk Subsystem: 4 18GB 15K Ultra3 SCSI Disk Controllers: Integrated Ultra3 SCSI Other Hardware: None

Software

Operating System: Red Hat Linux Advanced Server 2.1 File System: ext2 Other Software: None

HTTPS Software

Vendor: Zeus Technology Ltd HTTPS Software: Zeus 4.1r4 API: ISAPI Server Cache: None Log Mode: Binary Log Format

Test Sponsor

Test Date: Aug-2002 Tested By: Hewlett-Packard Company SPEC License: 3

Network

# of Controllers: 2 Network Controllers: 2 Integrated Broadcom NetXtreme GB Nic # of Nets: 2 Type of Nets: Gigabit Ethernet Network Speed: 1 Gb/s MSL (sec): 30 (Non RFC1122) Time-Wait (sec): 60 (Non RFC1122) MTU: 1500

Clients

# of Clients: 14 Model: HP Kayak XU Processor: Intel Pentium II at 550MHz # of Processors: 2 Memory: 256MB Network Controller: Alteon ACENIC 1000SX Operating System: Red Hat Linux 7.2 Compiler: gcc 2.96

Notes/Tuning Information

Operating System Notes

Tuning parameters:

/proc/sys/fs/file-max = 200000,maximum number of open files, default 1024 /proc/sys/net/core/rmem_max= 1048576,maximum receive socket buffer size, default 65535 /proc/sys/net/core/wmem_max= 1048576,maximum send socket buffer size, default 65535 /proc/sys/net/core/rmem_default= 1048576,default receive socket buffer size, default 65535 /proc/sys/net/ipv4/ip_local_port_range= 16384 65536,local port range for TCP and UDP,default 1024 4999 /proc/sys/net/core/wmem_default= 10485760,default send socket buffer size, default 65535 txqueuelen=20000, transmit queue length, default 100 Red Hat Linux Version: 2.4.17-4hpmckinleysmp

HTTPS Software Notes

Zeus Global Parameters: tuning!cache_files 356750 tuning!cache_max_bytes 0 tuning!cache_small_file 0 tuning!cache_large_file 1000000 tuning!cache_stat_expire 86400 tuning!cache_flush_interval 86400 tuning!listen_queue_size 8192 tuning!multiple_accept yes tuning!so_rbuff_size 0 tuning!so_wbuff_size 1048576 tuning!cbuff_size 65536 tuning!keepalive yes tuning!keepalive_timeout 1200

For more Information Contact

SPEC info@spec.org http://www.spec.org

SPECweb99_SSL Result

© Copyright 1999-2004, Standard Performance Evaluation Corporation

Notes/Tuning Information (Continued)

HTTPS Software Notes (Continued)

tuning!keepalive_max -1 tuning!timeout 600 tuning!unique_bind yes tuning!bind_any no tuning!sendfile no tuning!modules!cgi!cbuff_size 1048576 tuning!modules!cgi!cleansize 0 tuning!ssl_keepalive yes tuning!ssl_sessioncache_size 256 tuning!ssl_diskcache no tuning!softservers no tuning!use_poll no tuning!modules!stats!enabled no tuning!modules!nsapi!enabled no tuning!modules!isapi!enabled yes tuning!cache_cooling_time 0 tuning!maxaccept 1024 tuning!num_children 4

HTTP API Notes

Zeus ISAPI interface used Zeus PEPP Toolkit(0.6) used for SPECweb99_SSL dynamic content Intel(R) C++ Itanium(TM) Compiler for Itanium(TM)-based applications, Version 6.2 ./Configure --sendfile=no --checkconfig=yes --locking=semop --ssl=yes --64bit=yes

Hardware Notes

One 18GB 15K RPM disk for OS,paging Log, 3 18GB 15K for file set.

Other Notes

Tuning Disclosure: HP-20020724.txt Dynamic API: HP-20020724-API.tgz