Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

Hewlett-Packard Company

ProLiant DL380 G3 (3.2GHz/2MB L3 cache, Intel Xeon)

SPECfp2000 = SPECfp_base2000 =

1349 1318

SPEC license #: 3 Tested by: Hewlett-Packard Company Test date: Apr-2004 Hardware Avail: Feb-2004 Software Avail: Mar-2004

Benchmark

Reference

Time

Base Runtime

Base Ratio Runtime Ratio 1000 2000 3000 4000

168.wupwise 1600 106 1505 104 1535

171.swim 3100 185 1676 180 1719

172.mgrid 1800 156 1153 156 1157

173.applu 2100 187 1121 180 1169

177.mesa 1400 100 1394 100 1394

178.galgel 2900 109 2672 108 2682

179.art 2600 140 1860 118 2196

183.equake 1300 107 1220 106 1231

187.facerec 1900 130 1463 128 1488

188.ammp 2200 195 1129 195 1129

189.lucas 2000 140 1433 136 1474

191.fma3d 2100 190 1104 190 1104

200.sixtrack 1100 178 619 177 623

301.apsi 2600 243 1068 243 1072

Hardware

CPU: Intel Xeon (3.2GHz, 533MHz bus) CPU MHz: 3200 FPU: Integrated CPU(s) enabled: 1 core, 1 chip, 1 core/chip (HT Technology disabled) CPU(s) orderable: 1,2 Parallel: No Primary Cache: 12K micro-ops I + 8KBD on chip Secondary Cache: 512KB(I+D) on chip L3 Cache: 2048KB(I+D) on chip Other Cache: N/A Memory: 4x512MB PC2100 Disk Subsystem: 1x36.4GB 15K Ultra320 SCSI Other Hardware:

Software

Operating System: Windows Server 2003 Standard (Build 3790) Compiler: Intel C++ Compiler 8.0 Build 20031211Z

Intel Fortran Compiler 8.0 build 20040125Z Microsoft Visual Studio .NET 7.0.9466 (for libraries) MicroQuill Smartheap Library 7.0

File System: NTFS System State: Default

Notes/Tuning Information

 +FDO: PASS1=-Qprof_gen  PASS2=-Qprof_use
 Base tuning for all programs: -QxN -Qipo -O3 +FDO ONESTEP=yes
 Portability flags:
   178.galgel: -FI /F32000000
 Peak tuning:
   168.wupwise:    -Qipo -QxN  +FDO ONESTEP=yes
   171.swim:       -Qipo -QxN  -O3 +FDO ONESTEP=yes
   172.mgrid:      -Qipo -QaxN -O3 +FDO ONESTEP=yes
   173.applu:      -Qipo -QxN  -O3 -Qscalar_rep- -Qauto +FDO ONESTEP=yes
   177.mesa:       -Qipo -QxN  -O3 +FDO ONESTEP=yes
   178.galgel:     -Qipo -QxN  -O3 +FDO ONESTEP=yes
   179.art:        -Qipo -Oa -Qunroll4 -Zp4 ONESTEP=yes
   183.equake:     -Qipo -QxN  -Oa -Qrcd +FDO shlw32M.lib ONESTEP=yes
   187.facerec:    -Qipo -QaxN  -O3 -Qunroll1 -Qscalar_rep- +FDO ONESTEP=yes
   188.ammp:       basepeak=1
   189.lucas:      -Qipo -QaxN
   191.fma3d:      basepeak=1

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

Hewlett-Packard Company

ProLiant DL380 G3 (3.2GHz/2MB L3 cache, Intel Xeon)

SPECfp2000 = SPECfp_base2000 =

1349 1318

SPEC license #: 3 Tested by: Hewlett-Packard Company Test date: Apr-2004 Hardware Avail: Feb-2004 Software Avail: Mar-2004

Notes/Tuning Information (Continued)

   200.sixtrack:   -Qipo -QxN  +FDO ONESTEP=yes
   301.apsi:       -Qipo -QxN  -O3 +FDO ONESTEP=yes
 BIOS Configuration Notes
   HT Technology disabled