Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

ION Computer Systems

SR1325TP (3.4GHz Pentium 4 processor with HT Technology Extreme Edition)

SPECfp2000 = SPECfp_base2000 =

1524 1524

SPEC license #: 2697 Tested by: ION Test date: Apr-2004 Hardware Avail: May-2004 Software Avail: Apr-2004

Benchmark

Reference

Time

Base Runtime

Base Ratio Runtime Ratio 1000 2000 3000 4000

168.wupwise 1600 89.4 1790 89.4 1790

171.swim 3100 142 2190 142 2190

172.mgrid 1800 137 1312 137 1312

173.applu 2100 147 1425 147 1425

177.mesa 1400 88.8 1576 88.8 1576

178.galgel 2900 94.6 3065 94.6 3065

179.art 2600 123 2110 123 2110

183.equake 1300 75.8 1715 75.6 1720

187.facerec 1900 105 1816 105 1816

188.ammp 2200 222 992 221 994

189.lucas 2000 120 1662 120 1662

191.fma3d 2100 161 1307 161 1307

200.sixtrack 1100 168 653 168 653

301.apsi 2600 235 1108 235 1108

Hardware

CPU: Intel Pentium 4 processor with HT Technology Extreme Edition, 3.4GHz, 800MHz bus CPU MHz: 3392 FPU: Integrated CPU(s) enabled: 1 core, 1 chip, 1 core/chip, HT Technology disabled CPU(s) orderable: 1 Parallel: No Primary Cache: 12K(I) micro-ops + 8KB(D) on chip Secondary Cache: 512KB (I+D) on chip L3 Cache: 2048KB (I+D) on chip Other Cache: None Memory: 2 GB DDR400, 3-3-3, (4x512GB DIMMs) Disk Subsystem: 1x 200GB IDE, 7200rpm Other Hardware: None

Software

Operating System: Red Hat Enterprise Linux ES release 3 Compiler: Intel(R) Fortran Compiler for Linux 8.0 (Build 20040412Z)

Intel(R) C++ Compiler for Linux 8.0 (Build 20040412Z) MicroQuill SmartHeap Library 7.1 (www.microquill.com)

File System: ext2 System State: Multi-user, 2.4.21 up kernel

Notes/Tuning Information

 Hyper Threading Technology disabled in BIOS

 Baseline optimization flags:
       C programs: PASS1= -xN -prof_gen PASS2= -xN -fast -prof_use
 Fortran programs: PASS1= -xN -prof_gen PASS2= -xN -ipo -O3 -prof_use

 FP Peak optimization flags:
      168.wupwise: basepeak=yes
         171.swim: basepeak=yes
         72.mgrid:basepeak=yes
        173.applu: basepeak=yes
         177.mesa: basepeak=yes
       178.galgel: basepeak=yes
          179.art: basepeak=yes
       183.equake: PASS1= -xN -prof_gen PASS2= -xN -fast -Oa -prof_use

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

ION Computer Systems

SR1325TP (3.4GHz Pentium 4 processor with HT Technology Extreme Edition)

SPECfp2000 = SPECfp_base2000 =

1524 1524

SPEC license #: 2697 Tested by: ION Test date: Apr-2004 Hardware Avail: May-2004 Software Avail: Apr-2004

Notes/Tuning Information (Continued)

      187.facerec: basepeak=yes
         188.ammp: PASS1= -xW -prof_gen PASS2= -xW -fast -prof_use
        189.lucas: basepeak=yes
        191.fma3d: basepeak=yes
     200.sixtrack: basepeak=yes
         301.apsi: basepeak=yes

 FP Portability Flags:
       178.galgel:  -FI