Standard Performance Evaluation Corporation info@spec.org http://www.spec.org/

Page 1 spec^® SPEC

® CINT2006 Result

Copyright 2006-2014 Standard Performance Evaluation Corporation

Oracle Corporation

Sun Blade X6270 M2 (Intel Xeon X5680 3.33GHz)

SPECint^®_rate2006 = 369

SPECint_rate_base2006 = 337

CPU2006 license: 6 Test date: Mar-2010 Test sponsor: Oracle Corporation Hardware Availability: Jun-2010 Tested by: Oracle Corporation Software Availability: Jun-2010

400.perlbench

401.bzip2

403.gcc

429.mcf

445.gobmk

456.hmmer

458.sjeng

462.libquantum

464.h264ref

471.omnetpp

473.astar

483.xalancbmk

Copies

SPECint_rate2006 = 369

SPECint_rate_base2006 = 337

0 920

30.0 70.0 100 130 160 190 220 250 280 310 340 370 400 430 460 490 520 550 580 610 640 670 700 730 760 790 820 850 880 24 331 24 406

24 218 24 238

24 205 24 209

24 377 24 385

24 357 24 416

24 368 24 513

24 350 24 383

24 889 24 912

24 472 24 506

24 227 24 238

24 231

24 375 24 392

Hardware

CPU Name: Intel Xeon X5680 CPU Characteristics: Intel Turbo Boost Technology up to 3.60 GHz CPU MHz: 3333 FPU: Integrated CPU(s) enabled: 12 cores, 2 chips, 6 cores/chip, 2 threads/core CPU(s) orderable: 1 or 2 chips Primary Cache: 32 KB I + 32 KB D on chip per core Secondary Cache: 256 KB I+D on chip per core L3 Cache: 12 MB I+D on chip per chip Other Cache: None Memory: 48 GB (12 x 4 GB DDR3-1333 CL9, 2 Rank, ECC) Disk Subsystem: 1 x 300 GB, SAS, 10000 RPM Other Hardware: None

Software

Operating System: Oracle Solaris 10 10/09 Compiler: Oracle Solaris Studio Express 6/10 Auto Parallel: No File System: ufs System State: Default Base Pointers: 32-bit Peak Pointers: 32/64-bit Other Software: MicroQuill SmartHeap Library 9.01 for x64

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org/

Page 2 spec^® SPEC CINT2006 Result

Copyright 2006-2014 Standard Performance Evaluation Corporation

Oracle Corporation

Sun Blade X6270 M2 (Intel Xeon X5680 3.33GHz)

SPECint_rate2006 = 369 SPECint_rate_base2006 = 337

CPU2006 license: 6 Test date: Mar-2010 Test sponsor: Oracle Corporation Hardware Availability: Jun-2010 Tested by: Oracle Corporation Software Availability: Jun-2010

Results Table

Benchmark Copies Seconds Ratio Seconds Ratio Seconds Ratio

Base Copies Seconds Ratio Seconds Ratio Seconds Ratio

Peak

400.perlbench 24 721 325 708 331 707 332 24 585 400 577 406 577 406 401.bzip2 24 1056 219 1062 218 1069 217 24 969 239 973 238 973 238 403.gcc 24 960 201 944 205 943 205 24 920 210 941 205 922 209 429.mcf 24 580 377 579 378 582 376 24 565 387 569 385 569 385 445.gobmk 24 703 358 705 357 714 352 24 602 418 605 416 606 416 456.hmmer 24 607 369 609 368 614 365 24 437 513 437 513 437 513 458.sjeng 24 829 350 830 350 829 350 24 757 384 757 383 757 383 462.libquantum 24 560 889 560 888 559 889 24 545 912 545 912 545 912 464.h264ref 24 1098 484 1133 469 1125 472 24 1034 513 1140 466 1049 506 471.omnetpp 24 662 227 662 227 662 226 24 629 238 629 239 629 238 473.astar 24 731 230 729 231 730 231 24 731 230 729 231 730 231 483.xalancbmk 24 441 375 441 375 442 374 24 421 393 425 390 423 392

Results appear in the order in which they were run. Bold underlined text indicates a median measurement.

Submit Notes

The config file option ’submit’ was used.

Operating System Notes

 ulimit -s unlimited  (shell)
 /etc/system parameters
    tune_t_fsflushr=10
    autoup=900

Platform Notes

   Default BIOS settings used except:
     C-State                 : Disabled
     Data Reuse Optimization : Disabled

Base Compiler Invocation

C benchmarks:

cc

C++ benchmarks:

CC

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org/

Page 3 spec^® SPEC CINT2006 Result

Copyright 2006-2014 Standard Performance Evaluation Corporation

Oracle Corporation

Sun Blade X6270 M2 (Intel Xeon X5680 3.33GHz)

SPECint_rate2006 = 369

SPECint_rate_base2006 = 337

CPU2006 license: 6 Test date: Mar-2010 Test sponsor: Oracle Corporation Hardware Availability: Jun-2010 Tested by: Oracle Corporation Software Availability: Jun-2010

Base Portability Flags

400.perlbench: -DSPEC_CPU_SOLARIS_IA32

403.gcc: -DSPEC_CPU_SOLARIS 462.libquantum: -DSPEC_CPU_SOLARIS 483.xalancbmk: -DSPEC_CPU_SOLARIS

Base Optimization Flags

C benchmarks:

-fast -xtarget=nehalem -xipo=2 -xpagesize=2M
-M /usr/lib/ld/map.bssalign

C++ benchmarks:

-fast -xtarget=nehalem -xipo=2 -xpagesize=2M -xvector=simd
-xalias_level=compatible
-L/data1/SmartHeap_9/lib -R/data1/SmartHeap_9/lib -lsmartheap
-library=stlport4

Base Other Flags

C benchmarks:

-V -# -xjobs=24

C++ benchmarks:

-verbose=diags,version -xjobs=24

Peak Compiler Invocation

C benchmarks:

cc

C++ benchmarks:

CC

Peak Portability Flags

400.perlbench: -DSPEC_CPU_SOLARIS_X64 -DSPEC_CPU_LP64

403.gcc: -DSPEC_CPU_SOLARIS 462.libquantum: -DSPEC_CPU_SOLARIS 483.xalancbmk: -DSPEC_CPU_SOLARIS

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org/

Page 4 spec^® SPEC CINT2006 Result

Copyright 2006-2014 Standard Performance Evaluation Corporation

Oracle Corporation

Sun Blade X6270 M2 (Intel Xeon X5680 3.33GHz)

SPECint_rate2006 = 369

SPECint_rate_base2006 = 337

CPU2006 license: 6 Test date: Mar-2010 Test sponsor: Oracle Corporation Hardware Availability: Jun-2010 Tested by: Oracle Corporation Software Availability: Jun-2010

Peak Optimization Flags

C benchmarks:

400.perlbench: -xprofile=collect:./feedback(pass 1)

-xprofile=use:./feedback(pass 2) -fast -xtarget=nehalem
-xipo=1 -m64 -xalias_level=std -lbsdmalloc -lumem

401.bzip2: -fast -xtarget=nehalem -xipo=2 -m64 -xpagesize=2M

-xalias_level=std -lumem

403.gcc: -xprofile=collect:./feedback(pass 1)

-xprofile=use:./feedback(pass 2) -fast -xtarget=nehalem
-xipo=2 -xpagesize=2M -W2,-Rujam -W2,-Rtile

429.mcf: -xprofile=collect:./feedback(pass 1)

-xprofile=use:./feedback(pass 2) -fast -xtarget=nehalem
-xipo=2 -m32 -xpagesize=2M -xalias_level=strong
-xprefetch=no%auto -lbsdmalloc

445.gobmk: -xprofile=collect:./feedback(pass 1)

-xprofile=use:./feedback(pass 2) -fast -xtarget=nehalem
-m64 -xpagesize=2M -xrestrict -xalias_level=strong
-xdepend

456.hmmer: -xprofile=collect:./feedback(pass 1)

-xprofile=use:./feedback(pass 2) -fast -xtarget=nehalem
-xipo=2 -m64

458.sjeng: -xprofile=collect:./feedback(pass 1)

-xprofile=use:./feedback(pass 2) -fast -xtarget=nehalem
-xipo=2 -m64 -xpagesize=2M -xalias_level=strong

462.libquantum: -fast -xtarget=nehalem -xipo=2 -m64 -xalias_level=std

464.h264ref: -xprofile=collect:./feedback(pass 1)

-xprofile=use:./feedback(pass 2) -fast -xtarget=nehalem
-xipo=2 -m64 -xalias_level=strong -xrestrict

C++ benchmarks:

471.omnetpp: -xprofile=collect:./feedback(pass 1)

-xprofile=use:./feedback(pass 2) -fast -xtarget=nehalem
-xipo=2 -xpagesize=2M -library=stlport4
-L/data1/SmartHeap_9/lib -R/data1/SmartHeap_9/lib -lsmartheap

473.astar: basepeak = yes

483.xalancbmk: -xprofile=collect:./feedback(pass 1)

-xprofile=use:./feedback(pass 2) -fast -xtarget=nehalem
-xipo=2 -xunroll=2 -xpagesize=2M -xalias_level=compatible
-L/data1/SmartHeap_9/lib -R/data1/SmartHeap_9/lib -lsmartheap
-library=stlport4

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org/

Page 5 spec^® SPEC CINT2006 Result

Copyright 2006-2014 Standard Performance Evaluation Corporation

Oracle Corporation

Sun Blade X6270 M2 (Intel Xeon X5680 3.33GHz)

SPECint_rate2006 = 369 SPECint_rate_base2006 = 337

CPU2006 license: 6 Test date: Mar-2010 Test sponsor: Oracle Corporation Hardware Availability: Jun-2010 Tested by: Oracle Corporation Software Availability: Jun-2010

Peak Other Flags

C benchmarks:

-V -# -xjobs=24

C++ benchmarks:

-verbose=diags,version -xjobs=24

The flags file that was used to format this result can be browsed at

http://www.spec.org/cpu2006/flags/Oracle-Solaris-Studio-x86_64.html

You can also download the XML flags source by saving the following link:

http://www.spec.org/cpu2006/flags/Oracle-Solaris-Studio-x86_64.xml

Originally published on 8 July 2010.

Report generated on Wed Jul 23 13:23:18 2014 by SPEC CPU2006 PS/PDF formatter v6932.

Tested with SPEC CPU2006 v1.1.

For other inquiries, please contact webmaster@spec.org.

For questions about this result, please contact the tester.

holders.

this result are trademarks or registered trademarks of their respective

Evaluation Corporation. All other brand and product names appearing in

SPEC and SPECint are registered trademarks of the Standard Performance