Standard Performance Evaluation Corporation info@spec.org http://www.spec.org/

Page 1 spec^® SPEC

® CINT2006 Result

Copyright 2006-2014 Standard Performance Evaluation Corporation

Oracle Corporation SPARC T3-4

SPECint^®_rate2006 = 666

SPECint_rate_base2006 = 614

CPU2006 license: 6 Test date: Sep-2010 Test sponsor: Oracle Corporation Hardware Availability: Dec-2010 Tested by: Oracle Corporation Software Availability: Sep-2010

400.perlbench

401.bzip2

403.gcc

429.mcf

445.gobmk

456.hmmer

458.sjeng

462.libquantum

464.h264ref

471.omnetpp

473.astar

483.xalancbmk

Copies

SPECint_rate2006 = 666

SPECint_rate_base2006 = 614

0 2200

100 200 300 400 500 600 700 800 900 1000 1100 1200 1300 1400 1500 1600 1700 1800 1900 2000 510 611 510 771

510 377 510 382

510 394 510 402

510 473

510 755 510 840

510 483 510 519

510 669 510 725

510 2150

510 2170

510 784 510 820

510 600 510 644

510 446 510 498

510 607 510 762

Hardware

CPU Name: SPARC T3 CPU Characteristics: CPU MHz: 1649 FPU: Integrated CPU(s) enabled: 64 cores, 4 chips, 16 cores/chip, 8 threads/core CPU(s) orderable: 1 to 4 chips Primary Cache: 16 KB I + 8 KB D on chip per core Secondary Cache: 6 MB I+D on chip per chip L3 Cache: None Other Cache: None Memory: 512 GB (64 x 8 GB) Disk Subsystem: 821 GB (zfs 3 x 2-way mirrors on 6x SAS 300G 10000 RPM) Other Hardware: None

Software

Operating System: Oracle Solaris 10 9/10 Compiler: Oracle Solaris Studio 12.2 Auto Parallel: No File System: zfs with gzip compression System State: Default Base Pointers: 32-bit Peak Pointers: 32-bit Other Software: None

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org/

Page 2 spec^® SPEC CINT2006 Result

Copyright 2006-2014 Standard Performance Evaluation Corporation

Oracle Corporation SPARC T3-4

SPECint_rate2006 = 666

SPECint_rate_base2006 = 614

CPU2006 license: 6 Test date: Sep-2010 Test sponsor: Oracle Corporation Hardware Availability: Dec-2010 Tested by: Oracle Corporation Software Availability: Sep-2010

Results Table

Benchmark Copies Seconds Ratio Seconds Ratio Seconds Ratio

Base Copies Seconds Ratio Seconds Ratio Seconds Ratio

Peak

400.perlbench 510 8127 613 8151 611 8156 611 510 6432 775 6465 771 6478 769

401.bzip2 510 13084 376 13063 377 13054 377 510 12853 383 12882 382 12885 382

403.gcc 510 10405 395 10419 394 10418 394 510 10191 403 10204 402 10202 402

429.mcf 510 9840 473 9838 473 9839 473 510 9840 473 9838 473 9839 473

445.gobmk 510 7086 755 7082 755 7084 755 510 6367 840 6367 840 6366 840

456.hmmer 510 9887 481 9847 483 9847 483 510 9162 519 9163 519 9165 519

458.sjeng 510 9218 669 9222 669 9217 670 510 8510 725 8509 725 8513 725

462.libquantum 510 4924 2150 4923 2150 4923 2150 510 4878 2170 4876 2170 4879 2170

464.h264ref 510 14380 785 14388 784 14389 784 510 13766 820 13761 820 13767 820

471.omnetpp 510 5323 599 5315 600 5308 600 510 4952 644 4954 643 4952 644

473.astar 510 8035 446 8002 447 8036 446 510 7199 497 7196 498 7195 498

483.xalancbmk 510 5803 606 5800 607 5788 608 510 4618 762 4635 759 4621 762

Results appear in the order in which they were run. Bold underlined text indicates a median measurement.

Compiler Invocation Notes

 Oracle Solaris Studio 12.2 is distributed with mandatory OS patches
  118683-05  119963-20  120753-08
 Oracle Solaris Studio 12.2 and patches are available at
  http://oracle.com/goto/solarisstudio

Submit Notes

Processes were bound to cores using "submit" and "pbind".  The config
file option ’submit’ was used in order to accomplish this.

Operating System Notes

ulimit -s 131072 was used to limit the space
consumed by the stack (and therefore make more
space available to the heap).

 /etc/system parameters
    autoup=600
       Causes pages older than the listed number of seconds to
       be written by fsflush.
    tune_t_fsflushr=10
       Controls how many seconds elapse between runs of the
       page flush daemon, fsflush.
    lpg_alloc_prefer=1
        Indicates that extra effort should be taken to ensure
        that pages are created in the nearby lgroup (NUMA location).

Continued on next page

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org/

Page 3 spec^® SPEC CINT2006 Result

Copyright 2006-2014 Standard Performance Evaluation Corporation

Oracle Corporation SPARC T3-4

SPECint_rate2006 = 666

SPECint_rate_base2006 = 614

CPU2006 license: 6 Test date: Sep-2010 Test sponsor: Oracle Corporation Hardware Availability: Dec-2010 Tested by: Oracle Corporation Software Availability: Sep-2010

Operating System Notes (Continued)

    tsb_rss_factor=128
        Suggests that the the size of the TSB (Translation
        Storage Buffer) may be increased if it is more than
        25% (128/512) full.  Doing so may reduce TSB traps,
        at the cost of additional kernel memory.
    zfs:zfs_arc_max=0x10000000
    zfs:zfs_arc_min=0x10000000
        Limits the consumption of memory by the zfs file system
        cache to 256 MB.  (The arc_max sets the maximum cache
        size; arc_min sets the minimum.)
    zfs:zfs_prefetch_disable = 1
        Indicates that prefetching is not desired.  This setting
        may be desirable when the file system cache is small.
 USB devices were turned off with ILOM command
    set /SYS/MB/USB component_state=disabled
 The "webconsole" service was turned off using
     svcadm disable webconsole
 The system had 437 GB of swap space.

Base Compiler Invocation

C benchmarks:

cc

C++ benchmarks:

CC

Base Portability Flags

400.perlbench: -DSPEC_CPU_SOLARIS_SPARC

403.gcc: -DSPEC_CPU_SOLARIS 462.libquantum: -DSPEC_CPU_SOLARIS 483.xalancbmk: -DSPEC_CPU_SOLARIS

Base Optimization Flags

C benchmarks:

-g -fast -fma=fused -xipo=2 -xprefetch=no%auto -xpagesize=4M
-xalias_level=std -M /usr/lib/ld/map.bssalign

C++ benchmarks:

-g0 -library=stlport4 -fast -fma=fused -xipo=2 -xprefetch=no%auto
-xpagesize=4M -xdepend -xalias_level=compatible
-M /usr/lib/ld/map.bssalign

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org/

Page 4 spec^® SPEC CINT2006 Result

Copyright 2006-2014 Standard Performance Evaluation Corporation

Oracle Corporation SPARC T3-4

SPECint_rate2006 = 666

SPECint_rate_base2006 = 614

CPU2006 license: 6 Test date: Sep-2010 Test sponsor: Oracle Corporation Hardware Availability: Dec-2010 Tested by: Oracle Corporation Software Availability: Sep-2010

Base Other Flags

C benchmarks:

-xjobs=64 -V -#

C++ benchmarks:

-xjobs=64 -verbose=diags,version

Peak Compiler Invocation

C benchmarks:

cc

C++ benchmarks:

CC

Peak Portability Flags

400.perlbench: -DSPEC_CPU_SOLARIS_SPARC

403.gcc: -DSPEC_CPU_SOLARIS 462.libquantum: -DSPEC_CPU_SOLARIS 483.xalancbmk: -DSPEC_CPU_SOLARIS

Peak Optimization Flags

C benchmarks:

400.perlbench: -g -xprofile=collect:./feedback(pass 1)

-xprofile=use:./feedback(pass 2) -fast -fma=fused
-xpagesize=4M -M /usr/lib/ld/map.bssalign -xalias_level=std
-xipo=2 -Xc -xrestrict -lfast

401.bzip2: -g -xprofile=collect:./feedback(pass 1)

-xprofile=use:./feedback(pass 2) -fast -fma=fused
-xpagesize=4M -xalias_level=strong

403.gcc: -g -xprofile=collect:./feedback(pass 1)

-xprofile=use:./feedback(pass 2) -fast -fma=fused
-xpagesize=4M -xalias_level=std -xprefetch_level=1

429.mcf: basepeak = yes

445.gobmk: -g -xprofile=collect:./feedback(pass 1)

-xprofile=use:./feedback(pass 2) -fast -fma=fused
-xpagesize=4M -M /usr/lib/ld/map.bssalign -xalias_level=std
-xrestrict -xprefetch=no%auto

Continued on next page

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org/

Page 5 spec^® SPEC CINT2006 Result

Copyright 2006-2014 Standard Performance Evaluation Corporation

Oracle Corporation SPARC T3-4

SPECint_rate2006 = 666

SPECint_rate_base2006 = 614

CPU2006 license: 6 Test date: Sep-2010 Test sponsor: Oracle Corporation Hardware Availability: Dec-2010 Tested by: Oracle Corporation Software Availability: Sep-2010

Peak Optimization Flags (Continued)

456.hmmer: -g -xprofile=collect:./feedback(pass 1)

-xprofile=use:./feedback(pass 2) -fast -fma=fused -xipo=2
-xpagesize=4M -xunroll=14 -xalias_level=std

458.sjeng: -g -xprofile=collect:./feedback(pass 1)

-xprofile=use:./feedback(pass 2) -fast -fma=fused
-xpagesize=4M -xipo=2 -xprefetch=no%auto

462.libquantum: -g -fast -fma=fused -xpagesize=4M

-M /usr/lib/ld/map.bssalign -xipo=2 -xprefetch_level=3
-xalias_level=std

464.h264ref: -g -xprofile=collect:./feedback(pass 1)

-xprofile=use:./feedback(pass 2) -fast -fma=fused
-xpagesize=4M -xipo=2 -xalias_level=std

C++ benchmarks:

471.omnetpp: -g0 -library=stlport4 -xprofile=collect:./feedback(pass 1)

-xprofile=use:./feedback(pass 2) -fast -fma=fused -xipo=2
-xprefetch=no%auto -xpagesize=4M -xdepend
-xalias_level=compatible -M /usr/lib/ld/map.bssalign

473.astar: -g0 -library=stlport4 -xprofile=collect:./feedback(pass 1)

-xprofile=use:./feedback(pass 2) -fast -fma=fused
-xpagesize=4M -xdepend -xalias_level=compatible -xipo=2
-xprefetch=no%auto -lfast

483.xalancbmk: -g0 -library=stlport4 -xprofile=collect:./feedback(pass 1)

-xprofile=use:./feedback(pass 2) -fast -fma=fused
-xpagesize=4M -xdepend -xalias_level=compatible
-M /usr/lib/ld/map.bssalign -xipo=2 -xprefetch=no%auto
-lfast

Peak Other Flags

C benchmarks:

-xjobs=64 -V -#

C++ benchmarks:

-xjobs=64 -verbose=diags,version

The flags file that was used to format this result can be browsed at

http://www.spec.org/cpu2006/flags/Oracle-Solaris-Studio12.2-SPARC.20110110.html

You can also download the XML flags source by saving the following link:

http://www.spec.org/cpu2006/flags/Oracle-Solaris-Studio12.2-SPARC.20110110.xml

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org/

Page 6 spec^® SPEC CINT2006 Result

Copyright 2006-2014 Standard Performance Evaluation Corporation

Oracle Corporation SPARC T3-4

SPECint_rate2006 = 666 SPECint_rate_base2006 = 614

CPU2006 license: 6 Test date: Sep-2010 Test sponsor: Oracle Corporation Hardware Availability: Dec-2010 Tested by: Oracle Corporation Software Availability: Sep-2010

Originally published on 1 February 2011.

Report generated on Wed Jul 23 15:14:48 2014 by SPEC CPU2006 PS/PDF formatter v6932.

Tested with SPEC CPU2006 v1.1.

For other inquiries, please contact webmaster@spec.org.

For questions about this result, please contact the tester.

holders.

this result are trademarks or registered trademarks of their respective

Evaluation Corporation. All other brand and product names appearing in

SPEC and SPECint are registered trademarks of the Standard Performance