Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec HPC2002 Result

Copyright ©1999-2002, Standard Performance Evaluation Corporation

Sun Microsystems Sun HPC 3500

SPECchemM2002 = 2.21

SPEC license #: HPG0007A Tested by: Purdue University Test site: Purdue University Test date: Oct-2003 HW Avail: Dec-1998 SW Avail: Apr-2003

Benchmark

Reference Time Runtime Ratio 1 2 3 4 5

371.gamess_m 86400 39147 2.21

Hardware

CPU: UltraSPARC II CPU MHz: 400 FPU: Integrated CPU(s) enabled: 8 CPU(s) orderable: 1 to 8 Primary Cache: 16KBI+16KBD on chip Secondary Cache: 4MB(I+D) off chip L3 Cache: None Other Cache: None Memory: 8GB Disk Subsystem: 2 x Fujitsu MAA3182S SUN18G Other Hardware: 100Mbps Ethernet

Software

Parallel: OpenMP Processes-Threads: 8 MPI Processes: -- OpenMP Threads: 8 Operating System: Solaris 8 Compiler: Sun Forte Developer 7 C 5.4 2002/03/09

Sun Forte Developer 7 Fortran 95 7.0 Patch 111714-06 2003/04/10

File System: UFS System State: Multi User Other Software: --

Notes/Tuning Information

Tested by Purdue University

Flags:
  OPTIMIZE = -fast -xarch=v9a -xopenmp -xunroll=5
  FOPTIMIZE = -xtypemap=integer:64
  CPPFLAGS  = -I. -D_OPENMP

OS Environment:
  csh/tcsh: unlimit stacksize

The MPI result is about the same as the OpenMP result.