Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec OMPM2001 Result

Copyright ©1999-2002, Standard Performance Evaluation Corporation

Sun Microsystems Sun Fire V40z

SPECompMpeak2001 = SPECompMbase2001 =

8694 8382

SPEC license #:HPG0010 Tested by: Sun Microsystems, Santa Clara Test site: Menlo Park Test date: Oct-2004 Hardware Avail:Jul-2004 Software Avail:Jul-2004

Benchmark

Reference

Time

Base Runtime

Base Ratio

Peak Runtime

Peak Ratio 10000 20000 30000

310.wupwise_m 6000 489 12273 487 12315

312.swim_m 6000 501 11967 488 12305

314.mgrid_m 7300 771 9469 763 9565

316.applu_m 4000 622 6434 483 8280

318.galgel_m 5100 568 8971 554 9202

320.equake_m 2600 340 7647 330 7883

324.apsi_m 3400 392 8664 386 8811

326.gafort_m 8700 1282 6788 1249 6967

328.fma3d_m 4600 834 5518 834 5518

330.art_m 6400 371 17231 371 17231

332.ammp_m 7000 1674 4181 1658 4221

Hardware

CPU: AMD Opteron (TM) 850 CPU MHz: 2400 FPU: Integrated CPU(s) enabled: 4 cores, 4 chips, 1 core/chip CPU(s) orderable: 1,2,4 Primary Cache: 64KBI + 64KBD on chip Secondary Cache: 1024KB (I+D) on chip L3 Cache: None Other Cache: None Memory: 16x1GB, PC2700 CL2.5 DDR SDRAM ECC Registered Disk Subsystem: SCSI, 73GB, 10K RPM Other Hardware: None

Software

OpenMP Threads: 4 Parallel: OpenMP + Auto Concurrentization Operating System: SuSE Linux 9.0 Professional Compiler: PGI Fortran 5.2-1 File System: Linux/ext3 System State: Multi-User

Notes/Tuning Information

 Base tuning:
   C       : pgcc  -mp -fastsse -O4 -Minline=levels:8 -mcmodel=medium
   Fortran : pgf90 -mp -fastsse -O4 -Minline=levels:8 -mcmodel=medium
   ONESTEP=yes
   srcalt = purdue1 used for 330.art_m

 Peak tuning:
  ONESTEP=yes for all peak tests.

  310.wupwise_m   : -mp -fastsse -Minline=level:8  -mcmodel=medium
  312.swim_m      : -fastsse -Mconcur -Mipa=fast,inline  -mcmodel=medium
  314.mgrid_m     : -mp -fastsse    -Mnofptrap
  316.applu_m     : -mp -fastsse -O4  -Minline=levels:8 -mcmodel=medium
                    srcalt = ompl.32
  318.galgel_m    : -mp -fastsse -Mconcur -Mipa=fast,inline  -mcmodel=medium -Munsafe_par_align
  320.equake_m    : -mp -fastsse -O4 -Minline=levels:8 -mcmodel=medium
                    srcalt = ompl.32
  324.apsi_m      : -mp -fastsse -O4 -Minline=levels:8 -mcmodel=medium -Munsafe_par_align
                    srcalt = ompl.32
  326.gafort_m    : -mp -fastsse -O4 -Minline=levels:8 -mcmodel=medium
                    srcalt = ompl
  328.fma3d_m     : basepeak=yes

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec OMPM2001 Result

Copyright ©1999-2002, Standard Performance Evaluation Corporation

Sun Microsystems Sun Fire V40z

SPECompMpeak2001 = SPECompMbase2001 =

8694 8382

SPEC license #:HPG0010 Tested by: Sun Microsystems, Santa Clara Test site: Menlo Park Test date: Oct-2004 Hardware Avail:Jul-2004 Software Avail:Jul-2004

Notes/Tuning Information (Continued)

  330.art_m       : basepeak=yes
  332.ammp_m      : -mp -fastsse  -O -Minline  -Mframe

 Portablility flags:
  318.galgel_m    : -Mfixed -Mextend

 Base and Peak User Environment (bash):
   export OMP_NUM_THREADS=4
   export NCPUS=4
   export OMP_DYNAMIC=FALSE
   ulimit -s unlimited

 Default BIOS settings used.

 For a description of PGI compiler and portability flags, and
 system parameters used to generate this result, please refer to
 SUN-20041028-pgi-linux-opteron.txt file in the flags directory.