Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec OMPL2001 Result

Copyright ©1999-2007, Standard Performance Evaluation Corporation

Sun Microsystems Sun Fire X4600 M2

SPECompLpeak2001 = SPECompLbase2001 =

103466 100610

SPEC license #:HPG0010 Tested by: Sun Microsystems, Santa Clara Test site: Menlo Park Test date: Mar-2007 Hardware Avail:Oct-2006 Software Avail:Aug-2006

Benchmark

Reference

Time

Base Runtime

Base Ratio

Peak Runtime

Peak Ratio 200000 400000 600000

311.wupwise_l 9200 1174 125397 1080 136267

313.swim_l 12500 2432 82221 2405 83153

315.mgrid_l 13500 1807 119515 1807 119515

317.applu_l 13500 3703 58338 3588 60195

321.equake_l 13000 2830 73485 2745 75769

325.apsi_l 10500 2771 60623 2771 60623

327.gafort_l 11000 1613 109124 1613 109124

329.fma3d_l 23500 4313 87172 3920 95919

331.art_l 25000 1154 346714 1154 346714

Hardware

CPU: AMD Opteron (TM) 8220 CPU MHz: 2800 FPU: Integrated CPU(s) enabled: 8 cores, 4 chips, 2 cores/chip CPU(s) orderable: 4,8 (order by number of chips) Primary Cache: 64KBI + 64KBD (on chip) per core Secondary Cache: 1024KB (I+D) (on chip) per core L3 Cache: None Other Cache: None Memory: 32GB (16x2GB, DDR2-667 CL5 ECC Registered) Disk Subsystem: SAS, 73GB, 10K RPM Other Hardware: None

Software

OpenMP Threads: 8 Parallel: OpenMP Operating System: Red Hat Enterprise Linux AS release 4 Update 5 Compiler: QLogic PathScale Compiler Suite, Release 2.5 File System: ext2 System State: Multi-user run level 3

Notes/Tuning Information

 User environment:
 export OMP_DYNAMIC=FALSE
 export OMP_NUM_THREADS=8
 ulimit -s unlimited

 Default BIOS settings used.

 Baseline optimization flags:
   C programs:       -Ofast -mp
   Fortran programs: -Ofast -OPT:early_mp=on -mcmodel=medium -mp
 Peak optimization flags:
    311.wupwise_l: -mp -Ofast -msse3 -LNO:prefetch_ahead=5:prefetch=3
                   -OPT:unroll_times_max=8:unroll_size=128:IEEE_NaN_Inf=off:ro=3
                   -IPA:linear=on:plimit=50000:callee_limit=5000 -INLINE:aggressive=on
    313.swim_l:    -mp -O3 -OPT:Ofast -m3dnow -mcmodel=medium -LNO:simd=0
    315.mgrid_l:   basepeak=yes
    317.applu_l:   -mp -Ofast -mcmodel=medium -CG:local_fwd_sched=on
                   -LNO:fusion=2:fission=2:full_unroll_size=10000:prefetch=3 -TENV:X=3
    321.equake_l:  -Ofast -mp -OPT:alias=disjoint
    325.apsi_l:    basepeak=yes
    327.gafort_l:  basepeak=yes
    329.fma3d_l:   -mp -O2 -ipa -CG:load_exe=1
                   -OPT:Ofast:early_mp=on:IEEE_arith=3:ro=3 -WOPT:mem_opnds=on:retype_expr=on
                   -IPA:pu_reorder=1
    331.art_l:     basepeak=yes

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec OMPL2001 Result

Copyright ©1999-2007, Standard Performance Evaluation Corporation

Sun Microsystems Sun Fire X4600 M2

SPECompLpeak2001 = SPECompLbase2001 =

103466 100610

SPEC license #:HPG0010 Tested by: Sun Microsystems, Santa Clara Test site: Menlo Park Test date: Mar-2007 Hardware Avail:Oct-2006 Software Avail:Aug-2006

Notes/Tuning Information (Continued)

 For a description of PathScale v2.5 compiler flags, portability flags
 and system parameters used to generate this result, please refer to
 SUN-20070403-PathScale2.5-Linux-opteron.txt file in the flags directory.