Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec OMPM2001 Result

Copyright ©1999-2001, Standard Performance Evaluation Corporation

Fujitsu Limited PRIMEPOWER2000 (563MHz)

SPECompMpeak2001 = SPECompMbase2001 = -- 13986

SPEC license #:HPG0003 Tested by: Fujitsu Limited Test site: Test date: Jun-2001 Hardware Avail:Feb-2001 Software Avail:Sep-2001

Benchmark

Reference

Time

Base Runtime

Base Ratio

Peak Runtime

Peak Ratio 10000 20000 30000

310.wupwise_m 6000 284 21108

312.swim_m 6000 369 16267

314.mgrid_m 7300 367 19868

316.applu_m 4000 135 29537

318.galgel_m 5100 990 5149

320.equake_m 2600 227 11444

324.apsi_m 3400 137 24825

326.gafort_m 8700 485 17938

328.fma3d_m 4600 528 8718

330.art_m 6400 513 12478

332.ammp_m 7000 1005 6964

Hardware

CPU: SPARC64 GP CPU MHz: 563 FPU: Integrated CPU(s) enabled: 66 CPU(s) orderable: 8 to 128 Primary Cache: 128KBI+128KBD on chip Secondary Cache: 8MB(I+D) off chip, per CPU L3 Cache: None Other Cache: None Memory: 128GB Disk Subsystem: 2 x 18.2GB SCSI (10025rpm) Other Hardware: None

Software

OpenMP Threads: 64 Parallel: -- Operating System: Solaris 8 - 6/00 Fujitsu Parallelnavi 1.0.2 (NQS, CPU scheduler, largepage) Compiler: Fujitsu Parallelnavi 1.0.2 (C, F90) File System: ufs System State: Multi-user

Notes/Tuning Information

 Baseline flags:
     C:    -KOMP,largepage -Kfast_GP=2,V9FMADD -x-
     F90:  -KOMP,largepage -Kfast_GP=2,V9FMADD -Nautoobjstack -Knogs

 Portability Flags:
     318.galgel_m:  -Am -Fixed -w
     328.fma3d_m:   -Am

 Extra Flags:
     330.art_m:     -DINTS_PER_CACHELINE=16 -DDBLS_PER_CACHELINE=8

 System tunables:
     /etc/system:
         set shmsys:shminfo_shmmax=268435456
         set shmsys:shminfo_shmmni=4096
         set shmsys:shminfo_shmseg=4096
     /etc/opt/FJSVpnrm/lpg.conf:
         JOB=32G,SHMSEGSIZE=256M
     /etc/opt/FJSVpnrm/cpursc.conf:
         CPU_USE=0-1:0-1
     NQS:
         Per-process data size limit = 40 gigabytes

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec OMPM2001 Result

Copyright ©1999-2001, Standard Performance Evaluation Corporation

Fujitsu Limited PRIMEPOWER2000 (563MHz)

SPECompMpeak2001 = SPECompMbase2001 = -- 13986

SPEC license #:HPG0003 Tested by: Fujitsu Limited Test site: Test date: Jun-2001 Hardware Avail:Feb-2001 Software Avail:Sep-2001

Notes/Tuning Information (Continued)

         Per-process permanent file size limit = 1 gigabytes
         Per-process memory size limit = 40 gigabytes
         Per-request memory size limit = 32 gigabytes
         Per-process number of cpus limit = 126
         Per-process stack size limit = 4 gigabytes
         Per-process CPU time limit = 453600.000
         Execution mode = SImplex
         Jobclass = 0

 Submitting the runspec to NQS:
     Run the qsub command with the following sh script.

         cd /kaiser2/kit27
         . ./shrc
         OMP_NUM_THREADS=64
         export OMP_NUM_THREADS
         runspec --config=Fujitsu_PP2000_064 --reportable medium