Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec OMPL2001 Result

Copyright ©1999-2002, Standard Performance Evaluation Corporation

SGI_{SGI Origin 3900 128X 600MHz R14000A} SPECompLpeak2001 =

SPECompLbase2001 =

197838 193992

SPEC license #:HPG0014 Tested by: SGI Test site: SGI Test date: Nov-2002 Hardware Avail:Dec-2002 Software Avail:Dec-2002

Benchmark

Reference

Time

Base Runtime

Base Ratio

Peak Runtime

Peak Ratio 100000 200000 300000

311.wupwise_l 9200 497 296470 497 296470

313.swim_l 12500 1022 195626 1022 195626

315.mgrid_l 13500 904 239055 904 239055

317.applu_l 13500 1147 188297 989 218439

321.equake_l 13000 1870 111228 1870 111228

325.apsi_l 10500 1068 157350 1068 157350

327.gafort_l 11000 1118 157373 1118 157373

329.fma3d_l 23500 1752 214635 1703 220773

331.art_l 25000 1587 252116 1587 252116

Hardware

CPU: R14000 CPU MHz: 600 FPU: Integrated CPU(s) enabled: 128 CPU(s) orderable: 2-1024 Primary Cache: 32KBI + 32KBD on chip Secondary Cache: 8MB(I+D) off chip L3 Cache: N/A Other Cache: N/A Memory: 128 GB Disk Subsystem: 1 x 18 GB FC, 20x 18 GB (striped) FC Other Hardware: None

Software

OpenMP Threads: 128 Parallel: OpenMP Operating System: IRIX 6.5.18f Compiler: MIPSpro 7.4 C, Fortran90 File System: xfs System State: Single-user

Notes/Tuning Information

Baseline flags (C benchmarks): -64 -mp -Ofast=ip35
Baseline flags (Fortran benchmarks): -64 -mp -Ofast=ip35 -LNO:fusion=2

Peak flags:
311.wupwise_l: basepeak=true
313.swim_l: basepeak = true
315.mgrid_l: basepeak=true
317.applu_l: -64 -mp -Ofast=ip35 -LNO:prefetch=0:fusion=2 -CG:ld_latency=3
321.equake_l: basepeak = true
325.apsi_l: basepeak = true
327.gafort_l: basepeak=true
329.fma3d_l: -64 -mp -Ofast=ip35 -bigp_off -LNO:prefetch=0 -CG:ld_latency=2 -OPT:goto=off
331.art_l: basepeak = true

Baseline user environment:
   limit stacksize 512m
   OMP_NUM_THREADS=128
   OMP_DYNAMIC=FALSE
   MPC_GANG=OFF
   _DSM_MUSTRUN=

Peak user environment:
317.applu_l: PAGESIZE_DATA=4096, PAGESIZE_STACK=4096, _DSM_PLACEMENT=ROUND_ROBIN

The following O/S parameters were set via systune:
   percent_totalmem_4m_pages = 25 ; percent_totalmem_1m_pages = 25

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec OMPL2001 Result

Copyright ©1999-2002, Standard Performance Evaluation Corporation

SGI_{SGI Origin 3900 128X 600MHz R14000A} SPECompLpeak2001 =

SPECompLbase2001 =

197838 193992

SPEC license #:HPG0014 Tested by: SGI Test site: SGI Test date: Nov-2002 Hardware Avail:Dec-2002 Software Avail:Dec-2002

Notes/Tuning Information (Continued)

   percent_totalmem_256k_pages = 10 ; percent_totalmem_64k_pages = 10