Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec OMPL2001 Result

Copyright ©1999-2002, Standard Performance Evaluation Corporation

Sun Microsystems Sun Fire E25K (72 processor)

SPECompLpeak2001 = SPECompLbase2001 =

316182 240622

SPEC license #:HPG0010 Tested by: Sun Microsystems Test site: Sun Microsystems Test date: Feb-2004 Hardware Avail:May-2004 Software Avail:Jul-2004

Benchmark

Reference

Time

Base Runtime

Base Ratio

Peak Runtime

Peak Ratio 2000000 4000000

311.wupwise_l 9200 392 375539 302 487262

313.swim_l 12500 894 223826 672 297689

315.mgrid_l 13500 1007 214577 704 306847

317.applu_l 13500 917 235603 883 244551

321.equake_l 13000 2967 70107 1814 114639

325.apsi_l 10500 1290 130228 935 179767

327.gafort_l 11000 770 228430 721 244119

329.fma3d_l 23500 2366 158909 1315 285845

331.art_l 25000 208 1920101 198 2017639

Hardware

CPU: Sun UltraSPARC s400 CPU MHz: 1050 FPU: Integrated CPU(s) enabled: 144 cores, 72 chips, 2 cores/chip CPU(s) orderable: 4-72 (multiples of 4 chips) Primary Cache: 32KBI+64KBD per core on chip (64KBI+128KBD on chip) Secondary Cache: 8MB(I+D) per core off chip (16MB(I+D) off chip) L3 Cache: None Other Cache: None Memory: 288GB 16-way interleaved Disk Subsystem: 1x72GB Other Hardware: --

Software

OpenMP Threads: 143 Parallel: OpenMP + Auto Parallel Operating System: Solaris 9 04/04 Compiler: Sun Studio 9 Early Access 1 (Beta) File System: ufs System State: Multi-User

Notes/Tuning Information

 Base Flags and Notes:
   ONESTEP=yes for all benchmarks

   C:   -fast -xopenmp -xalias_level=std -xipo=2 -Xc
        -xprefetch_level=2 -xcode=abs44 -xarch=v9a -lmtmalloc
        -xprofile
   f90: -fast -openmp -xcode=abs44 -xarch=v9a -xipo=2 -autopar
        -xprofile

   submit = ppgsz -o heap=4m,stack=4m $command

 Extra art Base Flags:
   331.art_l:     -DINTS_PER_CACHELINE=16 -DDBLS_PER_CACHELINE=8

 Peak Flags and Notes:
   ONESTEP=yes for all benchmarks

   311.wupwise_l: -fast -openmp -autopar -xunroll=2
                  -Qoption iropt -Athr,-Ainline:inc=800:cp=1
                  -xipo=2 -xprefetch_level=3 -xarch=v9a
                  -xprofile
       submit = ppgsz -o heap=512k,stack=512k $command
   313.swim_l: -fast -openmp -xarch=v9a -xipo=2 -autopar
               -xprofile
       submit = ppgsz -o heap=512k,stack=512k $command

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec OMPL2001 Result

Copyright ©1999-2002, Standard Performance Evaluation Corporation

Sun Microsystems Sun Fire E25K (72 processor)

SPECompLpeak2001 = SPECompLbase2001 =

316182 240622

SPEC license #:HPG0010 Tested by: Sun Microsystems Test site: Sun Microsystems Test date: Feb-2004 Hardware Avail:May-2004 Software Avail:Jul-2004

Notes/Tuning Information (Continued)

   315.mgrid_l: -fast -openmp -xipo=2 -xprefetch_level=3
                -xprefetch=latx:2 -xprofile
                -Qoption iropt -Apf:largedim -xarch=v9a
       submit = ppgsz -o heap=512k,stack=512k $command
       OMP_NUM_THREADS=128
   317.applu_l: -fast -openmp -xipo=2
                -Qoption iropt -Aujam:inner=g -xunroll=1
                -xprefetch=latx:1.8 -xarch=v9a -xprofile
       submit = ppgsz -o heap=4m,stack=4m $command
       OMP_NUM_THREADS=133
   321.equake_l: -fast -xopenmp -xipo=2 -xcode=abs44
                 -xrestrict -xalias_level=strong
                 -xprefetch_level=3 -xprefetch=latx:2.5
                 -W2,-Apf:pdl=1 -Wc,-Qlp-ip=1-ol=1
                 -xarch=v9a -lmtmalloc -xprofile
       submit = ppgsz -o heap=64k,stack=64k $command
       OMP_NUM_THREADS = 117
   325.apsi_l: -fast -openmp -xcode=abs44
               -xipo -autopar -xarch=v9a -xprofile
       submit = ppgsz -o heap=4m,stack=4m $command
       OMP_NUM_THREADS = 140
   327.gafort_l: -fast -openmp -autopar -xarch=v9a -xprofile
       submit = ppgsz -o heap=4m,stack=4m $command
   329.fma3d_l: -fast -openmp -xipo=2 -xprefetch_level=3
                -Qoption iropt -Athr,-Apf:pdl=1
                -Qoption cg -Qlp-ip=1
                -xarch=v9a -lmtmalloc -xprofile
       submit = ppgsz -o heap=512k,stack=512k $command
   331.art_l: -fast -xopenmp -xipo=2
              -xalias_level=strong -xprefetch_level=2
              -W2,-Apf:outer=0:pdl=1 -Wc,-Qlp-ip=1
              -xarch=v9a -lmopt -lm -lmtmalloc -xprofile
       submit= ppgsz -o heap=512k,stack=512k $command

 Alternate Source for Peak:
   Change initial data distribution for WORK array
       Submitted Source:  ompl2001-dd-20040128.tar.gz
       325.apsi_l

 Feedback optimization (-xprofile) is done as follows,
 unless otherwise noted:
   fdo_pre0:  rm -rf ‘pwd‘/../feedback.profile
   PASS1:     -xprofile=collect:./feedback
   PASS2:     -xprofile=use:./feedback

 Base and Peak User Environment:
   unlimit stacksize   (in /bin/csh)
   setenv STACKSIZE 16384
   setenv OMP_NUM_THREADS 143
   setenv OMP_DYNAMIC FALSE
   setenv MT_BIND_PROCESSOR "0 4 1 5 2 6 3 7
   8 12 9 13 10 14 11 15  16 20 17 21 18 22 19 23
   24 28 25 29 26 30 27 31  32 36 33 37 34 38 35 39
   40 44 41 45 42 46 43 47  48 52 49 53 50 54 51 55
   56 60 57 61 58 62 59 63  64 68 65 69 66 70 67 71
   72 76 73 77 74 78 75 79  80 84 81 85 82 86 83 87

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec OMPL2001 Result

Copyright ©1999-2002, Standard Performance Evaluation Corporation

Sun Microsystems Sun Fire E25K (72 processor)

SPECompLpeak2001 = SPECompLbase2001 =

316182 240622

SPEC license #:HPG0010 Tested by: Sun Microsystems Test site: Sun Microsystems Test date: Feb-2004 Hardware Avail:May-2004 Software Avail:Jul-2004

Notes/Tuning Information (Continued)

   88 92 89 93 90 94 91 95  96 100 97 101 98 102 99 103
   104 108 105 109 106 110 107 111
   112 116 113 117 114 118 115 119
   120 124 121 125 122 126 123 127
   128 132 129 133 130 134 131 135
   136 140 137 141 138 142 139 143"

 Kernel Paramters (/etc/system):
   set autoup=900
   set tune_t_fsflushr=1

 Sun Studio 9 will be generally available July 2004

 System configuration details located at
   http://www.sun.com/servers/