Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec OMPM2001 Result

Copyright ©1999-2002, Standard Performance Evaluation Corporation

Sun Microsystems Sun Fire V40z

SPECompMpeak2001 = SPECompMbase2001 =

6486 6344

SPEC license #:HPG0010 Tested by: Sun Microsystems, Santa Clara Test site: Menlo Park Test date: Feb-2005 Hardware Avail:Apr-2005 Software Avail:Apr-2005

Benchmark

Reference

Time

Base Runtime

Base Ratio

Peak Runtime

Peak Ratio 10000 20000 30000

310.wupwise_m 6000 809 7412 803 7475

312.swim_m 6000 796 7535 761 7889

314.mgrid_m 7300 1124 6494 1124 6494

316.applu_m 4000 837 4777 722 5540

318.galgel_m 5100 735 6941 731 6973

320.equake_m 2600 350 7422 350 7422

324.apsi_m 3400 556 6116 537 6336

326.gafort_m 8700 1593 5462 1593 5462

328.fma3d_m 4600 1119 4111 1119 4111

330.art_m 6400 337 18984 337 18984

332.ammp_m 7000 2430 2881 2430 2881

Hardware

CPU: AMD Opteron (TM) 852 CPU MHz: 2600 FPU: Integrated CPU(s) enabled: 2 cores, 2 chips, 1 core/chip CPU(s) orderable: 1,2,4 Primary Cache: 64KBI + 64KBD on chip Secondary Cache: 1024KB (I+D) on chip L3 Cache: None Other Cache: None Memory: 8GB (4x2GB, PC3200 CL3 DDR SDRAM ECC Registered) Disk Subsystem: SCSI, 73GB, 10K RPM Other Hardware: None

Software

OpenMP Threads: 2 Parallel: OpenMP Operating System: SUSE LINUX Enterprise Server 9 Compiler: PathScale EKOPath Compiler Suite, Release 2.1 File System: ufs System State: Multi-User

Notes/Tuning Information

 Baseline Optimization Flags:
   Fortran : -Ofast -OPT:early_mp=on -mcmodel=medium -mp
   C       : -Ofast -mp

 Peak Optimization Flags:
   310.wupwise_m : -mp -Ofast -mcmodel=medium -LNO:prefetch_ahead=5:prefetch=3 -TENV:X=4
                   -OPT:unroll_times_max=8:unroll_size=128:IEEE_NaN_Inf=off:ro=3
   312.swim_m    : -mp -O3 -OPT:Ofast -m3dnow -mcmodel=medium -LNO:simd=0
   314.mgrid_m   :  basepeak=yes
   316.applu_m   :  -mp -Ofast -mcmodel=medium -CG:local_fwd_sched=on
                    -LNO:fusion=2:fission=2:full_unroll_size=10000:prefetch=3 -TENV:X=3
   318.galgel_m  :  -Ofast -mp -OPT:early_mp=on
   320.equake_m  :  basepeak=yes
   324.apsi_m    :  -mp -O3 -OPT:Ofast -TENV:x=4 -LNO:fusion=2:prefetch=0
   326.gafort_m  :  basepeak=yes
   328.fma3d_m   :  basepeak=yes
   330.art_m     :  basepeak=yes
   332.ammp_m    :  basepeak=yes

 Alternate Source:
   330.art_m  :  required srcalt purdue1 used for base and peak
   316.applu_m:  approved srcalt ompl.32 used for peak
   324.apsi_m :  approved srcalt ompl.32 used for peak

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec OMPM2001 Result

Copyright ©1999-2002, Standard Performance Evaluation Corporation

Sun Microsystems Sun Fire V40z

SPECompMpeak2001 = SPECompMbase2001 =

6486 6344

SPEC license #:HPG0010 Tested by: Sun Microsystems, Santa Clara Test site: Menlo Park Test date: Feb-2005 Hardware Avail:Apr-2005 Software Avail:Apr-2005

Notes/Tuning Information (Continued)

 Portability Flags:
   318.galgel_m      : -fixedform -extend_source
   330.art_m         : Extra Flag: -DINTS_PER_CACHELINE=16 -DDBLS_PER_CACHELINE=8

 Base and Peak User Environment:
   export OMP_NUM_THREADS=2
   export OMP_GUIDED_CHUNK_MAX=300
   ulimit -s unlimited

 Default BIOS settings used; Only 2 CPUs were present on the system.

 For a description of PathScale EKOPath Compiler Suite, Release 2.1 flags,
 portability flags and system parameters used to generate this result,
 please refer to SUN-20050302-PathScale2.1-SuSE-opteron.txt file in the
 flags directory.