Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec OMPM2001 Result

Copyright ©1999-2002, Standard Performance Evaluation Corporation

Hewlett-Packard Company

ProLiant DL585 (AMD Opteron (TM) 880)

SPECompMpeak2001 = SPECompMbase2001 =

17948 16621

SPEC license #:HPG0001 Tested by: Hewlett-Packard Company Test site: Austin, Texas Test date: Oct-2005 Hardware Avail:Sep-2005 Software Avail:Oct-2005

Benchmark

Reference

Time

Base Runtime

Base Ratio

Peak Runtime

Peak Ratio 20000 40000 60000

310.wupwise_m 6000 233 25723 224 26830

312.swim_m 6000 441 13606 375 15992

314.mgrid_m 7300 425 17181 418 17457

316.applu_m 4000 423 9460 302 13241

318.galgel_m 5100 334 15281 314 16249

320.equake_m 2600 135 19249 127 20513

324.apsi_m 3400 165 20613 161 21095

326.gafort_m 8700 538 16183 512 16978

328.fma3d_m 4600 428 10744 399 11536

330.art_m 6400 136 47031 136 47031

332.ammp_m 7000 738 9482 722 9694

Hardware

CPU: AMD Opteron (TM) 880 CPU MHz: 2400 FPU: Integrated CPU(s) enabled: 8 cores, 4 chips, 2 cores/chip CPU(s) orderable: 1,2,4 Primary Cache: 64KBI + 64KBD on chip Secondary Cache: 1024KB (I+D) on chip L3 Cache: None Other Cache: None Memory: 16x1GB, PC3200 CL3 DDR SDRAM ECC Registered Disk Subsystem: SCSI, 36GB, 15K RPM Other Hardware: None

Software

OpenMP Threads: 8 Parallel: OpenMP Operating System: RedHat Enterprise Linux, Advanced Server version 4 (2) Compiler: PathScale EKO Compiler Suite, Release 2.2.1 File System: ext3 System State: Multi-User

Notes/Tuning Information

 Environemnt Settings:
  export PSC_OMP_AFFINITY=TRUE
  export PSC_OMP_AFFINITY_MAP=0,1,2,3,4,5,6,7
  export PSC_OMP_STATIC_FAIR=TRUE
  export PSC_OMP_THREAD_SPIN=1000000000
  export OMP_DYNAMIC=FALSE
  export OMP_NUM_THREADS=8
  ONESTEP=yes for base and peak
  ulimit -s unlimited

 Machine Configuration
  DL585 BIOS version 4.12 A01 - 8/26/2005
  chkconfig --levels 12345 cpuspeed off

 Baseline optimization flags:
  COPTIMIZE = -mp -Ofast
  FOPTIMIZE = -mp -Ofast -OPT:early_mp=on -mcmodel=medium

 Peak optimization flags:
    310.wupwise_m: -mp -Ofast -msse3 -LNO:prefetch_ahead=5:prefetch=3
             -OPT:unroll_times_max=8:unroll_size=128:IEEE_NaN_Inf=off:ro=3
             -IPA:linear=on:plimit=50000:callee_limit=5000

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec OMPM2001 Result

Copyright ©1999-2002, Standard Performance Evaluation Corporation

Hewlett-Packard Company

ProLiant DL585 (AMD Opteron (TM) 880)

SPECompMpeak2001 = SPECompMbase2001 =

17948 16621

SPEC license #:HPG0001 Tested by: Hewlett-Packard Company Test site: Austin, Texas Test date: Oct-2005 Hardware Avail:Sep-2005 Software Avail:Oct-2005

Notes/Tuning Information (Continued)

             -INLINE:aggressive=on
    312.swim_m: -mp -O3 -OPT:Ofast -m3dnow -mcmodel=medium -LNO:simd=0
    314.mgrid_m: -mp -Ofast -CG:gcm=off:cflow=off -LNO:fusion=2:prefetch=0
             -msse3 -OPT:early_mp=on:unroll_times_max=8:unroll_size=256:ro=3
             -mcmodel=medium
    316.applu_m: -mp -Ofast -mcmodel=medium -CG:local_fwd_sched=on
             -LNO:fusion=2:fission=2:full_unroll_size=10000:prefetch=3
             -TENV:X=3
           use_submit_for_speed=1
             submit= numactl --interleave=0,1,2,3 $command
    318.galgel_m: -mp -Ofast -OPT:early_mp=on -OPT:fast_complex=on +ACML
     RM_SOURCES=lapak.f90
     -L<acml2.7.0-install-dir>/pathscale64_mp/lib -lacml
     -I<acml2.7.0-install-dir>/pathscale64_mp/include
    320.equake_m: -Ofast -mp -OPT:alias=disjoint
    324.apsi_m: -mp -O3 -OPT:Ofast -TENV:x=4 -LNO:fusion=2:prefetch=0
    326.gafort_m: -Ofast -OPT:early_mp=on -mp -LNO:vintr=0
    328.fma3d_m: -mp -O2 -ipa -CG:load_exe=1 -OPT:Ofast:IEEE_arith=3:ro=3
             -WOPT:mem_opnds=on:retype_expr=on -IPA:pu_reorder=1
    330.art_m: basepeak=yes
    332.ammp_m: -mp -O3 -OPT:alias=disjoint:unroll_times_max=8:Ofast:ro=3
             -fno-math-errno -TENV:X=4 -LNO:prefetch=0
           use_submit_for_speed=1
              submit= PSC_OMP_GUIDED_CHUNK_MAX=700 $command

    Portability Flags:
        318.galgel_m: -fixedform -extend_source

    Extra Flags:
        330.art_m: -DINTS_PER_CACHELINE=16 -DDBLS_PER_CACHELINE=8

 Alternate Source:
       330.art_m         : Required srcalt purdue1 used for base and peak
       310.wupwise_m     : Approved srcalt ompl.32 used for peak
       312.swim_m        : Approved srcalt ompl.32 used for peak
       314.mgrid_m       : Approved srcalt ompl    used for peak
       320.equake_m      : Approved srcalt ompl.32 used for peak
       324.apsi_m        : Approved srcalt ompl    used for peak

Math library acml2.7.0 available via download
    http://developer.amd.com/acml.aspx
        file = acml-2-7-0-pathscale-64bit.tgz
    Use the +ACML option to select this library.

For a description of Pathscale Compiler and portability
flags and system parameters used to generate this result,
please refer to HP-Pathscale-20051026.txt file in the flags directory.