Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec OMPL2001 Result

Copyright ©1999-2002, Standard Performance Evaluation Corporation

IBM Corporation

IBM System p5 595 (2300 MHz, 64 CPU)

SPECompLpeak2001 = SPECompLbase2001 =

1056459 1005583

SPEC license #:HPG0005 Tested by: IBM Austin Test site: Austin, TX Test date: Jul-2006 Hardware Avail:Aug-2006 Software Avail:Aug-2006

Benchmark

Reference

Time

Base Runtime

Base Ratio

Peak Runtime

Peak Ratio 2000000 4000000

311.wupwise_l 9200 96.4 1526710 96.5 1524700

313.swim_l 12500 226 883307 192 1042300

315.mgrid_l 13500 238 906926 238 906150

317.applu_l 13500 151 1434136 151 1434136

321.equake_l 13000 534 389228 397 523692

325.apsi_l 10500 203 826038 195 862658

327.gafort_l 11000 218 808117 230 763663

329.fma3d_l 23500 583 644540 581 647645

331.art_l 25000 112 3579341 113 3552658

Hardware

CPU: POWER5+ CPU MHz: 2300 FPU: Integrated CPU(s) enabled: 64 cores, 32 chips, 2 cores/chip (SMT on) CPU(s) orderable: 16,32,48,64 cores Primary Cache: 64 KB I + 32 KB D on chip per core Secondary Cache: 1920 KB I+D on chip per chip L3 Cache: 36 MB I+D off chip per chip, 32 chips per SUT Other Cache: None Memory: 256 GB (64x4 GB) Disk Subsystem: 2x73GB SCSI, 15K RPM Other Hardware: None

Software

OpenMP Threads: 128 Parallel: OpenMP Operating System: AIX 5L V5.3 Compiler: XL C/C++ Enterprise Edition Version 8.0 for AIX

XL Fortran Enterprise Edition Version 10.1 for AIX Other Software: ESSL 4.2.0.4

File System: AIX/JFS2 System State: Multi-user

Notes/Tuning Information

 Portability Flags & Environment Variables
   -qfixed used in: 311.wupwise_l, 313.swim_l, 315.mgrid_l, 317.applu_l, 325.apsi_l
   -qsuffix=f=f90 used in: 327.gafort_l, 329.fma3d_l

 Base Flags

   C:       -q64 -O5 -qsmp=omp -lmass -btextpsize:64K -bdatapsize:64K -bstackpsize:64K -qalign=natural

   FORTRAN: -q64 -O5 -qsmp=omp -lmass -btextpsize:64K -bdatapsize:64K -bstackpsize:64K

 Base & Peak User Environment:
   MEMORY_AFFINITY=MCM
   OMP_DYNAMIC=TRUE
   XLSMPOPTS=SPINS=0:YIELDS=0:STACK=8000000:SCHEDULE=STATIC:STARTPROC=0:STRIDE=1
   OMP_NUM_THREADS=128
   XLFRTEOPTS=intrinthds=1
   MALLOCMULTIHEAP=1

 Peak Flags:
   -qsmp=omp used in all cases
   311.wupwise_l:    -q64 -O5 -lmass -btextpsize:64K -bdatapsize:64K -bstackpsize:64K
                     OMP_DYNAMIC = FALSE

   313.swim_l:       -O5 -qipa=noobject -qmaxmem=-1 -q64 -btextpsize:64K -bdatapsize:64K -bstackpsize:64K

                     OMP_DYNAMIC = FALSE
                     OMP_NUM_THREADS=64

                     XLSMPOPTS=SPINS=0:YIELDS=0:STACK=8000000:SCHEDULE=STATIC:STARTPROC=0:STRIDE=2

   315.mgrid_l:      -q64 -O5 -lmass -btextpsize:64K -bdatapsize:64K -bstackpsize:64K

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec OMPL2001 Result

Copyright ©1999-2002, Standard Performance Evaluation Corporation

IBM Corporation

IBM System p5 595 (2300 MHz, 64 CPU)

SPECompLpeak2001 = SPECompLbase2001 =

1056459 1005583

SPEC license #:HPG0005 Tested by: IBM Austin Test site: Austin, TX Test date: Jul-2006 Hardware Avail:Aug-2006 Software Avail:Aug-2006

Notes/Tuning Information (Continued)

                     ENV_OMP_DYNAMIC = FALSE
   317.applu_l:      basepeak=1
   321.equake_l:     -q64 -O5 -lmass -btextpsize:64K -bdatapsize:64K -bstackpsize:64K
                     OMP_DYNAMIC = FALSE
                     OMP_NUM_THREADS=64

                     XLSMPOPTS=SPINS=0:YIELDS=0:STACK=8000000:SCHEDULE=STATIC:STARTPROC=0:STRIDE=2

   324.apsi_l:       -q64 -O5 -lmass -btextpsize:64K -bdatapsize:64K -bstackpsize:64K
                     OMP_DYNAMIC = FALSE
   327.gafort_l:     -q64 -O5 -lmass
                     OMP_DYNAMIC = FALSE
   329.fma3d_l:      -q64 -O5 -lmass -btextpsize:64K -bdatapsize:64K -bstackpsize:64K
                     OMP_DYNAMIC = FALSE

   330.art_m:        -O5 -qipa=noobject -qmaxmem=-1 -q64 -btextpsize:64K -bdatapsize:64K -bstackpsize:64K

                     EXTRA_CFLAGS= -DINTS_PER_CACHELINE=32 -DDBLS_PER_CACHELINE=16
                     OMP_DYNAMIC = FALSE

 _{The installed OS level is AIX 5L for POWER version 5.3 with the 5300-04 Recommended Maintenence package.}

  The installed C/C++ compiler is XL C/C++ Enterprise Edition Version 8.0 for AIX with the August 2006 PTF.
  The installed Fortran copiler is XL Fortran Enterprise Edition Version 10.1 with the August 2006 AIX PTF.

  SMT:  Acronym for "Simultaneous Multi-Threading". A processor technology that allows
        the simultaneous execution of multiple thread contexts within a single processor
        core. (Enabled by default)
  SUT:  Acronym for "System Under Test"
  ESSL: Engineering and Scientific Subroutine Library
  PTF:  IBM identifier for "Program Fix Level"

  C:        IBM XL C for AIX invoked as xlc_r
  Fortran:  IBM XL Fortran for AIX invoked as xlf_r

  ulimits set to unlimited.
  Large page mode and memory affinity were set as follows:
      vmo -r -o lgpg_regions=8192 -o lgpg_size=16777216
      chuser capabilities=CAP_BYPASS_RAC_VMM,CAP_PROPAGATE $USER
      bosboot -aD
      shutdown -rF
      export MEMORY_AFFINITY=MCM