Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec OMPL2001 Result

Copyright ©1999-2002, Standard Performance Evaluation Corporation

Hewlett-Packard DL585 G2

SPECompLpeak2001 = SPECompLbase2001 =

102283 99907

SPEC license #:HPG0001 Tested by: Hewlett-Packard Test site:Hewlett-Packard, Houston Test date: Feb-2007 Hardware Avail:Sep-2006 Software Avail:Aug-2006

Benchmark

Reference

Time

Base Runtime

Base Ratio

Peak Runtime

Peak Ratio 200000 400000 600000

311.wupwise_l 9200 1118 131699 1035 142212

313.swim_l 12500 2382 83972 2364 84614

315.mgrid_l 13500 1764 122426 1764 122426

317.applu_l 13500 4963 43518 4827 44752

321.equake_l 13000 2721 76448 2632 79016

325.apsi_l 10500 2634 63784 2634 63784

327.gafort_l 11000 1505 116948 1505 116948

329.fma3d_l 23500 4535 82906 4245 88572

331.art_l 25000 1124 356000 1124 356000

Hardware

CPU: AMD Opteron (TM) 8220SE CPU MHz: 2800 FPU: Integrated CPU(s) enabled: 8 cores, 4 chips, 2 cores/chip CPU(s) orderable: 2,4 chips Primary Cache: 64 KB I + 64 KB D on chip per core Secondary Cache: 1 MB I + D on chip per core L3 Cache: None Other Cache: None Memory: 32 GB (16x2 GB PC2-5300P CL5) Disk Subsystem: 1x72 GB 10 K SAS Other Hardware: None

Software

OpenMP Threads: 8 Parallel: OpenMP Operating System: RedHat Enterprise Linux 4.0 Advanced Server for AMD64/EM64T,

Update 4, Kernel 2.6.9-42.ELsmp

Compiler: QLogic PathScale Compiler Suite, Release 2.5 File System: ext2 System State: Multi-user run level 3

Notes/Tuning Information

 User environment:
 export PSC_OMP_STATIC_FAIR=TRUE
 export PSC_OMP_THREAD_SPIN=1000000000
 export PSC_OMP_AFFINITY=TRUE
 export OMP_DYNAMIC=FALSE
 export OMP_NUM_THREADS=8
 ulimit -s unlimited
 chkconfig --levels 12345 cpuspeed off
 DL585 G2 BIOS version A07 - 12/02/2006

 Baseline optimization flags:
   C programs:       -Ofast -mp
   Fortran programs: -Ofast -OPT:early_mp=on -mcmodel=medium -mp
 Peak optimization flags:
    311.wupwise_l: -mp -Ofast -msse3 -LNO:prefetch_ahead=5:prefetch=3
                   -OPT:unroll_times_max=8:unroll_size=128:IEEE_NaN_Inf=off:ro=3
                   -IPA:linear=on:plimit=50000:callee_limit=5000 -INLINE:aggressive=on
    313.swim_l:    -mp -O3 -OPT:Ofast -m3dnow -mcmodel=medium -LNO:simd=0
    315.mgrid_l:   basepeak=yes
    317.applu_l:   -mp -Ofast -mcmodel=medium -CG:local_fwd_sched=on
                   -LNO:fusion=2:fission=2:full_unroll_size=10000:prefetch=3 -TENV:X=3
    321.equake_l:  -Ofast -mp -OPT:alias=disjoint
    325.apsi_l:    basepeak=yes
    327.gafort_l:  basepeak=yes
    329.fma3d_l:   -mp -O2 -ipa -CG:load_exe=1

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec OMPL2001 Result

Copyright ©1999-2002, Standard Performance Evaluation Corporation

Hewlett-Packard DL585 G2

SPECompLpeak2001 = SPECompLbase2001 =

102283 99907

SPEC license #:HPG0001 Tested by: Hewlett-Packard Test site:Hewlett-Packard, Houston Test date: Feb-2007 Hardware Avail:Sep-2006 Software Avail:Aug-2006

Notes/Tuning Information (Continued)

                   -OPT:Ofast:early_mp=on:IEEE_arith=3:ro=3 -WOPT:mem_opnds=on:retype_expr=on
                   -IPA:pu_reorder=1
    331.art_l:     basepeak=yes
Flags description:  HP-20070228-PathScale25.v3.txt