Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec OMPM2001 Result

Copyright 1999-2008, Standard Performance Evaluation Corporation

Sun Microsystems Sun Fire X2250

SPECompMpeak2001 =

SPECompMbase2001 =

17195

16478

SPEC license #:HPG0010 Tested by: Sun Microsystems Test site: Menlo Park Test date: Apr-2009 Hardware Avail:Apr-2009 Software Avail:Nov-2008

Benchmark

Reference

Time

Base Runtime

Base Ratio

Peak Runtime

Peak Ratio 20000 40000 60000

310.wupwise_m 6000 313 19163 312 19206

312.swim_m 6000 629 9540 628 9560

314.mgrid_m 7300 598 12207 599 12188

316.applu_m 4000 368 10860 351 11407

318.galgel_m 5100 310 16460 263 19365

320.equake_m 2600 178 14590 168 15462

324.apsi_m 3400 131 25902 127 26857

326.gafort_m 8700 513 16946 509 17097

328.fma3d_m 4600 299 15404 284 16200

330.art_m 6400 191 33583 178 36029

332.ammp_m 7000 380 18397 369 18968

Hardware

CPU: Intel Xeon X5482 CPU MHz: 3200 FPU: Integrated CPU(s) enabled: 8 cores, 2 chips, 4 cores/chip CPU(s) orderable: 1,2 chips Primary Cache: 32 KB I + 32 KB D on chip per core Secondary Cache: 12 MB I+D on chip per chip, 6 MB shared / 2 cores L3 Cache: None Other Cache: None Memory: 16 GB (4x4GB Dual-rank PC2-6400 CL5-5-5 FB-DIMMs) Disk Subsystem: 1 x 250 GB SATA 7200 RPM Other Hardware: None

Software

OpenMP Threads: 8 Parallel: OpenMP and Automatic parallel Operating System: OpenSolaris 2008.05 Compiler: Sun Studio Express 11/08 File System: zfs System State: Multi-User

Notes/Tuning Information

 Compiler Invocation:
   C   : cc
   F90 : f90
   F77 : f90

 Base tuning:
   Fortran :  -fast  -xautopar -xopenmp -xipo=2  -xvector=lib
              -m64 -aligncommon=16  -fns=no -lmtmalloc
   C       :  -fast -xopenmp -xautopar -xipo=2 -xvector=lib -xprefetch
              -xprefetch_level=3 -m64 -lmtmalloc
   ONESTEP=yes

 Peak tuning:
  ONESTEP=yes for all peak tests.

  310.wupwise_m   : -fast -xautopar -xopenmp -xipo=2 -xvector=lib
                    -xprefetch -xprefetch_level=3 -m64 -lmtmalloc
  312.swim_m      : -fast -xmodel=medium -Qoption ube -fsimple=3
                    -xipo=2 -m64 -xvector=simd -xopenmp -lmvec
                     srcalt = ompl.32
  314.mgrid_m     : -fast -xopenmp -xautopar -xipo=2 -xvector=lib
                    -xprefetch -xprefetch_level=3 -m64 -lmtmalloc
  316.applu_m     : -fast -xopenmp -xautopar -xipo=2 -xvector=lib -xprefetch

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec OMPM2001 Result

Copyright 1999-2008, Standard Performance Evaluation Corporation

Sun Microsystems Sun Fire X2250

SPECompMpeak2001 =

SPECompMbase2001 =

17195

16478

SPEC license #:HPG0010 Tested by: Sun Microsystems Test site: Menlo Park Test date: Apr-2009 Hardware Avail:Apr-2009 Software Avail:Nov-2008

Notes/Tuning Information (Continued)

                    -xprefetch_level=3 -m64 -xmodel=medium -lmtmalloc
                     srcalt = ompl
  318.galgel_m    : -O3 -xpagesize=2M -xipo=2 -xvector=simd -m64 -xopenmp
                    -xlic_lib=sunperf +FDO
                     RM_SOURCES=lapak.f90
  320.equake_m    : -fast -fns=no -xalias_level=layout -xdepend=no
                    -m64 -xopenmp -lmvec
                    srcalt = ompl.32
  324.apsi_m      : -fast -xipo=2 -m64 -xprefetch_level=3 -xvector
                    -xopenmp -lmtmalloc
                    srcalt = ompl.32
  326.gafort_m    : -fast -fstore  -aligncommon=8 -xpagesize=2M -m64
                    -xipo=2 -xvector=simd -xopenmp -lmvec
  328.fma3d_m     : -fast -xipo=2 -m64 -xvector=simd -xopenmp
                    srcalt = ompl.32
  330.art_m       : -fast -xipo=2 -m64 -xopenmp
  332.ammp_m      : -fast -xautopar -xipo=2 -xvector=simd -m64
                    -Wu,-fsimple=3 -xopenmp -xpagesize=2M

 Portability flags:
   318.galgel_m   : -e -fixed

 Extra art allowed flags:
   330.art_m      : -DINTS_PER_CACHELINE=16 -DDBLS_PER_CACHELINE=8

 Base and Peak User Environment:
   export OMP_NUM_THREADS=16
   export SUNW_MP_PROCBIND=TRUE
   export SUNW_MP_THR_IDLE=SPIN
   export OMP_NESTED=FALSE
   export STACKSIZE=16384
   export OMP_DYNAMIC=TRUE
   ulimit -s unlimited

 For a description of Sun Studio 10 Compiler flags, portability flags
 and system parameters used to generate this result, please refer to
 SUN-20090504-Studio-Solaris-X86_64.txt file in the flags directory.

 Default BIOS settings used.