Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CINT2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

Sun Microsystems Sun Enterprise 450

SPECint2000 = SPECint_base2000 = 234 225 SPEC license #: 6 Tested by: Sun Microsystems, Palo Alto Test date: Aug-2000 Hardware Avail: Aug-2000 Software Avail: Oct-2000

Benchmark

Reference

Time

Base Runtime

Base Ratio Runtime Ratio 100 200 300 400 500

164.gzip 1400 851 165 851 165

175.vpr 1400 662 212 634 221

176.gcc 1100 474 232 470 234

181.mcf 1800 506 356 499 361

186.crafty 1000 571 175 571 175

197.parser 1800 853 211 829 217

252.eon 1300 622 209 608 214

253.perlbmk 1800 729 247 706 255

254.gap 1100 642 171 642 171

255.vortex 1900 626 304 506 375

256.bzip2 1500 633 237 614 244

300.twolf 3000 1235 243 1110 270

Hardware

CPU: UltraSPARC II CPU MHz: 480 FPU: Integrated CPU(s) enabled: 1 core, 1 chip, 1 core/chip CPU(s) orderable: 1 to 4 Parallel: None Primary Cache: 16KBI+16KBD on chip Secondary Cache: 8MB(I+D) off chip L3 Cache: None Other Cache: None Memory: 512MB Disk Subsystem: 2*9.1GB(7200 RPM)

Other Hardware:

Software

Operating System: Solaris 8 Compiler: Forte Developer 6 update 1

File System: UFS System State: single user

Notes/Tuning Information

 Portability: 176.gcc: -Dalloca=__builtin_alloca -DHOST_WORDS_BIG_ENDIAN
 Portability: 186.crafty: -DSUN
 Portability: 252.eon: -library=iostream,no%Cstd
 Portability: 253.perlbmk: -DSPEC_CPU2000_SOLARIS

 Portability: 254.gap: -DSYS_IS_USG -DSYS_HAS_TIME_PROTO -DSYS_HAS_SIGNAL_PROTO -DSYS_HAS_CALLOC_PROTO -DSYS_HAS_IOCTL_PROTO

 Base C   flags: -fast -xcrossfile -xprofile
 Base C++ flags: -fast -xcrossfile -xprofile

 Peak flags:
   164.gzip   : -fast -xcrossfile -xprofile
   175.vpr    : -fast -xalias_level=std -xcrossfile -xprofile -dn
   176.gcc    : -fast -xcrossfile -xprofile -dn
   181.mcf    : -fast -xcrossfile -xprofile -dn
   186.crafty : -fast -xcrossfile -xprofile
   197.parser : -fast -xalias_level=std -xcrossfile -xprofile -dn
   252.eon    : -fast -xcrossfile -xprofile -dn

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CINT2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

Sun Microsystems Sun Enterprise 450

SPECint2000 = SPECint_base2000 = 234 225 SPEC license #: 6 Tested by: Sun Microsystems, Palo Alto Test date: Aug-2000 Hardware Avail: Aug-2000 Software Avail: Oct-2000

Notes/Tuning Information (Continued)

   253.perlbmk: -fast -xalias_level=std -xcrossfile -xprofile -dn
   254.gap    : -fast -xcrossfile -xprofile

   255.vortex : -fast -xsafe=mem -xcrossfile -W2,-Mt500,-Mr6000,-crit -xalias_level=std -xprofile -dn
   256.bzip2  : -fast -xarch=v8 -W2,-Abopt -xcrossfile -xalias_level=std -Wc,-Qiselect-funcalign=32 -xprofile -dn

   300.twolf  : -fast -xO5 -xarch=v8plus -W2,-whole -xprofile
 Proper operation of -xcrossfile requires simultaneous presentation of all source
 files to the compiler.  This is accomplished within the SPECcpu2000 suite by
 setting ONESTEP = yes.