Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CINT2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

Sun Microsystems Sun Fire 6800

SPECint2000 = SPECint_base2000 = -- 360 SPEC license #: 597 Tested by: Verlag Heinz Heise (iX) Test date: May-2001 Hardware Avail: Mar-2001 Software Avail: May-2001

Benchmark

Reference

Time

Base Runtime

Base Ratio Runtime Ratio 100 200 300 400 500

164.gzip 1400 466 300

175.vpr 1400 455 307

176.gcc 1100 323 341

181.mcf 1800 488 369

186.crafty 1000 243 412

197.parser 1800 506 355

252.eon 1300 340 382

253.perlbmk 1800 483 373

254.gap 1100 470 234

255.vortex 1900 408 466

256.bzip2 1500 338 444

300.twolf 3000 746 402

Hardware

CPU: UltraSPARC-III CPU MHz: 750 FPU: Integrated CPU(s) enabled: 24 cores, 24 chips, 1 core/chip CPU(s) orderable: 2-24 Parallel: No Primary Cache: 32KBI+64KBD on chip Secondary Cache: 8MB(I+D) off chip L3 Cache: None Other Cache: None Memory: 48GB Disk Subsystem: 8x36GB (RAID 10)

Other Hardware:

Software

Operating System: Solaris 8 Compiler: Forte Developer 6 update 2 C 5.3

File System: UFS System State: Multi User

Notes/Tuning Information

 Portability: 252.eon: -library=iostream,no%Cstd

 C   flags: -fast -xcrossfile -xprofile
 C++ flags: -fast -xcrossfile -xprofile