Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

Hewlett-Packard Company hp workstation j6750

SPECfp2000 = SPECfp_base2000 = 651 580 SPEC license #: 3 Tested by: HP Test date: Oct-2002 Hardware Avail: Nov-2002 Software Avail: Aug-2002

Benchmark

Reference

Time

Base Runtime

Base Ratio Runtime Ratio 500 1000 1500 2000

168.wupwise 1600 364 439 224 715

171.swim 3100 363 854 363 854

172.mgrid 1800 318 565 318 565

173.applu 2100 322 652 322 652

177.mesa 1400 201 697 201 695

178.galgel 2900 187 1553 187 1553

179.art 2600 414 627 244 1064

183.equake 1300 323 402 250 520

187.facerec 1900 447 425 432 440

188.ammp 2200 407 540 359 613

189.lucas 2000 446 448 428 467

191.fma3d 2100 530 396 525 400

200.sixtrack 1100 233 472 206 534

301.apsi 2600 386 674 386 674

Hardware

CPU: PA-8700+ CPU MHz: 875 FPU: Integrated CPU(s) enabled: 1 core, 1 chip, 1 core/chip CPU(s) orderable: 1 to 2 Parallel: No Primary Cache: 0.75MB(I) + 1.5MB(D) on chip Secondary Cache: None L3 Cache: None Other Cache: None Memory: 1GB (4x256MB DIMMs total) Disk Subsystem: 1x36 GB SCSI 15K Other Hardware: None

Software

Operating System: HP-UX 11i TCOE B.11.11.0206 Compiler: HP ANSI C 11.11.04 (Dec 2001 bundle)

HP aC++ Compiler C.03.33.01 (Dec 2001 bundle) Fortran90 11.11.47 (patch PHSS_25772) PHSS_24207 libm patch

File System: VxFS System State: Multi-user

Notes/Tuning Information

  Portability flags:
   178.galgel: +source=fixed

 Baseline compile flags:
   fortran: +O3 +Onofltacc -Wl,-a,archive -Wl,+FPD
   C      : +I/+P +O4 +Odataprefetch -Wl,-a,archive

 Peak compile flags:
   168.wupwise: (ONESTEP) +cat +O3 +Odataprefetch +Onofltacc
                -Wl,+FPD -Wl,-a,archive
   171.swim: basepeak=true
   172.mgrid: basepeak=true
   173.applu: basepeak=true
   177.mesa: +I/+P +Oall +Odataprefetch +Opromote_indirect_calls
             -Wl,+FPD -Wl,-a,archive
   178.galgel: basepeak=true

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

Hewlett-Packard Company hp workstation j6750

SPECfp2000 = SPECfp_base2000 = 651 580 SPEC license #: 3 Tested by: HP Test date: Oct-2002 Hardware Avail: Nov-2002 Software Avail: Aug-2002

Notes/Tuning Information (Continued)

   179.art: +I/+P +Oall +Onodataprefetch +Onofltacc +Optrs_strongly_typed
            +Opromote_indirect_calls -Wl,+FPD -Wl,-a,archive
   183.equake: +O4 +Olibcalls +Odataprefetch +Optrs_strongly_typed
               +Opromote_indirect_calls -Wl,+FPD -Wl,-a,archive
   187.facerec: (ONESTEP) +cat +O3 +Ofastaccess -Wl,+FPD -Wl,-a,archive
   188.ammp: +I/+P +Oall +Odataprefetch +Optrs_strongly_typed
             +Opromote_indirect_calls -Wl,+FPD -Wl,-a,archive
   189.lucas: +O3 +Onoinline -Wl,+FPD -Wl,-a,archive
   191.fma3d: +O3 +Onolimit -Wl,+FPD -Wl,-a,archive
   200.sixtrack: (ONESTEP) +cat +O3 +Onolibcalls +Onolimit +Onoinline
                 +Onodataprefetch -Wl,+FPD -Wl,-a,archive
   301.apsi: basepeak=true

 Operating system configuration notes:

   vps_pagesize 4096, vps_ceiling 16384
   dbc_min_pct=20, dbc_max_pct=20
   maxssiz=0x10000000
   second CPU disabled at boot: co cpu 1 off