Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

Bull NovaScale 4040

SPECfp2000 = SPECfp_base2000 =

1404 1391

SPEC license #: 20 Tested by: JFL Test date: Feb-2003 Hardware Avail: Apr-2003 Software Avail: Apr-2003

Benchmark

Reference

Time

Base Runtime

Base Ratio Runtime Ratio 2000 4000 6000 8000

168.wupwise 1600 167 959 167 959

171.swim 3100 97.1 3194 97.1 3194

172.mgrid 1800 103 1745 101 1784

173.applu 2100 90.5 2320 90.5 2320

177.mesa 1400 194 723 194 723

178.galgel 2900 120 2410 120 2410

179.art 2600 59.6 4365 59.6 4365

183.equake 1300 79.3 1639 79.3 1639

187.facerec 1900 154 1232 154 1232

188.ammp 2200 249 884 249 884

189.lucas 2000 142 1409 137 1462

191.fma3d 2100 281 749 281 749

200.sixtrack 1100 124 889 124 889

301.apsi 2600 405 642 377 690

Hardware

CPU: Itanium 2 processor 1000 MHz CPU MHz: 1000 FPU: Integrated CPU(s) enabled: 1 core, 1 chip, 1 core/chip CPU(s) orderable: 1 to 4 Parallel: No Primary Cache: 16KBI + 16KBD on chip Secondary Cache: 256KB(I+D) on chip L3 Cache: 3MB (I+D) off chip Other Cache: N/A Memory: 2 GB (16 * 256 MB DIMMs) Disk Subsystem: 1 SCSI Maxtor 10krpm Other Hardware:

Software

Operating System: Linux 64 bit : Red Hat Advanced Server 2.1 Compiler: Intel C++ & Fortan Compilers 7.0 for Linux64 Build 20030213 File System: ext2 System State: Single User

Notes/Tuning Information

 +FDO: PASS1=-prof_gen  PASS2=-prof_use
 Base tuning:
 C programs:       -ipo -O3 +FDO -ansi_alias
 Fortran programs: -ipo -O3 +FDO
 Portability:
 178.galgel: -FI
 4 CPU machine with only 1 CPU enabled thanks to boot Linux
 with option maxcpus=0 (ie=UP kernel) in elilo.conf
168.wupwise: +FDO -ipo -O3 -ansi_alias -IPF_fltacc -IPF_flt_eval_method0 -static -ftz
171.swim: +FDO -ipo -O3 (basepeak=yes)
172.mgrid: -O3 -ipo -ansi_alias -IPF_fltacc -IPF_flt_eval_method0 -ftz
173.applu: +FDO -ipo -O3  (basepeak=yes)
177.mesa: +FDO -ipo -O3  (basepeak=yes)
178.galgel: +FDO -ipo -O3  (basepeak=yes)
179.art: +FDO -ipo -O3 -ansi_alias (basepeak=yes)
183.equake: +FDO -ipo -O3 (basepeak=yes)
187.facerec: +FDO -ipo -O3  (basepeak=yes)

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

Bull NovaScale 4040

SPECfp2000 = SPECfp_base2000 =

1404 1391

SPEC license #: 20 Tested by: JFL Test date: Feb-2003 Hardware Avail: Apr-2003 Software Avail: Apr-2003

Notes/Tuning Information (Continued)

188.ammp: +FDO -ipo -O3 (basepeak=yes)
189.lucas: -O3 -ipo -ansi_alias -IPF_fltacc -IPF_flt_eval_method0 -ftz
191.fma3d: +FDO -ipo -O3  (basepeak=yes)
200.sixtrack: +FDO -O3 -ipo (basepeak=yes)
301.apsi: -O3 -ipo -ansi_alias -IPF_fltacc -IPF_flt_eval_method0 -ftz