Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CINT2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

Einux A4800

SPECint2000 = SPECint_base2000 = -- 1045

SPEC license #: 49 Tested by: AMD Austin TX Test date: Apr-2003 Hardware Avail: Jul-2003 Software Avail: May-2003

Benchmark

Reference

Time

Base Runtime

Base Ratio Runtime Ratio 500 1000 1500 2000

164.gzip 1400 151 927

175.vpr 1400 146 957

176.gcc 1100 85.9 1280

181.mcf 1800 310 581

186.crafty 1000 64.0 1562

197.parser 1800 209 863

252.eon 1300 87.7 1483

253.perlbmk 1800 156 1151

254.gap 1100 114 965

255.vortex 1900 159 1192

256.bzip2 1500 154 972

300.twolf 3000 301 997

Hardware

CPU: AMD Opteron 144, 1.8 GHz CPU MHz: 1800 FPU: Integrated CPU(s) enabled: 1 core, 1 chip, 1 core/chip CPU(s) orderable: 1,2,4 Parallel: No Primary Cache: 64KBI + 64KBD on chip Secondary Cache: 1 MB(I+D) L3 Cache: N/A Other Cache: N/A Memory: 4x512MB PC2700 DDR ECC Registered SDRAM CL2.5 Disk Subsystem: IDE 7200 RPM Other Hardware: None

Software

Operating System: SuSE Linux Enterprise Server 8 for AMD64 Compiler: SuSE optional package gcc33 File System: ext2 System State: Run level 3

Notes/Tuning Information

 +FDO: PASS1=-fprofile-arcs PASS2=-fbranch-probabilities
 Portability:
                  PORTABILITY=-DSPEC_CPU2000_LP64 is applied to all benchmarks.
  176.gcc:        Approved src.alt is used
  186.crafty:     EXTRA_CFLAGS=-DLINUX_i386
  252.eon:        EXTRA_CXXFLAGS=-DHAS_ERRLIST -DFMAX_IS_DOUBLE
  253.perlbmk:    EXTRA_CFLAGS=-DSPEC_CPU2000_LINUX_I386 -DSPEC_CPU2000_NEED_BOOL
                               -DSPEC_CPU2000_GLIBC22
  254.gap:        EXTRA_CFLAGS=-DSYS_IS_USG -DSYS_HAS_IOCTL_PROTO -DSYS_HAS_TIME_PROTO
                               -DSYS_HAS_ANSI -DSYS_HAS_CALLOC_PROTO
 Base C flags:    -O3 -funroll-all-loops +FDO
 Base C++ flags:  -O3 -funroll-all-loops +FDO