Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CINT2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

Sun Microsystems Sun Java Workstation W2100z

SPECint2000 = SPECint_base2000 =

1584 1437

SPEC license #: 6 Tested by: Sun Microsystems, Santa Clara Test date: Jun-2004 Hardware Avail: Jul-2004 Software Avail: May-2004

Benchmark

Reference

Time

Base Runtime

Base Ratio Runtime Ratio 1000 2000 3000 4000

164.gzip 1400 96.3 1453 96.1 1457

175.vpr 1400 121 1158 116 1208

176.gcc 1100 66.3 1658 66.3 1658

181.mcf 1800 251 718 159 1129

186.crafty 1000 48.1 2081 48.1 2081

197.parser 1800 164 1097 142 1266

252.eon 1300 75.7 1717 62.7 2073

253.perlbmk 1800 110 1634 102 1771

254.gap 1100 73.9 1488 73.9 1488

255.vortex 1900 80.3 2367 80.3 2367

256.bzip2 1500 112 1334 112 1334

300.twolf 3000 233 1285 179 1673

Hardware

CPU: AMD Opteron (TM) 250 CPU MHz: 2400 FPU: Integrated CPU(s) enabled: 1 core, 1 chip, 1 core/chip CPU(s) orderable: 2 Parallel: No Primary Cache: 64KBI + 64KBD on chip Secondary Cache: 1024KB (I+D) on chip L3 Cache: N/A Other Cache: N/A Memory: 4x1GB, PC3200 CL3 DDR SDRAM ECC Registered Disk Subsystem: SCSI, 73GB, 10K RPM Other Hardware: None

Software

Operating System: Red Hat Enterprise Linux WS 3 (AMD64) Compiler: PathScale EKO Compiler Suite, Release 1.1

Red Hat gcc 3.5 ssa (from RHEL WS 3)

File System: Linux/ext3 System State: Multi-user, Run level 3

Notes/Tuning Information

 Feedback-directed optimization is indicated by "+FDO", which means,
 unless otherwise noted:
      PASS1: -fb_create fbdata
      PASS2: -fb_opt    fbdata

 Compiler: pathcc (PathScale C) unless otherwise noted.
 If other compilers are used, they are indicated as:
    g++     Gnu C++
    pathCC  PathScale C++

 Integer base tuning:
   C programs:       pathcc -O3 -ipa +FDO
   C++ programs:     pathCC -Ofast +FDO

 Peak Tuning:
 164.gzip:     -O3 -ipa -WOPT:val=0 -CG:p2align_freq=10000 +FDO
 175.vpr:      -O2 -ipa -OPT:alias=disjoint -LNO:prefetch_ahead=2
               -CG:p2align_freq=500000 -INLINE:aggressive=on
               -IPA:space=300:plimit=10000:callee_limit=5000:linear=on

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CINT2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

Sun Microsystems Sun Java Workstation W2100z

SPECint2000 = SPECint_base2000 =

1584 1437

SPEC license #: 6 Tested by: Sun Microsystems, Santa Clara Test date: Jun-2004 Hardware Avail: Jul-2004 Software Avail: May-2004

Notes/Tuning Information (Continued)

               +FDO
 176.gcc:      basepeak = true
 181.mcf:      -O3 -static -OPT:Ofast -m32 +FDO
 186.crafty:   basepeak = true
 197.parser:   -O3 -ipa -m32 -IPA:ctype=on +FDO
 252.eon:      g++ -O3 -msse2 -funroll-all-loops -ffast-math
               -finline-limit=5000
               Uses g++ style Feedback Directed Optimization:
                  PASS1: -fprofile-arcs   PASS2: -fbranch-probabilities
               Previous feedback is removed prior to compiles, using:
                  fdo_pre0 = rm -f *.da *.life analyz_prbrob.out
 253.perlbmk:  -O3 -ipa -TENV:X=3 -IPA:min_hotness=5:plimit=20000 +FDO
 254.gap:      basepeak=yes
 255.vortex:   basepeak=yes
 256.bzip2:    basepeak=yes
 300.twolf:    -O2 -OPT:unroll_times=8:unroll_size=256:alias=disjoint:Ofast
               -CG:gcm=off:p2align_freq=100000 -TENV:X=4 +FDO -m32

 Portability:
 186.crafty:  -DLINUX_i386
 252.eon:     -DHAS_ERRLIST  -DSPEC_CPU2000_LP64 -lm
              srcalt = fmax_errno
 253.perlbmk: -DSPEC_CPU2000_LINUX_I386 -DSPEC_CPU2000_NEED_BOOL
              -DSPEC_CPU2000_GLIBC22 -DSPEC_CPU2000_LP64
 254.gap:     -DSYS_IS_USG -DSYS_HAS_IOCTL_PROTO -DSYS_HAS_TIME_PROTO
              -DSYS_HAS_SIGNAL_PROTO -DSYS_HAS_ANSI -DSYS_HAS_CALLOC_PROTO
              -DSPEC_CPU2000_LP64
 255.vortex:  -DSPEC_CPU2000_LP64

 Notes:
      BIOS build A5S1, default setting was used.
      Only one CPU was present in the system, other CPU was physically removed.