Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

Hewlett-Packard Company HP 9000 Model N4000

SPECfp2000 = SPECfp_base2000 = 297 266 SPEC license #: 3 Tested by: Hewlett-Packard Company Test date: Nov-1999 Hardware Avail: Nov-1999 Software Avail: Feb-2000

Benchmark

Reference

Time

Base Runtime

Base Ratio Runtime Ratio 100 200 300 400 500 600

168.wupwise 1600 638 251 513 312

171.swim 3100 553 560 544 570

172.mgrid 1800 523 344 525 343

173.applu 2100 484 434 483 434

177.mesa 1400 602 232 602 233

178.galgel 2900 769 377 770 376

179.art 2600 854 305 631 412

183.equake 1300 666 195 462 282

187.facerec 1900 2456 77.4 1882 101

188.ammp 2200 754 292 687 320

189.lucas 2000 944 212 844 237

191.fma3d 2100 1054 199 1050 200

200.sixtrack 1100 500 220 437 252

301.apsi 2600 662 393 661 393

Hardware

CPU: 440 MHz PA-RISC 8600 CPU MHz: 440 FPU: Integrated CPU(s) enabled: 1 core, 1 chip, 1 core/chip CPU(s) orderable: max config 8 CPUs Parallel: -- Primary Cache: 512KBI+1MBD Secondary Cache: None L3 Cache: None Other Cache: None Memory: 8GB Disk Subsystem: 1 9GB Ultra-SCSI 7200 rpm Other Hardware: --

Software

Operating System: HP-UX B.11.00 Compiler: HP-UX f77 971027 (162928) B.11.00.01 File System: HP-UX VxFS System State: Multi-user

Notes/Tuning Information

Portability flags:
cc: -Ae
168.wupwise: -K
178.galgel: +source=fixed

Base Flags:
f90: +O3   +Odataprefetch +Onofltacc -Wl,+FPD
cc: +Oall +Odataprefetch -Wl,-a,archive +I/+P

Peak flags:
168.wupwise: f77 +DA2.0 +DS2.0 +O4 +Odataprefetch +Onofltacc
171.swim: f77 +DA2.0 +DS2.0 +O4 +Odataprefetch +Ocachepadcommon +Oloop_unroll
172.mgrid: base #basepeak=true
173.applu: base #basepeak=true
177.mesa: base #basepeak=true
178.galgel:base #basepeak=true
179.art: +Oall +Odataprefetch +Onofltacc +Optrs_strongly_typed -Wl,+FPD -Wl,-a,archive +I/+P

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

Hewlett-Packard Company HP 9000 Model N4000

SPECfp2000 = SPECfp_base2000 = 297 266 SPEC license #: 3 Tested by: Hewlett-Packard Company Test date: Nov-1999 Hardware Avail: Nov-1999 Software Avail: Feb-2000

Notes/Tuning Information (Continued)

183.equake: +Oall +Odataprefetch +Optrs_strongly_typed

187.facerec: +O2 +Ofastaccess +Omultiprocessor -Wl,+FPD -Wl,-a,archive -Wl,/opt/langtools/lib/fastmem.o

188.ammp: +Oall +Odataprefetch +Optrs_strongly_typed +I/+P
189.lucas: +O3 +Odataprefetch +Onofltacc +Omultiprocessor
191.fma3d: base #basepeak=true
200.sixtrack: f90 +Oall +Ofastaccess +Oloop_block +Omultiprocessor +Onofltacc
              LIBS = -Wl,+FPD -Wl,-a,archive -Wl,/opt/langtools/lib/fastmem.o
301.apsi: base #basepeak=true