Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

Dell_{Precision WorkStation 420 (1.0 GHz Pentium III)} SPECfp2000 =

SPECfp_base2000 = 304 292 SPEC license #: 55 Tested by: Dell, Round Rock, TX Test date: Aug-2000 Hardware Avail: Sep-2000 Software Avail: Oct-2000

Benchmark

Reference

Time

Base Runtime

Base Ratio Runtime Ratio 100 200 300 400 500

168.wupwise 1600 464 345 449 357

171.swim 3100 693 447 690 449

172.mgrid 1800 716 251 716 251

173.applu 2100 842 250 837 251

177.mesa 1400 358 391 358 391

178.galgel 2900 939 309 877 331

179.art 2600 786 331 799 325

183.equake 1300 526 247 428 304

187.facerec 1900 803 237 733 259

188.ammp 2200 732 301 732 301

189.lucas 2000 645 310 645 310

191.fma3d 2100 769 273 717 293

200.sixtrack 1100 668 165 627 175

301.apsi 2600 770 338 727 357

Hardware

CPU: 1.0 GHz Pentium III processor CPU MHz: 1000 FPU: Integrated CPU(s) enabled: 1 core, 1 chip, 1 core/chip CPU(s) orderable: 1, 2 Parallel: No Primary Cache: 16KBI + 16KBD on chip Secondary Cache: 256KB(I+D) on chip L3 Cache: None Other Cache: None Memory: 256 MB ECC PC800 RDRAM Disk Subsystem: 1 x 9.1GB Quantum Atlas 10K Ultra3 Other Hardware:

Software

Operating System: Windows NT 4.0 (SP5) Compiler: Intel C/C++ and Fortran Compiler 4.5 for Windows NT 4.0

Microsoft Visual Studio 6.0 (for libraries) MicroQuill SmartHeap Library 5.0

File System: NTFS System State: Default

Notes/Tuning Information

 +FDO: PASS1=-Qprof_gen  PASS2=-Qprof_use
 Base tuning: -QaxK -Qipo_wp -O3 +FDO
 Portability:
 178.galgel: -FI -Fe$@ -link -stack:32000000
 Peak tuning:
 168.wupwise: -Qipo_wp -QxK  +FDO
 171.swim: -Qipo_wp -QaxK -O3 +FDO
 172.mgrid: -Qipo_wp -QaxK -O3 +FDO
 173.applu: -Qipo_wp -QxK  +FDO
 177.mesa: -Qipo_wp -QaxK -O3 +FDO
 178.galgel: -Qipo_wp -QxK -O3 +FDO -Zi shlW32M.lib
 179.art: -Qipo_wp -QxK +FDO shlW32M.lib
 183.equake: -QxK -Qrcd -Ow -Qipo_wp +FDO shlW32M.lib
 187.facerec: -Qipo_wp -QxK -O3 +FDO -Zi shlW32M.lib
 188.ammp: -Qipo_wp -QaxK -O3 +FDO
 189.lucas: -Qipo_wp -QxK -O3 +FDO -Zi shlW32M.lib
 191.fma3d: -QxK -O1 +FDO

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

Dell_{Precision WorkStation 420 (1.0 GHz Pentium III)} SPECfp2000 =

SPECfp_base2000 = 304 292 SPEC license #: 55 Tested by: Dell, Round Rock, TX Test date: Aug-2000 Hardware Avail: Sep-2000 Software Avail: Oct-2000

Notes/Tuning Information (Continued)

 200.sixtrack: -Qipo_wp -QxK  +FDO
 301.apsi: -Qipo_wp -QxK  +FDO