Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

Sun Microsystems Sun Blade 1000 Model 1900

SPECfp2000 = SPECfp_base2000 = 482 427 SPEC license #: 6 Tested by: Sun Microsystems, Palo Alto Test date: Sep-2000 Hardware Avail: Dec-2000 Software Avail: Oct-2000

Benchmark

Reference

Time

Base Runtime

Base Ratio Runtime Ratio 500 1000 1500 2000

168.wupwise 1600 322 497 308 520

171.swim 3100 412 752 403 769

172.mgrid 1800 478 377 471 382

173.applu 2100 951 221 422 498

177.mesa 1400 299 469 295 474

178.galgel 2900 229 1266 223 1300

179.art 2600 263 990 210 1239

183.equake 1300 616 211 588 221

187.facerec 1900 265 718 263 723

188.ammp 2200 522 421 484 455

189.lucas 2000 980 204 698 287

191.fma3d 2100 695 302 685 307

200.sixtrack 1100 402 273 402 273

301.apsi 2600 765 340 731 356

Hardware

CPU: UltraSPARC-III CPU MHz: 900 FPU: Integrated CPU(s) enabled: 1 core, 1 chip, 1 core/chip CPU(s) orderable: 1-2 Parallel: No Primary Cache: 32KBI+64KBD on chip Secondary Cache: 8MB(I+D) off chip L3 Cache: None Other Cache: None Memory: 1GB Disk Subsystem: 1 x 18GB Other Hardware: --

Software

Operating System: Solaris 8 update 2 Compiler: Forte Developer 6 update 1 File System: UFS System State: single user

Notes/Tuning Information

 Portability: 178.galgel: -e -fixed

 Base C   flags: -fast -xcrossfile -xprofile -xalias_level=std
 Base F90 flags: -fast -xcrossfile -xprofile

 Peak:
 168.wupwise: -fast -xcrossfile -stackvar -xregs=syst
 171.swim: -fast -xchip=ultra2
 172.mgrid: f77 -fast -xregs=syst
 173.applu: f77 -fast -Qoption iropt -Adata_access,-Mt6000,-Mm12000,-Mr40000,-Ma400,-whole
            -xregs=syst
 177.mesa: -fast -xcrossfile -xalias_level=strong -xprofile
 178.galgel: -fast -xcrossfile -xregs=syst -xprofile -dn
 179.art: -fast -xalias_level=strong -xdepend -xregs=syst -xprofile -dn -lmopt
 183.equake: -fast -xalias_level=strong -xdepend -xprofile -lmopt
 187.facerec: -fast -xcrossfile -stackvar -xprofile

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

Sun Microsystems Sun Blade 1000 Model 1900

SPECfp2000 = SPECfp_base2000 = 482 427 SPEC license #: 6 Tested by: Sun Microsystems, Palo Alto Test date: Sep-2000 Hardware Avail: Dec-2000 Software Avail: Oct-2000

Notes/Tuning Information (Continued)

 188.ammp: -fast -xcrossfile -xalias_level=strong -xdepend -xregs=syst -W2,-whole -xprofile
 189.lucas: -fast -qoption f90comp -array_pad_rows,1024 -Qoption iropt -whole -xprofile
 191.fma3d: -fast -xcrossfile -stackvar -xprofile
 200.sixtrack: -fast -xcrossfile -xprofile
 301.apsi: -fast -qoption f90comp -expansion -xprofile

Note: ONESTEP=yes in base and peak for all benchmarks.
Stack size set to unlimited by: ulimit -s unlimited
 Note: Forte Developer 6 update 1 patches include:
          109503-07,109505-08,109506-06,109513-06
 For results with recommended patch 111228-01 and obp 4.0.40 (or later),
 see publication in July-2001