Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

Hewlett-Packard Company hp visualize b2000 UNIX workstation

SPECfp_rate2000 = SPECfp_rate_base2000 =

4.15 3.72

SPEC license #: 3 Tested by: HP TCL Fort Collins CO Test date: Oct-2000 Hardware Avail: Feb-2000 Software Avail: Sep-2000

Benchmark

Base Copies

Base Runtime

Base Ratio Copies Runtime Ratio 1 2 3 4 5 6 7 8 9 168.wupwise 1 638 2.91 1 471 3.94

171.swim 1 422 8.53 1 414 8.70

172.mgrid 1 508 4.11 1 508 4.11

173.applu 1 439 5.55 1 439 5.55

177.mesa 1 641 2.53 1 570 2.85

178.galgel 1 619 5.43 1 587 5.73

179.art 1 602 5.01 1 426 7.08

183.equake 1 498 3.03 1 334 4.52

187.facerec 1 975 2.26 1 922 2.39

188.ammp 1 707 3.61 1 637 4.01

189.lucas 1 698 3.32 1 698 3.32

191.fma3d 1 930 2.62 1 930 2.62

200.sixtrack 1 524 2.43 1 466 2.74

301.apsi 1 635 4.75 1 635 4.75

Hardware

CPU: 400 MHz PA-8500 CPU MHz: 400 FPU: Integrated CPU(s) enabled: 1 core, 1 chip, 1 core/chip CPU(s) orderable: 1 Parallel: -- Primary Cache: 500KBI+1MBD (on chip) Secondary Cache: none L3 Cache: none Other Cache: None Memory: 2GB Disk Subsystem: 1x9Gbye 10000RPM + 1x9Gbyte LVD 10000RPM Other Hardware: --

Software

Operating System: HP-UX B.11.0 Compiler: HP-UX f90 20000928 (181730) B.11.01.25

HP92453-01 A.11.01.21505.GP HP C Compiler HP-UX f77 971027 (162928) B.11.00.01

File System: HP-UX VxFS System State: Multi-user

Notes/Tuning Information

Portability flags:
cc: -Ae
178.galgel: +source=fixed

Base flags:
f90: +O3 +Onofltacc -Wl,-a,archive -Wl,+FPD
cc: +Oall +Odataprefetch -Wl,-a,archive +I/+P

Peak flags:
Peak flags = base flags for: 172.mgrid, 173.applu, 189.lucas, 191.fma3d and 301.apsi
168.wupwise: f77 +DA2.0 +DS2.0 +O4 +Odataprefetch +Onofltacc -Wl,+FPD -Wl,-a,archive
171.swim: +O3  +Ocachepadcommon +Oloop_unroll -Wl,+FPD -Wl,-a,archive
177.mesa: +I/+P +Oall +Odataprefetch  +Opromote_indirect_calls -Wl,+FPD -Wl,-a,archive
178.galgel: +Oall +fastallocatable-Wl,+FPD -Wl,-a,archive -llapack
178.galgel: RM_SOURCES = lapak.f90
179.art: +Oall +Onodataprefetch +Onofltacc +I/+P +Optrs_strongly_typed -Wl,+FPD -Wl,-a,archive
183.equake: +Oall +Odataprefetch +Optrs_strongly_typed -Wl,+FPD -Wl,-a,archive

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

Hewlett-Packard Company hp visualize b2000 UNIX workstation

SPECfp_rate2000 = SPECfp_rate_base2000 =

4.15 3.72

SPEC license #: 3 Tested by: HP TCL Fort Collins CO Test date: Oct-2000 Hardware Avail: Feb-2000 Software Avail: Sep-2000

Notes/Tuning Information (Continued)

187.facerec: +O2 +Ofastaccess +fastallocatable -Wl,+FPD
       -Wl,-a,archive -Wl,/opt/langtools/lib/fastmem.o
188.ammp: +Oall +Odataprefetch +Optrs_strongly_typed +I/+P  -Wl,+FPD -Wl,-a,archive
200.sixtrack: +Oall +fastallocatable +Onodataprefetch -Wl,+FPD
     -Wl,-a,archive -Wl,/opt/langtools/lib/fastmem.o

Kernel tunables:
vps_pagesize=4096, vps_ceiling=4096, dbc_min_pct=25, dbc_max_pct=25