Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

Sun Microsystems Sun Enterprise 3500/4500

SPECfp2000 = SPECfp_base2000 = 261 246 SPEC license #: 6 Tested by: Sun Microsystems, Palo Alto Test date: Sep-2000 Hardware Avail: Dec-1998 Software Avail: Oct-2000

Benchmark

Reference

Time

Base Runtime

Base Ratio Runtime Ratio 200 400 600 800

168.wupwise 1600 608 263 608 263

171.swim 3100 1073 289 1040 298

172.mgrid 1800 816 221 813 222

173.applu 2100 1527 138 831 253

177.mesa 1400 606 231 590 237

178.galgel 2900 470 617 470 617

179.art 2600 327 795 327 795

183.equake 1300 969 134 926 140

187.facerec 1900 500 380 483 393

188.ammp 2200 949 232 935 235

189.lucas 2000 1020 196 1020 196

191.fma3d 2100 1121 187 1121 187

200.sixtrack 1100 771 143 771 143

301.apsi 2600 1410 184 1341 194

Hardware

CPU: UltraSPARC-II CPU MHz: 400 FPU: Integrated CPU(s) enabled: 1 core, 1 chip, 1 core/chip CPU(s) orderable: 1-8/1-14 Parallel: None Primary Cache: 16KBI+16KBD on chip Secondary Cache: 8MB(I+D) off chip L3 Cache: None Other Cache: None Memory: 8GB Disk Subsystem: 6 x 9GB

Other Hardware: --

Software

Operating System: Solaris 8 Compiler: Forte Developer 6 update 1 File System: UFS System State: multiuser

Notes/Tuning Information

 Portability: 178.galgel: -e -fixed

 Base:
     C: -fast -xcrossfile -xprofile -xalias_level=std
     F90: -fast -xcrossfile -xprofile

 Peak:
     168.wupwise:  basepeak

     171.swim:     -fast -Qoption f90comp -expansion -xsafe=mem -xprefetch -inline=%auto -xvector -xpad=common:15

                   -Qoption iropt -O5+ansi_alias+scalarrep+algassoc+bcopy+bmerge -xprofile
     172.mgrid:    -fast -xregs=syst

     173.applu:    -fast -Qoption iropt -Adata_access,-Mt6000,-Mm12000,-Mr40000,-Ma400,-whole -xregs=syst

     177.mesa:     -fast -xcrossfile -xalias_level=strong -xprofile
     178.galgel:   basepeak
     179.art:      basepeak
     183.equake:   -fast -xalias_level=strong -xdepend -xprofile -lmopt -lm

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

Sun Microsystems Sun Enterprise 3500/4500

SPECfp2000 = SPECfp_base2000 = 261 246 SPEC license #: 6 Tested by: Sun Microsystems, Palo Alto Test date: Sep-2000 Hardware Avail: Dec-1998 Software Avail: Oct-2000

Notes/Tuning Information (Continued)

     187.facerec:  -fast -xcrossfile -stackvar -xprofile
     188.ammp:     -fast -xcrossfile -xalias_level=strong -xdepend -xregs=syst -xprofile
     189.lucas:    basepeak
     191.fma3d:    basepeak
     200.sixtrack: basepeak
     301.apsi:     -fast -qoption f90comp -expansion -xprofile
 ONESTEP=yes for both base and peak