Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

Dell_{Precision WorkStation 330 (1.40 GHz P4)} SPECfp2000 =

SPECfp_base2000 = 532 524 SPEC license #: 55 Tested by: Dell, Round Rock, TX Test date: Nov-2000 Hardware Avail: Nov-2000 Software Avail: Oct-2000

Benchmark

Reference

Time

Base Runtime

Base Ratio Runtime Ratio 500 1000 1500 2000

168.wupwise 1600 219 731 221 725

171.swim 3100 253 1227 253 1227

172.mgrid 1800 343 525 314 573

173.applu 2100 337 623 337 624

177.mesa 1400 274 511 277 505

178.galgel 2900 568 511 568 510

179.art 2600 512 508 499 521

183.equake 1300 183 712 167 778

187.facerec 1900 451 421 444 428

188.ammp 2200 625 352 620 355

189.lucas 2000 273 733 273 733

191.fma3d 2100 523 402 523 402

200.sixtrack 1100 463 238 462 238

301.apsi 2600 640 406 640 406

Hardware

CPU: Pentium 4 CPU MHz: 1400 FPU: Integrated CPU(s) enabled: 1 core, 1 chip, 1 core/chip CPU(s) orderable: 1 Parallel: No Primary Cache: 12K micro-ops I + 8KB D Secondary Cache: 256KB(I+D) on chip L3 Cache: N/A Other Cache: N/A Memory: 2 x 128MB PC800 RDRAM Disk Subsystem: 1 x 40GB Maxtor 7.2K ATA/5 Other Hardware:

Software

Operating System: Windows NT 4.0 (SP5) Compiler: Intel C and Fortran Compiler 5.0 for Windows NT

Microsoft Visual C++ 6.0 (for libraries) MicroQuill SmartHeap Library 5.0

File System: NTFS System State: Default

Notes/Tuning Information

 +FDO: PASS1=  -Qprof_gen  PASS2=-Qprof_use
 Base tuning:  -Qipo -QxW -O3 +FDO
 Portability:
 178.galgel:   -FI /F32000000
 Peak tuning:
 168.wupwise:  -Qipo -QxW  -O3 +FDO
 171.swim:     -Qipo -QxW  -O3 +FDO
 172.mgrid:    -Qipo -QaxW -O3 +FDO
 173.applu:    -Qipo -QxW  -O3 +FDO
 177.mesa:     -Qipo -QxW  -Oa -O3 +FDO shlW32M.lib
 178.galgel:   -Qipo -QxW  -O3 +FDO
 179.art:      -Qipo -QxW  -O3 -Oa +FDO shlW32M.lib
 183.equake:   -Qipo -QxW  -Qrcd -Oa +FDO shlW32M.lib
 187.facerec:  -Qipo -QxW  -O3 +FDO shlW32M.lib
 188.ammp:     -Qipo -QxW  -O3 -Oa +FDO
 189.lucas:    -Qipo -QxW  -O3 +FDO
 191.fma3d:    -Qipo -QxW  -O3 +FDO

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

Dell_{Precision WorkStation 330 (1.40 GHz P4)} SPECfp2000 =

SPECfp_base2000 = 532 524 SPEC license #: 55 Tested by: Dell, Round Rock, TX Test date: Nov-2000 Hardware Avail: Nov-2000 Software Avail: Oct-2000

Notes/Tuning Information (Continued)

 200.sixtrack: -Qipo -QxW  +FDO
 301.apsi:     -Qipo -QxW  -O3 +FDO
 Library ordering for 187.facerec (include SmartHeap correctly with default libs):
 LIBS=libIEPCF90.lib libintrins.lib libF90.lib libqwind.lib libm.lib shlW32M.lib
      LIBC.lib libirc.lib OLDNAMES.lib