Non-Compliant

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

Sun Microsystems Sun Fire 280R

SPECfp_rate2000 = SPECfp_rate_base2000 = NC NC SPEC license #: 6 Tested by: Sun Microsystems, Palo Alto Test date: Dec-2000 Hardware Avail: Jan-2001 Software Avail: Jan-2001

SPEC has determined that this result was not in compliance with the SPEC CPU2000 run and reporting rules. Specifically, the system did not ship to customers in a configuration that achieved the same results (within 1.75%) thus failing to meet the 3-month availability requirement. Replacement results can be found at: http://www.spec.org/osg/cpu2000/results/res2001q3/cpu2000-20010718-00770.html

Benchmark

Base Copies

Base Runtime

Base Ratio Copies Runtime Ratio 1 2 3 4 5 168.wupwise 2 NC NC 2 NC NC 171.swim 2 NC NC 2 NC NC 172.mgrid 2 NC NC 2 NC NC 173.applu 2 NC NC 2 NC NC 177.mesa 2 NC NC 2 NC NC 178.galgel 2 NC NC 2 NC NC 179.art 2 NC NC 2 NC NC 183.equake 2 NC NC 2 NC NC 187.facerec 2 NC NC 2 NC NC 188.ammp 2 NC NC 2 NC NC 189.lucas 2 NC NC 4 NC NC 191.fma3d 2 NC NC 4 NC NC 200.sixtrack 2 NC NC 4 NC NC 301.apsi 2 NC NC 4 NC NC

Hardware

CPU: UltraSPARC-III CPU MHz: 750 FPU: Integrated CPU(s) enabled: 2 cores, 2 chips, 1 core/chip CPU(s) orderable: 2 Parallel: No Primary Cache: 32KBI+64KBD on chip Secondary Cache: 8MB(I+D) off chip L3 Cache: None Other Cache: None Memory: 4GB Disk Subsystem: 1 x 36 GB + 1 x 9 GB

Other Hardware: --

Software

Operating System: Solaris 8 update 3 Compiler: Forte Developer 6 update 1 File System: UFS System State: Single user

Notes/Tuning Information

 Portability: 178.galgel: -e -fixed

 Base C   flags: -fast -xcrossfile -xprofile -xalias_level=std
 Base F90 flags: -fast -xcrossfile -xprofile

Non-Compliant

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

Sun Microsystems Sun Fire 280R

SPECfp_rate2000 = SPECfp_rate_base2000 = NC NC SPEC license #: 6 Tested by: Sun Microsystems, Palo Alto Test date: Dec-2000 Hardware Avail: Jan-2001 Software Avail: Jan-2001

SPEC has determined that this result was not in compliance with the SPEC CPU2000 run and reporting rules. Specifically, the system did not ship to customers in a configuration that achieved the same results (within 1.75%) thus failing to meet the 3-month availability requirement. Replacement results can be found at: http://www.spec.org/osg/cpu2000/results/res2001q3/cpu2000-20010718-00770.html

Notes/Tuning Information (Continued)

 Peak:
 168.wupwise: -fast -xcrossfile -xprofile
 171.swim: -fast -xchip=ultra2
 172.mgrid: f77 -fast -xregs=syst

 173.applu: f77 -fast -Qoption iropt -Adata_access,-Mt6000,-Mm12000,-Mr40000,-Ma400,-whole -xregs=syst

 177.mesa: -fast -xcrossfile -xalias_level=strong -xprofile
 178.galgel: -fast -xcrossfile -xregs=syst -xprofile -dn
 179.art: -fast -xalias_level=strong -xdepend -xregs=syst -xprofile -dn -lmopt -lm
 183.equake: -fast -xalias_level=strong -xdepend -xprofile -lmopt -lm
 187.facerec: -fast -xcrossfile -xprofile
 188.ammp: -fast -xcrossfile -xalias_level=strong -xdepend -xregs=syst -W2,-whole -xprofile
 189.lucas: -fast -qoption f90comp -array_pad_rows,1024 -Qoption iropt -whole -xprofile
 191.fma3d: -fast -xcrossfile -stackvar -xprofile
 200.sixtrack: -fast -xcrossfile -xprofile
 301.apsi: -fast -qoption f90comp -expansion -xprofile
 Note: ONESTEP=yes in base and peak for all benchmarks.
 Stack size set to unlimited by: ulimit -s unlimited
 Note: Forte Developer 6 update 1 patches include:
         109503-07,109505-08,109506-06,109513-06
 For results with patch 111228-01 and obp 4.0.40 or later (included
 in standard configuration) see publication in July-2001