Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

Hewlett-Packard Company hp workstation j6700

SPECfp_rate2000 = SPECfp_rate_base2000 =

10.5 9.76

SPEC license #: 3 Tested by: HP Fort Collins, CO Test date: Mar-2001 Hardware Avail: Jul-2001 Software Avail: Jul-2001

Benchmark

Base Copies

Base Runtime

Base Ratio Copies Runtime Ratio 3 6 9 12 15 18 21 24 27 168.wupwise 2 393 9.46 2 295 12.6

171.swim 2 756 9.52 2 756 9.52

172.mgrid 2 489 8.54 2 482 8.66

173.applu 2 616 7.91 2 616 7.91

177.mesa 2 310 10.5 2 305 10.7

178.galgel 2 251 26.8 2 251 26.8

179.art 2 600 10.1 2 500 12.1

183.equake 2 423 7.13 2 368 8.20

187.facerec 2 554 7.96 2 515 8.55

188.ammp 2 473 10.8 2 422 12.1

189.lucas 2 592 7.84 2 580 8.00

191.fma3d 2 647 7.53 2 629 7.74

200.sixtrack 2 280 9.12 2 244 10.4

301.apsi 2 480 12.6 2 480 12.6

Hardware

CPU: PA-8700 CPU MHz: 750 FPU: Integrated CPU(s) enabled: 2 cores, 2 chips, 1 core/chip CPU(s) orderable: 2 Parallel: -- Primary Cache: 768KBI + 1536KBD (on chip) Secondary Cache: none L3 Cache: none Other Cache: none Memory: 1GB Disk Subsystem: 1 x 18 GB LVD Other Hardware: --

Software

Operating System: HP-UX 11.0 Compiler: HP ANSI C 11.11.02 HP Fortran90 B.11.01.40 File System: HP-UX VxFS System State: Multi-user

Notes/Tuning Information

 Portability Flags:
   178.galgel:  +source=fixed
 Base Flags:
   f90: +O3 +Onofltacc -Wl,-a,archive -Wl,+FPD
   C:   +I/+P +O4 +Odataprefetch -Wl,-a,archive
 Peak flags same as base for 173.applu, 178.galgel, 301.apsi
 Peak Flags:
   All:         -Wl,+FPD -Wl,-a,archive
   168.wupwise: +cat +O3 +Odataprefetch +Onofltacc
   171.swim:    +O3 +Onolimit +Oinline_budget=1000
   172.mgrid:   +O3 +Ocache_pad_common +Oloop_unroll=6
                +Oinline_budget=10
   177.mesa:    +I/+P +Oall +Odataprefetch +Opromote_indirect_calls
   179.art:     +I/+P +Oall +Onodataprefetch +Onofltacc
                +Optrs_strongly_typed +Opromote_indirect_calls
   183.equake:  +O4 +Olibcalls +Odataprefetch +Optrs_strongly_typed
                +Opromote_indirect_calls

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

Hewlett-Packard Company hp workstation j6700

SPECfp_rate2000 = SPECfp_rate_base2000 =

10.5 9.76

SPEC license #: 3 Tested by: HP Fort Collins, CO Test date: Mar-2001 Hardware Avail: Jul-2001 Software Avail: Jul-2001

Notes/Tuning Information (Continued)

   187.facerec: +cat +O3 +Ofastaccess
   188.ammp:    +I/+P +Oall +Odataprefetch +Optrs_strongly_typed
                +Opromote_indirect_calls
   189.lucas:   +O3 +Onoinline
   191.fma3d:   +O3 +Onolimit
   200.sixtrack: +cat +O3 +Onolibcalls +Onolimit +Onoinline
                 +Onodataprefetch
   ONESTEP=true for 168.wupwise, 187.facerec, 200.sixtrack
 System tunables:
 vps_pagesize 4096, vps_ceiling 4096
 dbc_min_pct 15, dbc_max_pct 15