Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

Dell_{Precision WorkStation 530 (1.40 GHz Xeon)} SPECfp_rate2000 =

SPECfp_rate_base2000 =

9.97 9.70

SPEC license #: 55 Tested by: Dell, Round Rock, TX Test date: May-2001 Hardware Avail: May-2001 Software Avail: Oct-2000

Benchmark

Base Copies

Base Runtime

Base Ratio Copies Runtime Ratio 2 4 6 8 10 12 14 16 18 168.wupwise 2 233 16.0 2 233 15.9

171.swim 2 485 14.8 2 485 14.8

172.mgrid 2 427 9.78 2 422 9.90

173.applu 2 439 11.1 2 426 11.4

177.mesa 2 273 11.9 2 268 12.1

178.galgel 2 709 9.48 2 709 9.49

179.art 2 1022 5.90 2 1016 5.94

183.equake 2 230 13.1 2 187 16.1

187.facerec 2 473 9.32 2 461 9.56

188.ammp 2 745 6.86 2 739 6.90

189.lucas 2 342 13.6 2 339 13.7

191.fma3d 2 641 7.60 2 607 8.03

200.sixtrack 2 459 5.56 2 452 5.64

301.apsi 2 759 7.95 2 755 7.99

Hardware

CPU: Intel Xeon CPU MHz: 1400 FPU: Integrated CPU(s) enabled: 2 cores, 2 chips, 1 core/chip CPU(s) orderable: 1, 2 Parallel: No Primary Cache: 12K(I) micro-ops + 8KB(D) on chip Secondary Cache: 256KB(I+D) on chip L3 Cache: N/A Other Cache: N/A Memory: 2 x 256MB PC800 ECC RDRAM Disk Subsystem: 1 x 36GB Quantum Atlas 10K II U160 Other Hardware:

Software

Operating System: Windows 2000 (SP1) Compiler: Intel C++ and Fortan Compiler 5.0 Build 001004

Microsoft Visual C++ 6.0 (for libraries) MicroQuill SmartHeap Library 5.0

File System: NTFS System State: Default

Notes/Tuning Information

 PORTABILITY
   178.galgel:   -FI /F32000000
 FEEDBACK-DIRECTED OPTIMIZATION
   FDO1:         PASS1= /Qprof_gen
   FDO2:         PASS1= /Qprof_gen  PASS2= /Qprof_use
 BASE TUNING
   C/F77/F90:    -Qipo +FDO2 -QxW -O3
 PEAK TUNING
   168.wupwise:  /Qipo +FDO2 /QxW /Qprefetch
   171.swim:     /Qipo +FDO2 /QxW /O3
   172.mgrid:    /Qipo +FDO2 /QaxW /O3
   173.applu:    /Qipo +FDO2 /QxW /O3 /Qscalar_rep- /Qauto
   177.mesa:     -Qwp_ipo +FDO2 -QxW -Qunroll0
   178.galgel:   /Qipo +FDO2 /QxW /O3
   179.art:      -Qipo +FDO2 -QxW -Oa shlW32M.lib
   183.equake:   -Qwp_ipo +FDO2 -QxW -Oa shlW32M.lib
   187.facerec:  /Qipo +FDO2 /QxW /O3 /Qauto shlW32M.lib

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

Dell_{Precision WorkStation 530 (1.40 GHz Xeon)} SPECfp_rate2000 =

SPECfp_rate_base2000 =

9.97 9.70

SPEC license #: 55 Tested by: Dell, Round Rock, TX Test date: May-2001 Hardware Avail: May-2001 Software Avail: Oct-2000

Notes/Tuning Information (Continued)

   188.ammp:     -Qipo +FDO2 -QaxW -Oa
   189.lucas:    /Qipo +FDO1 /QxW /Qunroll0
   191.fma3d:    /Qipo +FDO2 /QxW /O3
   200.sixtrack: /Qipo +FDO2 /QaxW
   301.apsi:     /Qipo +FDO1 /QxW /O3
 EXTRA LIBRARIES
   shlW32M.lib:  MicroQuill SmartHeap Library 5.0
                 www.microquill.com
 LIBRARY ORDERING
   187.facerec:  libIEPCF90.lib libintrins.lib libF90.lib libqwind.lib
                 libm.lib shlW32M.lib LIBC.lib libirc.lib OLDNAMES.lib