Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

Dell_{Precision WorkStation 730 (800 MHz Itanium)} SPECfp2000 =

SPECfp_base2000 = -- 645 SPEC license #: 55 Tested by: Dell, Round Rock, TX Test date: Jun-2001 Hardware Avail: Jun-2001 Software Avail: Jun-2001

Benchmark

Reference

Time

Base Runtime

Base Ratio Runtime Ratio 500 1000 1500 2000

168.wupwise 1600 278 575

171.swim 3100 227 1365

172.mgrid 1800 241 746

173.applu 2100 209 1005

177.mesa 1400 470 298

178.galgel 2900 303 957

179.art 2600 182 1429

183.equake 1300 163 796

187.facerec 1900 372 510

188.ammp 2200 461 477

189.lucas 2000 245 816

191.fma3d 2100 667 315

200.sixtrack 1100 204 540

301.apsi 2600 774 336

Hardware

CPU: Intel Itanium CPU MHz: 800 FPU: Integrated CPU(s) enabled: 1 core, 1 chip, 1 core/chip CPU(s) orderable: 1, 2 Parallel: No Primary Cache: 16KBI + 16KBD on chip Secondary Cache: 96KB(I+D) on chip L3 Cache: 2MB(I+D) off chip Other Cache: N/A Memory: 2GB (16 x 128MB PC100 SDRAM) Disk Subsystem: 1 x 18GB Quantum Atlas 10K Ultra3 Other Hardware:

Software

Operating System: Windows XP Professional 64-bit Beta 2 (2462) Compiler: Intel C++ and Fortran Compiler 5.0.1 (20010529)

Microsoft Platform SDK (2462)

File System: NTFS System State: Default

Notes/Tuning Information

 FEEDBACK-DIRECTED OPTIMIZATION
   +FDO: PASS1=-Qprof_gen  PASS2=-Qprof_use
 BASE TUNING
   C:       -Qipo -O3 +FDO
   F77/F90: -Qipo -O3 -Qftz +FDO
 PORTABILITY
   178.galgel: -FI