Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CINT2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

Sun Microsystems Sun Blade 1000 Model 2900

SPECint_rate2000 = SPECint_rate_base2000 =

10.7 10.0

SPEC license #: 6 Tested by: Sun Microsystems, Palo Alto Test date: Apr-2001 Hardware Avail: Aug-2001 Software Avail: Mar-2001

Benchmark

Base Copies

Base Runtime

Base Ratio Copies Runtime Ratio 2 4 6 8 10 12 14 16 164.gzip 2 411 7.91 2 407 7.98

175.vpr 2 374 8.68 2 348 9.34

176.gcc 2 228 11.2 2 225 11.3

181.mcf 2 410 10.2 2 387 10.8

186.crafty 2 226 10.3 2 208 11.2

197.parser 2 432 9.66 2 399 10.5

252.eon 2 282 10.7 2 265 11.4

253.perlbmk 2 395 10.6 2 378 11.0

254.gap 2 380 6.72 4 746 6.84

255.vortex 2 329 13.4 2 276 15.9

256.bzip2 2 302 11.5 2 278 12.5

300.twolf 2 620 11.2 2 589 11.8

Hardware

CPU: UltraSPARC-III CPU MHz: 900 FPU: Integrated CPU(s) enabled: 2 cores, 2 chips, 1 core/chip CPU(s) orderable: 1-2 Parallel: None Primary Cache: 32KBI+64KBD on chip Secondary Cache: 8MB(I+D) off chip L3 Cache: None Other Cache: None Memory: 1GB Disk Subsystem: 1 x 18GB Other Hardware: --

Software

Operating System: Solaris 8 10/00 Compiler: Forte Developer 6 update 1 w/ latest patches File System: UFS System State: Single User

Notes/Tuning Information

 Portability:
     176.gcc:     -Dalloca=__builtin_alloca -DHOST_WORDS_BIG_ENDIAN
     186.crafty:  -DSUN
     252.eon:     -library=iostream
     253.perlbmk: -DSPEC_CPU2000_SOLARIS
     254.gap:     -DSYS_IS_USG -DSYS_HAS_TIME_PROTO -DSYS_HAS_SIGNAL_PROTO
                  -DSYS_HAS_CALLOC_PROTO -DSYS_HAS_IOCTL_PROTO

 Base C   flags: -fast -xcrossfile -xprofile
 Base C++ flags: -fast -xcrossfile -xprofile

 Peak:
 164.gzip: -fast -xalias_level=std -xcrossfile -W2,-whole -xprofile
 175.vpr: -fast -xalias_level=std -xcrossfile -xdepend -xregs=syst -W2,-whole -xprofile
          -lmopt
 176.gcc: -fast -xcrossfile -W2,-whole -Wc,-Qgsched-trace_late=1,-Qgsched-T4 -xprofile
 181.mcf: -fast -xcrossfile -xdepend -Wc,-Qgsched-trace_late=1,-Qgsched-T4 -xsafe=mem
          -xprofile
 186.crafty: -fast -xcrossfile -Wc,-Qgsched-trace_late=1,-Qgsched-T4
             -xalias_level=strong -xregs=syst -xchip=ultra2 -xprofile

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CINT2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

Sun Microsystems Sun Blade 1000 Model 2900

SPECint_rate2000 = SPECint_rate_base2000 =

10.7 10.0

SPEC license #: 6 Tested by: Sun Microsystems, Palo Alto Test date: Apr-2001 Hardware Avail: Aug-2001 Software Avail: Mar-2001

Notes/Tuning Information (Continued)

 197.parser: -fast -xcrossfile -xdepend -xregs=syst -Wc,-Qgsched-trace_late=1,-Qgsched-T4
             -xalias_level=strong -xprofile
 252.eon: -fast -xcrossfile -xsafe=mem -Qoption iropt -Mt500,-restrict_g,-restrict
          -Qoption cg -Qgsched-trace_late=1,-Qgsched-T4 -xprofile

 253.perlbmk: -fast -Wc,-Qgsched-trace_late=1,-Qgsched-T4,-Qgsched-trace_spec_load=1
              -xcrossfile -xalias_level=std -xsafe=mem -xprofile
 254.gap: -fast -xarch=v8 -W2,-crit,-whole -xcrossfile -Wc,-Qiselect-funcalign=32
          -xalias_level=std -xprofile

 255.vortex: -fast -xsafe=mem -xcrossfile -W2,-Aheap,-reroll=1,-Aunroll,-Ms1,-Mt500,-Mr6000,-crit
             -Wc,-Qdepgraph-early_cross_call=1 -Wc,-Qiselect-funcalign=32 -Wc,-Qpeep-Sh0
             -xrestrict -xdepend -Wc,-Qgsched-trace_late=1,-Qgsched-T4 -xprofile

 256.bzip2: -fast -xarch=v8 -W2,-Abopt -xcrossfile -xalias_level=strong -Wc,-Qiselect-funcalign=32

            -xdepend -xregs=syst -xprofile
 300.twolf: -fast -xalias_level=strong -W2,-whole -xsafe=mem -xprofile

 Note: ONESTEP=yes for all benchmarks.

 Forte Developer 6 update 1 patches include:
    109503-02,109504-01,109505-08,109506-02,109508-04,109510-01,109513-06

 Patch 111228-01 and obp 4.0.40 (or later) is required.

 System configuration details located (as of June 2001) at
         http://www.sun.com/desktop/sunblade1000