Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

Compaq Computer Corporation AlphaServer DS20E Model 6/667

SPECfp2000 = SPECfp_base2000 = 582 535 SPEC license #: 2 Tested by: Compaq NH Test date: Aug-2001 Hardware Avail: Mar-2000 Software Avail: May-2001

Benchmark

Reference

Time

Base Runtime

Base Ratio Runtime Ratio 500 1000 1500 2000

168.wupwise 1600 355 451 299 535

171.swim 3100 313 991 313 992

172.mgrid 1800 508 354 338 533

173.applu 2100 419 502 418 503

177.mesa 1400 263 532 264 530

178.galgel 2900 262 1107 262 1106

179.art 2600 196 1329 159 1631

183.equake 1300 522 249 490 265

187.facerec 1900 253 751 243 782

188.ammp 2200 559 394 477 461

189.lucas 2000 340 588 326 614

191.fma3d 2100 435 483 428 490

200.sixtrack 1100 404 273 375 294

301.apsi 2600 588 442 581 448

Hardware

CPU: Alpha 21264A CPU MHz: 667 FPU: Integrated CPU(s) enabled: 1 core, 1 chip, 1 core/chip CPU(s) orderable: 1 to 2 Parallel: No Primary Cache: 64KB(I)+64KB(D) on chip Secondary Cache: 8MB off chip L3 Cache: None Other Cache: None Memory: 512MB (16x32MB) Disk Subsystem: 1x18GB Other Hardware: None

Software

Operating System: Tru64 UNIX V5.1 UNIX V5.1 Patch Kit 2 Compiler: Compaq C T6.4-208-46B2F Compaq Fortran V5.4A-1472-46B2F Compaq Fortran 77 V5.4-196-46B2F KAP Fortran 77 V4.1 980926 KAP C V4.1 000607 File System: AdvFS System State: Multi-user

Notes/Tuning Information

 Baseline   C: cc  -arch ev6 -fast -O4 ONESTEP
      Fortran: f90 -arch ev6 -fast -O5 ONESTEP

 Peak:    -g3 -arch ev6 -non_shared ONESTEP plus:
    168.wupwise: kf77 -fast -O4 -pipeline -unroll 2
       171.swim: f90 -fast -O5
      172.mgrid: kf77 -O5 -transform_loops -tune ev6 -unroll 8
      173.applu: f90 -fast -O5
       177.mesa: cc -fast -O4
     178.galgel: f90 -fast -O5
        179.art: kcc -fast -O4 -ckapargs=’-arl=4 -ur=4’ -unroll 10
     183.equake:  cc -fast -xtaso_short
    187.facerec: f90 -fast -O4
       188.ammp: cc -fast -O4 -xtaso_short
      189.lucas: kf90 -O5 -fkapargs=’-ur=1’
      191.fma3d: kf90 -O4
   200.sixtrack: f90 -fast -O5 -assume accuracy_sensitive

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CFP2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

Compaq Computer Corporation AlphaServer DS20E Model 6/667

SPECfp2000 = SPECfp_base2000 = 582 535 SPEC license #: 2 Tested by: Compaq NH Test date: Aug-2001 Hardware Avail: Mar-2000 Software Avail: May-2001

Notes/Tuning Information (Continued)

       301.apsi: kf90 -O5 -transform_loops -unroll 8 -fkapargs=’-ur=1’

 Portability: galgel: -fixed

 Information on UNIX V5.1 Patches can be found at
 http://ftp1.service.digital.com/public/unix/v5.1/