Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CINT2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

Hewlett-Packard Company hp server rx4610

SPECint_rate2000 = SPECint_rate_base2000 = -- 4.40

SPEC license #: 3 Tested by: HP Richardson Test date: Aug-2001 Hardware Avail: Jun-2001 Software Avail: Aug-2001

Benchmark

Base Copies

Base Runtime

Base Ratio Copies Runtime Ratio 1 2 3 4 5 6 7 8 164.gzip 1 435 3.74

175.vpr 1 348 4.66

176.gcc 1 257 4.96

181.mcf 1 297 7.02

186.crafty 1 280 4.14

197.parser 1 569 3.67

252.eon 1 351 4.29

253.perlbmk 1 563 3.71

254.gap 1 427 2.99

255.vortex 1 403 5.48

256.bzip2 1 414 4.20

300.twolf 1 667 5.22

Hardware

CPU: Intel Itanium CPU MHz: 800 FPU: Integrated CPU(s) enabled: 1 core, 1 chip, 1 core/chip CPU(s) orderable: 2 to 4 Parallel: No Primary Cache: 16KBI + 16KBD (on die) Secondary Cache: 96KB (on die) L3 Cache: 4MB (off die, on CPU package) Other Cache: None Memory: 8GB (32x256MB DIMMs) Disk Subsystem: 1x36 GB SCSI Other Hardware: None

Software

Operating System: HP-UX 11.20 Compiler: HP C/ANSI B.11.20

HP aC++ Compiler C.05.03 PHSS_24461 - LIBCL general patch PHSS_24463 - Aries cumulative patch PHSS_24464 - Assembler cumulative patch PHSS_24465 - SIN cumulative library Patch PHSS_24466 - SIN product patch PHSS_24467 - u2comp product patch PHSS_24468 - libm cumulative patch PHSS_24469 - aCC library patch PHSS_24470 - aCC product patch PHSS_24471 - C dev cumulative patch PHSS_24472 - C-TOOLS cumulative patch PHSS_24513 - linker cumulative patch PHSS_24648 - unwind cumulative patch

File System: VxFS System State: Multi-user

Notes/Tuning Information

Portability Flags:
175.vpr     : -DSPEC_CPU2000
176.gcc     : -DHOST_WORDS_BIG_ENDIAN
181.mcf     : -DWANT_STDC_PROTO
186.crafty  : -DHP -DSPEC_CPU2000
197.parser  : -DSPEC_CPU2000
252.eon     : -I. -DFMAX_IS_DOUBLE -DNDEBUG srcalt=stdcpp
253.perlbmk : -DSPEC_CPU2000_HP
254.gap     : -DSPEC_CPU2000_HP -DSYS_IS_USG -DSYS_HAS_IOCTL_PROTO
              -DSYS_HAS_TIME_PROTO -DSYS_HAS_CALLOC_PROTO
300.twolf   : -DSPEC_CPU2000

Base Flags:
  C         : +I/+P +Ofaster -exec -Wl,-aarchive_shared
  C++       : +I/+P +Ofaster +inline_level 2

Kernel Tunables:

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org spec CINT2000 Result

Copyright ©1999-2004, Standard Performance Evaluation Corporation

Hewlett-Packard Company hp server rx4610

SPECint_rate2000 = SPECint_rate_base2000 = -- 4.40

SPEC license #: 3 Tested by: HP Richardson Test date: Aug-2001 Hardware Avail: Jun-2001 Software Avail: Aug-2001

Notes/Tuning Information (Continued)

maxdsiz            0x7b03a000
maxdsiz_64bit   0x04000000000
maxssiz            0X10000000
maxssiz_64bit      0x40000000
vps_ceiling             16384
vps_pagesize             4096
swapmem_on                  0
dbc_max_pct                 2
dbc_min_pct                 2

One processor booted (boot vmunix -P1).